{"text_format":"3","workbook":"xlsx","n_sheets":396,"sheets":["Tabelle1","09340048","09340049","09340050","09340051","09340052","09340053","09340054","09340056","09340585","09340611","09340612","09340613","09342379","09342380","09342381","09342382","09342384","09342385","09342386","09342387","09342668","09342668_1","09342669","09342670","09342671","09342829","09342831","09342832","09342833","09342834","09342838","09342839","09342840","09343175","09345300","09345333","09345333_1","09345334","09345335","09345336","09345337","09345338","09345339","09345340","09345341","09345342","09345342_1","09345455","09345487","09345488","09345577","09345819","09345820","09345821","09340048SE03","09340049SE02","09340052SE02","09340053RR02","09340053SE01","09340054SE01","09340054SE02","09340056GA04","09340056GA06","09340056NN01","09340056SE02","09340056SE03","09340056SE05","09340585GA01","09340585GA02","09340585GA04","09340585GA06","09340585GA08","09340585GA09","09340585GA10","09340585NN05","09340585NN11","09340585RR03","09340585RR07","09340611RS03","09340611SE02","09342380GA01","09342380GA03","09342380GA04","09342380GA05","09342380GA06","09342380GA07","09342380GA08","09342380GA09","09342380GA10","09342380GA11","09342380GA12","09342380GA13","09342380GA14","09342380GA15","09342380GA17","09342380GA18","09342380GA20","09342380NN02","09342380NN16","09342380NN19","09342380NN21","09342380NN22","09342381GA01","09342381GA03","09342381GA04","09342381GA05","09342381GA06","09342381GA07","09342381GA08","09342381GA09","09342381GA10","09342381GA11","09342381GA12","09342381GA13","09342381GA14","09342381GA15","09342381GA16","09342381GA17","09342381GA18","09342381GA19","09342381RS20","09342382GA01","09342382GA04","09342382GA05","09342382GA06","09342382GA08","09342382GA09","09342382GA10","09342382GA12","09342382GA13","09342382GA14","09342382GA16","09342382GA17","09342382GA18","09342382GA20","09342382GA21","09342382GA22","09342382GA24","09342382GA25","09342382NN15","09342382NN19","09342382NN23","09342382RV03","09342382RV07","09342382RV11","09342383GA01","09342383GA04","09342383GA05","09342383GA06","09342383GA08","09342383GA09","09342383GA10","09342383GA12","09342383GA13","09342383GA14","09342383GA16","09342383GA17","09342383GA18","09342383GA20","09342383GA21","09342383GA22","09342383GA24","09342383GA25","09342383NN07","09342383NN15","09342383NN19","09342383NN23","09342383RV03","09342383RV11","09342384GA01","09342384GA03","09342384GA05","09342384GA07","09342384GA09","09342384GA10","09342384GA11","09342384GA12","09342384GA13","09342384GA15","09342384GA16","09342384GA17","09342384GA18","09342384GA19","09342384GA20","09342384NN14","09342384RV02","09342384RV04","09342384RV06","09342384RV08","09342385GA02","09342385GA03","09342385GA04","09342385GA06","09342385GA07","09342385GA09","09342385NN05","09342385NN08","09342385NN10","09342385NN11","09342385NN12","09342385RV01","09342386GA01","09342386GA04","09342386RV02","09342386RV03","09342387GA02","09342387GA04","09342387NN06","09342387RS08","09342387RV03","09342387RV05","09342387RV07","09342668GA02","09342668GA03","09342668GA04","09342668GA05","09342668RS07","09342668RV06","09342668SE01","09342668_1SE01","09342669GA02","09342669GA03","09342669GA04","09342669GA05","09342669GA06","09342669RV01","09342670RS03","09342670RV01","09342670SE02","09342671GA01","09342671GA02","09342671GA04","09342671GA05","09342671GA06","09342671GA07","09342671GA08","09342671SE03","09342829GA01","09342829GA03","09342829GA05","09342829GA09","09342829GA10","09342829GA11","09342829NN07","09342829RS02","09342829RS04","09342829RS06","09342829RS08","09342831GA02","09342831GA04","09342831GA06","09342831GA08","09342831GA10","09342831NN03","09342831RR01","09342831RR05","09342831RR07","09342831RR09","09342832GA02","09342832GA04","09342832GA06","09342832GA08","09342832GA10","09342832RR01","09342832RR03","09342832RR05","09342832RR07","09342832RR09","09342833GA02","09342833GA03","09342833GA04","09342833GA05","09342833GA06","09342833GA07","09342833NN01","09342834GA01","09342834RS04","09342834RS07","09342834RS09","09342834RV03","09342834RV05","09342834RV08","09342834SE02","09342838GA01","09342838GA03","09342838GA05","09342838GA07","09342838GA09","09342838GA10","09342838NN11","09342838RS02","09342838RS04","09342838RS06","09342838RS08","09342839GA01","09342839GA03","09342839GA05","09342839GA07","09342839GA11","09342839NN09","09342839RS02","09342839RS04","09342839RS06","09342839RS08","09342839RS10","09342840GA03","09342840GA04","09342840NN05","09342840RS01","09342840RV02","09342841","09343174","09343175GA01","09343175GA03","09343175RR02","09345300GA02","09345300GA03","09345300GA04","09345300NN01","09345300RR05","09345333GA04","09345333NN01","09345333NN02","09345333NN05","09345333SE03","09345333_1GA02","09345333_1GA03","09345333_1GA05","09345333_1GA06","09345333_1NN04","09345333_1RR01","09345334GA02","09345334GA04","09345334NN03","09345334NN06","09345334RV01","09345334RV05","09345335NN01","09345335NN02","09345335NN03","09345335NN04","09345335NN05","09345335NN06","09345335RV07","09345336GA01","09345336GA06","09345336NN04","09345336NN05","09345336RS02","09345336RV03","09345338GA01","09345338RS02","09345338SE03","09345339NN02","09345339SE01","09345339SE03","09345340GA01","09345342_1NN01","09345455NN01","09345455NN02","09345455NN03","09345455NN04","09345455NN05","09345455NN06","09345455NN07","09345487GA02","09345487RS02","09345488NN01","09345488NN03","09345488SE02","09345540","09345577NN01","09345577NN02","09345819NN01","09345819NN03","09345819RR02","09345819RR04","09345819RR05","09345819RR06","09345820NN04","09345820NN05","09345820RR01","09345820RR02","09345820RR03","09345821RR01","09345821RR02","09345821RR03","09345821RR04","09345821RR05","09345821RR06","09346098","09346099","09346100","09346101","09346102"],"not_rendered":{"comments":6},"read":"whole","date_system":"1900"}

{"sheet":"Tabelle1","index":0,"n_rows":62,"n_cols":14,"rows_kept":62,"merged":[[46,0,46,3]]}
[{"$nulls":10},"Info",null,null,"Sanierungsvorschlag"]
["BAB","Rissbildung Riss komplexe Rissbildung",{"$nulls":8},"Vorschlag Sanierung fehlt noch",null,null,"Kurzliner "]
["BAF ","Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar",{"$nulls":8},"Vorschlag Sanierung fehlt noch",null,null,"keine Reparatur wirtschaftlich"]
["BAH","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) "]
[]
[]
[]
[]
[]
["Änderungen:"]
["Haltungsbezeichnung immer von … nach  angeben. Haltungsbezeichung alleine reicht nicht aus."]
[]
["Möglichkeit alle untersuchten Haltungen und Leitungen in eigene Zusammenfassungen zu bringen, damit eine Übersicht entsteht + Massen?"]
[]
["Haltung",null,"Sanierungsvorschlag","Sanierungskosten","Priorität","TV-Neubefahrung","TV-Neubefahrung","Bemerkung"]
["xa39328","xa39329","Schlauch",{"v":15000,"d":"15,000.00 €"},"Kurzfristig","ja","Befahrung mangelhaft"]
["xa39329","xa39330","Reparatur",{"v":1200,"d":"1,200.00 €"},"mittelfristig","nein"]
["xa39330","xa39331","Schlauch",{"v":8000,"d":"8,000.00 €"},"langfristig","nein",null,"Haltung sehr flach, wenn möglich Erneuerung"]
["xa39331","xa39332","Schlauch",{"v":7500,"d":"7,500.00 €"},"Kurzfristig","nein"]
["xa39332","xa39333","Schlauch",{"v":4500,"d":"4,500.00 €"},"mittelfristig","nein"]
["xa39333","xa39334","Schlauch",{"v":21000,"d":"21,000.00 €"},"mittelfristig","nein"]
["xa39334","xa39335","Schlauch",{"v":12000,"d":"12,000.00 €"},"Kurzfristig","nein"]
["xa39335","xa39336","Schlauch",{"v":11000,"d":"11,000.00 €"},"Kurzfristig","nein"]
["xa39336","xa39337","Schlauch",{"v":8500,"d":"8,500.00 €"},"Kurzfristig","ja","Sohle nicht einsehbar"]
["xa39337","xa39338","Schlauch",{"v":9000,"d":"9,000.00 €"},"mittelfristig","ja","Haltung unvollständig befahren"]
["xa39338","xa39339","Erneuerung",{"v":45000,"d":"45,000.00 €"},"Kurzfristig","ja","Sohle nicht einsehbar","Orstsbesichtigung ob Tiefbau möglich"]
["xa39339","xa39340","Reparatur",{"v":2550,"d":"2,550.00 €"},"langfristig","nein"]
["xa39340","xa39341","Reparatur",{"v":2100,"d":"2,100.00 €"},"langfristig","nein"]
["xa39341","xa39342","Reparatur",{"v":900,"d":"900.00 €"},"langfristig","nein"]
["xa39342","xa39343","Schlauch",{"v":1860,"d":"1,860.00 €"},"mittelfristig","nein"]
["xa39343","xa39344","Schlauch",{"v":12000,"d":"12,000.00 €"},"mittelfristig","nein"]
["xa39344","xa39345","Reparatur",{"v":500,"d":"500.00 €"},"Kurzfristig","nein"]
["xa39345","xa39346","Reparatur",{"v":990,"d":"990.00 €"},"Kurzfristig","nein"]
[null,"Summe:",null,{"$f":"SUM(D16:D33)","v":{"v":163600,"d":"163,600.00 €"}}]
[]
["Zusammenfassung:"]
[]
["Schlauchlining",null,{"$f":"SUM(D31,D30,D18:D25,D16)","v":{"v":110360,"d":"110,360.00 €"}}]
[]
["Reparatur",null,{"$f":"SUM(D32:D33,D27:D29,D17)","v":{"v":8240,"d":"8,240.00 €"}}]
[]
["Erneuerng",null,{"$f":"SUM(D26)","v":{"v":45000,"d":"45,000.00 €"}}]
[]
["Gesamt:",null,{"$f":"SUM(C37:C43)","v":{"v":163600,"d":"163,600.00 €"}}]
[]
[]
["Sanierungpriorität:",{"$nulls":3},"Sanierungskosten:"]
[]
["kurzfristig",null,{"v":8,"d":"8.00"},"Haltungen",{"$f":"SUM(D32:D33,D26,D24,D23,D22,D19,D16)","v":{"v":100490,"d":"100,490.00 €"}}]
[]
["mittelfristig",null,{"v":6,"d":"6.00"},"Haltungen",{"$f":"SUM(D30:D31,D25,D20:D21,D17)","v":{"v":49560,"d":"49,560.00 €"}}]
[]
["langfristig",null,{"v":4,"d":"4.00"},"Haltungen",{"$f":"SUM(D18,D27:D29)","v":{"v":13550,"d":"13,550.00 €"}}]
[]
[{"$nulls":3},"Kontrollsumme:",{"$f":"SUM(E49:E53)","v":{"v":163600,"d":"163,600.00 €"}}]
[]
[]
["Abschließende Bewertung:"]
[]
["Upgrade Haltungen empfohlen:"]
[]
["3 Haltungen von mittelfristig in kurzfristig (manuelle Auswertung)"]

{"sheet":"09340048","index":1,"n_rows":50,"n_cols":14,"rows_kept":50,"merged":[[49,0,52,4]]}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340048","BERLINER STRAßE","30,70","31,70","Not Implemented yet",{"$nulls":3},"300","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAB","B / C","2,00","12 - 12",null,"Rissbildung Riss komplexe Rissbildung",null,"Kurzliner",{"v":450,"d":"€450"},null,null,"Kurzliner",{"v":450,"d":"€450"}]
["13,00","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen (nicht fachgerecht)",null,"Stutzensanierung",{"v":600,"d":"€600"},null,null,"Stutzensanierung",{"v":600,"d":"€600"}]
["23,10","BCA","C / A","200,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["23,10","BAH","B",null,"3 - 9","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) ",null,"Stutzensanierung",{"v":600,"d":"€600"},null,null,"Kurzliner",{"v":450,"d":"€450"}]
["23,10","BAP",null,null,"3 - 9","JA","Hohlraum sichtbar  ",{"$nulls":5},"Stutzensanierung",{"v":600,"d":"€600"}]
["27,70","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen (nicht fachgerecht)",null,"Stutzensanierung",{"v":600,"d":"€600"}]
["30,60","BAB","B / D","1,00","12 - 12","JA","Rissbildung Riss gewundene oder spiralförmige Rissbildung",null,"Kurzliner",{"v":450,"d":"€450"}]
["30,70","BCE","XP",{"$nulls":3},"Endknoten  ",{"$nulls":5},"Kurzliner",{"v":450,"d":"€450"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J13)","v":{"v":2700,"d":"€2,700"}},null,null,"Stutzensanierung",{"v":600,"d":"€600"}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H15/100)*J14","v":{"v":270,"d":"€270"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H16/100)*J14","v":{"v":135,"d":"€135"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H17/100)*J14","v":{"v":324,"d":"€324"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",30.7,2,{"$f":"H18*I18","v":{"v":61.4,"d":"€61"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",30.7,3,{"$f":"H19*I19","v":{"v":92.1,"d":"€92"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J14:J19)","v":{"v":3582.5,"d":"€3,583"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H21/100)*J20","v":{"v":680.675,"d":"€681"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J20:J21)","v":{"v":4263.175,"d":"€4,263"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340048","BERLINER STRAßE","30,70","31,70","Not Implemented yet",{"$nulls":3},"300","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAB","B / C","2,00","12 - 12",null,"Rissbildung Riss komplexe Rissbildung"]
["13,00","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen (nicht fachgerecht)",null,"Einmessen,Öffnen,Stsan",{"v":800,"d":"€800"},null,null,"Einmessen,Öffnen,Stsan",{"v":800,"d":"€800"}]
["23,10","BCA","C / A","200,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",{"$nulls":5},"Einmessen,Öffnen,Stsan",{"v":800,"d":"€800"}]
["23,10","BAH","B",null,"3 - 9","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) ",null,"Einmessen,Öffnen,Stsan",{"v":800,"d":"€800"}]
["23,10","BAP",null,null,"3 - 9","JA","Hohlraum sichtbar  "]
["27,70","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen (nicht fachgerecht)",null,"Einmessen,Öffnen,Stsan",{"v":800,"d":"€800"}]
["30,60","BAB","B / D","1,00","12 - 12","JA","Rissbildung Riss gewundene oder spiralförmige Rissbildung"]
["30,70","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3170,"d":"€3,170"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J31:J39)","v":{"v":5570,"d":"€5,570"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":557,"d":"€557"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":278.5,"d":"€279"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":668.4,"d":"€668"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",30.7,2,{"$f":"H44*I44","v":{"v":61.4,"d":"€61"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",30.7,3,{"$f":"H45*I45","v":{"v":92.1,"d":"€92"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":7227.4,"d":"€7,227"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":1373.206,"d":"€1,373"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":8600.606,"d":"€8,601"}}]
[]
["Info: Steinzeughaltung. Diverse Muffenversätze, vor einer Schlauchlinersanierung wegen Haltungsgröße DN300 vorab nicht anzufräsen. Sanierung mittelfristig. Stutzen angeschlagen, Hohlräume teilweise sichtbar. "]

{"sheet":"09340049","index":2,"n_rows":60,"n_cols":12,"rows_kept":60,"merged":[[52,0,55,4]]}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340049","BERLINER STRAßE","18,00","19,00","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAB","B / A","5,00","9",null,"Rissbildung Riss in Längsrichtung",null,"Kurzliner",{"v":450,"d":"€450"}]
["0,20","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen (nicht fachgerecht)",null,"Stutzensanierung",{"v":600,"d":"€600"}]
["3,60","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["3,60","BAH","A",null,"12 - 3",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,"Stutzensanierung",{"v":600,"d":"€600"}]
["16,20","BCA","C / A","200,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["17,80","BAB","B / A","2,00","10",null,"Rissbildung Riss in Längsrichtung",null,"Kurzliner",{"v":450,"d":"€450"}]
["18,00","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":2100,"d":"€2,100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":210,"d":"€210"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":105,"d":"€105"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":252,"d":"€252"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",18,2,{"$f":"H17*I17","v":{"v":36,"d":"€36"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",18,3,{"$f":"H18*I18","v":{"v":54,"d":"€54"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":2757,"d":"€2,757"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":523.83,"d":"€524"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":3280.83,"d":"€3,281"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340049","BERLINER STRAßE","18,00","19,00","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAB","B / A","5,00","9",null,"Rissbildung Riss in Längsrichtung"]
["0,20","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen (nicht fachgerecht)",null,"Einmessen,Öffnen,Stsan",{"v":800,"d":"€800"},null,"wenn Hinweis Sattelschluss, dann Stutzensanierung"]
["3,60","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen (nicht fachgerecht)",null,"Einmessen,Öffnen,Stsan",{"v":800,"d":"€800"}]
["3,60","BAH","A",null,"12 - 3",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["16,20","BCA","C / A","200,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen (nicht fachgerecht)",null,"Einmessen,Öffnen,Stsan",{"v":800,"d":"€800"}]
["17,80","BAB","B / A","2,00","10",null,"Rissbildung Riss in Längsrichtung"]
["18,00","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":2470,"d":"€2,470"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":4870,"d":"€4,870"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":487,"d":"€487"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":243.5,"d":"€244"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":584.4,"d":"€584"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",18,3,{"$f":"H42*I42","v":{"v":54,"d":"€54"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",18,4,{"$f":"H43*I43","v":{"v":72,"d":"€72"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":6310.9,"d":"€6,311"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":1199.071,"d":"€1,199"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":7509.971,"d":"€7,510"}}]
[]
[]
[]
[]
[]
["Haltungsbewertung:"]
["Info: Haltung Beton, deutliche Alterserscheinigungen, beginnende Betonkorrosion. Schlauchliner mittelfristig zu empfehlen. Stutzen nicht fachgerecht und undicht. Sanierungsempfehlung:"]
[]
[]
[]
[]
["Sanierungsempfehlung:"," Renovation Schlauch"]
[]
["TV-Befahrung:","Sohle sichtbar:",5,"% Wasser in der Sohle"]

{"sheet":"09340050","index":3,"n_rows":49,"n_cols":11,"rows_kept":49,"merged":[[40,0,43,4]]}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340051 - 09340050","BERLINER STRAßE","11,90","12,90","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A",null,null,"Streckenschaden! Sanierungsvorschlag automatisch Schlauch="]
["11,90","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["11,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",11.9,2,{"$f":"H13*I13","v":{"v":23.8,"d":"€24"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",11.9,3,{"$f":"H14*I14","v":{"v":35.7,"d":"€36"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":59.5,"d":"€60"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":11.305,"d":"€11"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":70.805,"d":"€71"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340051 - 09340050","BERLINER STRAßE","11,90","12,90","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A",null,null,"Streckenschaden! Sanierungsvorschlag automatisch Schlauch="]
["11,90","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["11,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":1935,"d":"€1,935"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":1935,"d":"€1,935"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":193.5,"d":"€194"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":96.75,"d":"€97"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":232.2,"d":"€232"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",11.9,2,{"$f":"H34*I34","v":{"v":23.8,"d":"€24"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",11.9,3,{"$f":"H35*I35","v":{"v":35.7,"d":"€36"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":2516.95,"d":"€2,517"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":478.22049999999996,"d":"€478"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":2995.1704999999997,"d":"€2,995"}}]
[]
["Haltungsbewertung:"]
["Info: Haltung Beton, deutliche Alterserscheinigungen, beginnende Betonkorrosion. Schlauchliner mittelfristig zu empfehlen. Stutzen nicht fachgerecht und undicht. Sanierung im Reparaturverfahren nicht zu empfehlen"]
[]
[]
[]
[]
["Sanierungsempfehlung:"," Renovation Schlauch"]
[]
["Hinweis:"]
["TV-Befahrung:","Sohle sichtbar:",20,"% Wasser in der Sohle"]

{"sheet":"09340051","index":4,"n_rows":45,"n_cols":10,"rows_kept":45,"merged":[[36,0,39,4]]}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340052 - 09340051","BERLINER STRAßE","9,90","10,90","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["9,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.9,2,{"$f":"H11*I11","v":{"v":19.8,"d":"€20"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.9,3,{"$f":"H12*I12","v":{"v":29.700000000000003,"d":"€30"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":49.5,"d":"€50"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":9.405,"d":"€9"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":58.905,"d":"€59"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340051","BERLINER STRAßE","9,90","10,90","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["9,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":1635,"d":"€1,635"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":1635,"d":"€1,635"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":163.5,"d":"€164"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":81.75,"d":"€82"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":196.2,"d":"€196"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.9,2,{"$f":"H30*I30","v":{"v":19.8,"d":"€20"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.9,3,{"$f":"H31*I31","v":{"v":29.700000000000003,"d":"€30"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":2125.95,"d":"€2,126"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":403.9305,"d":"€404"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":2529.8804999999998,"d":"€2,530"}}]
[]
["Haltungsbewertung:"]
["Info: Haltung Beton, deutliche Alterserscheinigungen, beginnende Betonkorrosion. Schlauchliner mittelfristig zu empfehlen. Stutzen nicht fachgerecht und undicht. Sanieriung im Reparaturverfahren nicht zu empfehlen"]
[]
[]
[]
[]
["Sanierungsempfehlung:"," Renovation Schlauch"]
[]
["Hinweis:"]
["TV-Befahrung:","Sohle sichtbar:",20,"% Wasser in der Sohle"]

{"sheet":"09340052","index":5,"n_rows":74,"n_cols":10,"rows_kept":74,"merged":[[64,0,67,4]]}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340053 - 09340052","BERLINER STRAßE","22,80","23,80","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["6,80","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["8,10","BAH","A",null,"1 - 4",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["8,10","BCA","C / A","200,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["8,10","BAH","C",null,"12 - 12",null,"Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) ",null,"Stutzensanierung",{"v":600,"d":"€600"}]
["8,50","BCA","C / A","150,00","1",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["8,50","BAH","A",null,"12 - 2",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,"Einzelbaugrube",{"v":3000,"d":"€3,000"}]
["9,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["9,10","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["16,20","BAH","B",null,"3 - 9","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) ",null,"Stutzensanierung",{"v":600,"d":"€600"}]
["16,20","BAP",null,null,"7 - 9",null,"Hohlraum sichtbar  "]
["16,20","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["20,60","BDD","C","10,00",null,null,"Wasserspiegel trüb ","A"]
["22,80","BDD","C","10,00",null,null,"Wasserspiegel trüb ","B"]
["22,80","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["22,80","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J20)","v":{"v":4200,"d":"€4,200"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H22/100)*J21","v":{"v":420,"d":"€420"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H23/100)*J21","v":{"v":210,"d":"€210"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H24/100)*J21","v":{"v":504,"d":"€504"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",22.8,2,{"$f":"H25*I25","v":{"v":45.6,"d":"€46"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",22.8,3,{"$f":"H26*I26","v":{"v":68.4,"d":"€68"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J21:J26)","v":{"v":5448,"d":"€5,448"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H28/100)*J27","v":{"v":1035.1200000000001,"d":"€1,035"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J27:J28)","v":{"v":6483.12,"d":"€6,483"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340053 - 09340052","BERLINER STRAßE","22,80","23,80","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["6,80","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["8,10","BAH","A",null,"1 - 4",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["8,10","BCA","C / A","200,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Stsan",{"v":800,"d":"€800"}]
["8,10","BAH","C",null,"12 - 12",null,"Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) "]
["8,50","BCA","C / A","150,00","1",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,",{"v":200,"d":"€200"}]
["8,50","BAH","A",null,"12 - 2",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,"Einzelbaugrube",{"v":3000,"d":"€3,000"}]
["9,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["9,10","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["16,20","BAH","B",null,"3 - 9","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) "]
["16,20","BAP",null,null,"7 - 9",null,"Hohlraum sichtbar  "]
["16,20","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Stsan",{"v":800,"d":"€800"}]
["20,60","BDD","C","10,00",null,null,"Wasserspiegel trüb ","A"]
["22,80","BDD","C","10,00",null,null,"Wasserspiegel trüb ","B"]
["22,80","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["22,80","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3094,"d":"€3,094"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J38:J53)","v":{"v":7894,"d":"€7,894"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H55/100)*J54","v":{"v":789.4000000000001,"d":"€789"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H56/100)*J54","v":{"v":394.70000000000005,"d":"€395"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H57/100)*J54","v":{"v":947.28,"d":"€947"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",22.8,2,{"$f":"H58*I58","v":{"v":45.6,"d":"€46"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",22.8,3,{"$f":"H59*I59","v":{"v":68.4,"d":"€68"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J54:J59)","v":{"v":10139.380000000001,"d":"€10,139"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H61/100)*J60","v":{"v":1926.4822000000001,"d":"€1,926"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J60:J61)","v":{"v":12065.862200000001,"d":"€12,066"}}]
[]
["Haltungsbewertung:"]
["Info: Haltung Beton, deutliche Alterserscheinigungen, fortgeschrittene Betonkorrosion. Schlauchliner kurzfristig zu empfehlen. Stutzen nicht fachgerecht und undicht. Sanierung im Reparaturverfahren nicht zu empfehlen.                    Stutzen bei 8,50 m in geschlossener Bauweise nicht fachgerecht sanierbar, Einzelbaugrube"]
[]
[]
[]
[]
["Sanierungsempfehlung:"," Renovation Schlauch"]
[]
["Hinweis:"]
["TV-Befahrung:","Sohle sichtbar:",20,"% Wasser in der Sohle"]
[null,null,"Sohle nicht einsehbar"]

{"sheet":"09340053","index":6,"n_rows":58,"n_cols":10,"rows_kept":58,"merged":[[48,0,51,4]]}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340054 -  09340053","BERLINER STRAßE","19,40","20,40","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["9,80","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["16,90","BAI","Z","5,00","6 - 10","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":80,"d":"€80"}]
["18,00","BAH","A",null,"10 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,"Einzelbaugrube",{"v":3000,"d":"€3,000"}]
["18,00","BCA","C / A","150,00","11",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["19,00","BBF","B",null,"12 - 12","JA","Infiltration Tropfen "]
["19,00","BBB","A","5,00","12 - 12","JA","Anhaftende Stoffe Inkrustation ",null,"Fräsen",{"v":50,"d":"€50"}]
["19,40","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":3130,"d":"€3,130"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":313,"d":"€313"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":156.5,"d":"€157"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":375.59999999999997,"d":"€376"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",19.4,2,{"$f":"H17*I17","v":{"v":38.8,"d":"€39"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",19.4,3,{"$f":"H18*I18","v":{"v":58.199999999999996,"d":"€58"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":4072.1,"d":"€4,072"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":773.699,"d":"€774"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":4845.799,"d":"€4,846"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340054 -  09340053","BERLINER STRAßE","19,40","20,40","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["9,80","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Stsan",{"v":800,"d":"€800"}]
["16,90","BAI","Z","5,00","6 - 10","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["18,00","BAH","A",null,"10 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,"Einzelbaugrube",{"v":3000,"d":"€3,000"}]
["18,00","BCA","C / A","150,00","11",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen, ",{"v":200,"d":"€200"}]
["19,00","BBF","B",null,"12 - 12","JA","Infiltration Tropfen "]
["19,00","BBB","A","5,00","12 - 12","JA","Anhaftende Stoffe Inkrustation ",null,"Fräsen",{"v":80,"d":"€80"}]
["19,40","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":2652,"d":"€2,652"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":6732,"d":"€6,732"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":673.2,"d":"€673"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":336.6,"d":"€337"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":807.8399999999999,"d":"€808"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",19.4,2,{"$f":"H42*I42","v":{"v":38.8,"d":"€39"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",19.4,3,{"$f":"H43*I43","v":{"v":58.199999999999996,"d":"€58"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":8646.64,"d":"€8,647"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":1642.8616,"d":"€1,643"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":10289.5016,"d":"€10,290"}}]
[]
["Haltungsbewertung:"]
["Info: Haltung Beton, deutliche Alterserscheinigungen, fortgeschrittene Betonkorrosion. Schlauchliner kurzfristig zu empfehlen. Stutzen nicht fachgerecht und undicht. Sanierung im Reparaturverfahren nicht zu empfehlen.                                                                                                                                                                                                  Stutzen bei 18,00 m in geschlossener Bauweise nicht fachgerecht sanierbar, Einzelbaugrube"]
[]
[]
[]
[]
["Sanierungsempfehlung:"," Renovation Schlauch"]
[]
["Hinweis:"]
["TV-Befahrung:","Sohle sichtbar:",20,"% Wasser in der Sohle"]
[null,null,"Sohle nicht einsehbar"]

{"sheet":"09340054","index":7,"n_rows":64,"n_cols":10,"rows_kept":64,"merged":[[52,0,55,4]]}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["9340054 - 09340613","BERLINER STRAßE","38,80","39,80","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BDD","C","20,00",null,null,"Wasserspiegel trüb ","A"]
["1,20","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["4,00","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["7,30","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["27,50","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["27,50","BAH","B",null,"12 - 12","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) ",null,null,{"v":0,"d":"€0"}]
["38,10","BAC","B","50,00","11 - 3","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["38,80","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["38,80","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J14)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H16/100)*J15","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H17/100)*J15","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H18/100)*J15","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",38.8,2,{"$f":"H19*I19","v":{"v":77.6,"d":"€78"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",38.8,3,{"$f":"H20*I20","v":{"v":116.39999999999999,"d":"€116"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J15:J20)","v":{"v":194,"d":"€194"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H22/100)*J21","v":{"v":36.86,"d":"€37"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J21:J22)","v":{"v":230.86,"d":"€231"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["9340054 - 09340613","BERLINER STRAßE","38,80","39,80","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BDD","C","20,00",null,null,"Wasserspiegel trüb ","A"]
["1,20","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["4,00","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["7,30","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Stsan",{"v":800,"d":"€800"}]
["27,50","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einzelbaugrube",{"v":3000,"d":"€3,000"}]
["27,50","BAH","B",null,"12 - 12","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) ",null,"Einmessen,Öffnen, ",{"v":200,"d":"€200"}]
["38,10","BAC","B","50,00","11 - 3","JA","Rohrbruch / Einsturz Fehlen von Teilen ",null,"keine Sanierung erforderl"]
["38,80","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["38,80","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3979.9999999999995,"d":"€3,980"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J32:J41)","v":{"v":7980,"d":"€7,980"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H43/100)*J42","v":{"v":798,"d":"€798"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H44/100)*J42","v":{"v":399,"d":"€399"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H45/100)*J42","v":{"v":957.5999999999999,"d":"€958"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",38.8,2,{"$f":"H46*I46","v":{"v":77.6,"d":"€78"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",38.8,3,{"$f":"H47*I47","v":{"v":116.39999999999999,"d":"€116"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J42:J47)","v":{"v":10328.6,"d":"€10,329"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H49/100)*J48","v":{"v":1962.4340000000002,"d":"€1,962"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J48:J49)","v":{"v":12291.034,"d":"€12,291"}}]
[]
["Haltungsbewertung:"]
["Info: Haltung Beton, deutliche Alterserscheinigungen, fortgeschrittene Betonkorrosion. Schlauchliner kurzfristig zu empfehlen. Stutzen nicht fachgerecht und undicht. Sanierung im Reparaturverfahren nicht zu empfehlen.                                                                                                                                                                                                  Stutzen bei 27,50m in geschlossener Bauweise nicht fachgerecht sanierbar, Einzelbaugrube"]
[]
[]
[]
[]
["Sanierungsempfehlung:"," Renovation Schlauch"]
[]
["Hinweis:"]
["TV-Befahrung:","Sohle sichtbar:",20,"% Wasser in der Sohle"]
[null,null,"Sohle nicht einsehbar"]
[]
["Kanal gereinigt:",null,"nein"]

{"sheet":"09340056","index":8,"n_rows":60,"n_cols":10,"rows_kept":60,"merged":[[44,0,44,1],[49,0,49,4]]}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340056 - 09340054","BERLINER STRAßE","36,40","37,40","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["8,70","BCA","B / A","150,00","2",null,"Anschluss Sattelanschluss – gebohrt offen"]
["13,70","BCA","B / A","150,00","11",null,"Anschluss Sattelanschluss – gebohrt offen"]
["15,80","BCA","B / A","150,00","3",null,"Anschluss Sattelanschluss – gebohrt offen"]
["27,30","BCA","B / A","150,00","1",null,"Anschluss Sattelanschluss – gebohrt offen"]
["31,50","BCA","B / A","150,00","11",null,"Anschluss Sattelanschluss – gebohrt offen"]
["34,90","BCA","B / A","150,00","2",null,"Anschluss Sattelanschluss – gebohrt offen"]
["36,40","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",36.4,2,{"$f":"H17*I17","v":{"v":72.8,"d":"€73"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",36.4,3,{"$f":"H18*I18","v":{"v":109.19999999999999,"d":"€109"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":182,"d":"€182"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":34.58,"d":"€35"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":216.57999999999998,"d":"€217"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340056 - 09340054","BERLINER STRAßE","36,40","37,40","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["8,70","BCA","B / A","150,00","2",null,"Anschluss Sattelanschluss – gebohrt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["13,70","BCA","B / A","150,00","11",null,"Anschluss Sattelanschluss – gebohrt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["15,80","BCA","B / A","150,00","3",null,"Anschluss Sattelanschluss – gebohrt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["27,30","BCA","B / A","150,00","1",null,"Anschluss Sattelanschluss – gebohrt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["31,50","BCA","B / A","150,00","11",null,"Anschluss Sattelanschluss – gebohrt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["34,90","BCA","B / A","150,00","2",null,"Anschluss Sattelanschluss – gebohrt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["36,40","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3740,"d":"€3,740"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":6680,"d":"€6,680"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":668,"d":"€668"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":334,"d":"€334"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":801.6,"d":"€802"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",36.4,2,{"$f":"H42*I42","v":{"v":72.8,"d":"€73"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",36.4,3,{"$f":"H43*I43","v":{"v":109.19999999999999,"d":"€109"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":8665.6,"d":"€8,666"}}]
["langfristig + TV-neu in 10 Jahren:",null,"ja",{"$nulls":3},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":1646.4640000000002,"d":"€1,646"}}]
[{"$nulls":6},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":10312.064,"d":"€10,312"}}]
["Sanierung im Verbund","ja oder nein"]
[]
["Haltungsbewertung:"]
["Info: Haltung neueren Datums, keine sichtbaren Schäden. Anschlussleitungen wurnden in PP erneuert (KG2000). Endschacht ebenfalls erneuert. Startschacht nicht bekannt. Keine Sanierung erforderlich."]
[]
[]
[]
[]
["Sanierungsempfehlung:"," Renovation Schlauch"]
[]
["Hinweis:"]
["TV-Befahrung:","Sohle sichtbar:",10,"% Wasser in der Sohle"]
[]
["Kanal gereinigt:",null,"nein"]

{"sheet":"09340585","index":9,"n_rows":142,"n_cols":14,"rows_kept":142,"merged":[[130,0,133,4]]}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
[" 09340612 - 09340585","BERLINER STRAßE","56,60","57,60","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans.","Material HA","Zustand"]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,50","BAJ","B","25,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"},null,null,"0,50","Besichtigung Schacht erforderlich, ob Haltung abgesackt"]
["1,40","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["2,30","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["2,30","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,20","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,20","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["5,20","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","A"]
["5,40","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["7,00","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["7,40","BAJ","B","25,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["8,30","BBA","B","2,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["11,30","BBA","B","2,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["11,40","BAB","B / A","2,00","1","JA","Rissbildung Riss in Längsrichtung"]
["12,40","BAB","B / A","2,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","A"]
["13,10","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["13,30","BAB","B / A","5,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","B"]
["14,40","BAB","B / A","3,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","A"]
["15,20","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",{"$nulls":3},"Steinzeug","gut"]
["15,90","BAB","B / A","3,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","B"]
["21,30","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",{"$nulls":3},"Steinzeug","gut"]
["26,00","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",{"$nulls":3},"Beton","stark korrdiert"]
["26,60","BCA","C / A","100,00","1",null,"Anschluss Sattelanschluss – gemeißelt offen",{"$nulls":3},"PVC","gut","einragend"]
["26,60","BAG",null,"25,00","12 - 3",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["28,40","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["31,60","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["31,60","BAH","D",null,"12 - 12",null,"Schadhafter Anschluss Anschluss beschädigt ",null,null,{"v":0,"d":"€0"},"Steinezeug","gut","Scherbe am RA"]
["32,70","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["33,50","BAP",null,null,"3 - 9","JA","Hohlraum sichtbar  "]
["33,50","BAJ","B","20,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["34,50","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["36,60","BAC","B","100,00","5 - 7",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["37,80","BBE","D","5,00","4 - 6",null,"Andere Hindernisse Gegenstand ragt durch die Wand ein "]
["37,90","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",{"$nulls":3},"Steinzeug","gut"]
["42,00","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",{"$nulls":3},"Beton","stark korrodiert"]
["42,00","BAH","C",null,"12 - 12","JA","Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) ",null,"Fräsen,Hut",{"v":450,"d":"€450"},"PVC","gut","einragend"]
["43,40","BCA","C / A","100,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["43,40","BBE","D","10,00","2 - 4",null,"Andere Hindernisse Gegenstand ragt durch die Wand ein "]
["48,30","BAG",null,"10,00","1 - 3",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"},"Steinzeug","gut","einragend"]
["48,30","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["49,10","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["51,50","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["52,50","BCA","C / A","150,00","1",null,"Anschluss Sattelanschluss – gemeißelt offen",{"$nulls":3},"Steinzeug","gut","einragend"]
["52,50","BBC","C","5,00","1 - 6",null,"Ablagerungen hartes oder verdichtetes Material ",null,"Fräsen",{"v":50,"d":"€50"}]
["52,50","BAG",null,"5,00","12 - 2",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["55,00","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["55,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["55,00","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","B"]
["56,60","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J53)","v":{"v":1150,"d":"€1,150"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H55/100)*J54","v":{"v":115,"d":"€115"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H56/100)*J54","v":{"v":57.5,"d":"€58"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H57/100)*J54","v":{"v":138,"d":"€138"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",56.6,2,{"$f":"H58*I58","v":{"v":113.2,"d":"€113"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",56.6,3,{"$f":"H59*I59","v":{"v":169.8,"d":"€170"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J54:J59)","v":{"v":1743.5,"d":"€1,744"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H61/100)*J60","v":{"v":331.265,"d":"€331"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J60:J61)","v":{"v":2074.765,"d":"€2,075"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
[" 09340612 - 09340585","BERLINER STRAßE","56,60","57,60","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans.","Material HA","Zustand"]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,50","BAJ","B","25,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"},null,null,"0,50","Besichtigung Schacht erforderlich, ob Haltung abgesackt"]
["1,40","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["2,30","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["2,30","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["5,20","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["5,20","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["5,20","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","A"]
["5,40","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["7,00","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["7,40","BAJ","B","25,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["8,30","BBA","B","2,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["11,30","BBA","B","2,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["11,40","BAB","B / A","2,00","1","JA","Rissbildung Riss in Längsrichtung"]
["12,40","BAB","B / A","2,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","A"]
["13,10","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["13,30","BAB","B / A","5,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","B"]
["14,40","BAB","B / A","3,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","A"]
["15,20","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":600,"d":"€600"},"Steinzeug","gut"]
["15,90","BAB","B / A","3,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","B"]
["21,30","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":600,"d":"€600"},"Steinzeug","gut"]
["26,00","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":600,"d":"€600"},"Beton","stark korrdiert"]
["26,60","BCA","C / A","100,00","1",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":600,"d":"€600"},"PVC","gut","einragend"]
["26,60","BAG",null,"25,00","12 - 3",null,"Einragender Anschluss  "]
["28,40","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["31,60","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":600,"d":"€600"}]
["31,60","BAH","D",null,"12 - 12",null,"Schadhafter Anschluss Anschluss beschädigt ",{"$nulls":3},"Steinezeug","gut","Scherbe am RA"]
["32,70","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["33,50","BAP",null,null,"3 - 9","JA","Hohlraum sichtbar  "]
["33,50","BAJ","B","20,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["34,50","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["36,60","BAC","B","100,00","5 - 7",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["37,80","BBE","D","5,00","4 - 6",null,"Andere Hindernisse Gegenstand ragt durch die Wand ein "]
["37,90","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":600,"d":"€600"},"Steinzeug","gut"]
["42,00","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":600,"d":"€600"},"Beton","stark korrodiert"]
["42,00","BAH","C",null,"12 - 12","JA","Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) ",{"$nulls":3},"PVC","gut","einragend"]
["43,40","BCA","C / A","100,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":600,"d":"€600"}]
["43,40","BBE","D","10,00","2 - 4",null,"Andere Hindernisse Gegenstand ragt durch die Wand ein "]
["48,30","BAG",null,"10,00","1 - 3",null,"Einragender Anschluss  ",{"$nulls":3},"Steinzeug","gut","einragend"]
["48,30","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":600,"d":"€600"}]
["49,10","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["51,50","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["52,50","BCA","C / A","150,00","1",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":600,"d":"€600"},"Steinzeug","gut","einragend"]
["52,50","BBC","C","5,00","1 - 6",null,"Ablagerungen hartes oder verdichtetes Material ",null,"Fräsen",{"v":50,"d":"€50"}]
["52,50","BAG",null,"5,00","12 - 2",null,"Einragender Anschluss  "]
["55,00","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["55,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["55,00","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","B"]
["56,60","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":5760,"d":"€5,760"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J71:J119)","v":{"v":12210,"d":"€12,210"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",5,null,{"$f":"(H121/100)*J120","v":{"v":610.5,"d":"€611"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H122/100)*J120","v":{"v":610.5,"d":"€611"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",10,null,{"$f":"(H123/100)*J120","v":{"v":1221,"d":"€1,221"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",56.6,4,{"$f":"H124*I124","v":{"v":226.4,"d":"€226"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",56.6,4,{"$f":"H125*I125","v":{"v":226.4,"d":"€226"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J120:J125)","v":{"v":15104.8,"d":"€15,105"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H127/100)*J126","v":{"v":2869.912,"d":"€2,870"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J126:J127)","v":{"v":17974.712,"d":"€17,975"}}]
[]
["Haltungsbewertung:"]
["Info: Haltung Beton, deutliche Alterserscheinigungen, sehr starke Betonkorrosion. Schlauchliner kurzfristig zu empfehlen. Stutzen nicht fachgerecht und undicht. Sanierung im Reparaturverfahren nicht zu empfehlen.                                                                                                                                                                                                  Anfang der Haltung unklar, ob Haltung abgesackt. Teilweise Rissbildung im Sohlbereich > Vier-Gelenkriss. Sanierung mit gewebeverstärktem Preliner wegen freiligenden Zuschlagstoffe"]
[]
[]
[]
[]
["Sanierungsempfehlung:"," Renovation Schlauch"]
[]
["Hinweis:"]
["TV-Befahrung:","Sohle sichtbar:",20,"% Wasser in der Sohle"]
[null,null,"Sohle nicht einsehbar"]
[]
["Kanal gereinigt:",null,"nein"]

{"sheet":"09340611","index":10,"n_rows":68,"n_cols":12,"rows_kept":68,"merged":[[56,0,59,4]]}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340612 - 09340611","BERLINER STRAßE","28,10","29,10","Not Implemented yet",{"$nulls":3},"250","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,30","BDD","C","25,00",null,null,"Wasserspiegel trüb ","A"]
["3,70","BAF","C / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["5,80","BAH","C",null,"1 - 12",null,"Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) ",null,"Fräsen,Hut",{"v":450,"d":"€450"}]
["5,80","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["9,60","BAF","C / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["9,60","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["13,00","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["27,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["27,30","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["27,40","BAB","B / A","2,00","9","JA","Rissbildung Riss in Längsrichtung"]
["28,10","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J16)","v":{"v":450,"d":"€450"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H18/100)*J17","v":{"v":45,"d":"€45"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H19/100)*J17","v":{"v":22.5,"d":"€23"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H20/100)*J17","v":{"v":54,"d":"€54"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",28.1,2,{"$f":"H21*I21","v":{"v":56.2,"d":"€56"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",28.1,3,{"$f":"H22*I22","v":{"v":84.30000000000001,"d":"€84"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J17:J22)","v":{"v":712,"d":"€712"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H24/100)*J23","v":{"v":135.28,"d":"€135"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J23:J24)","v":{"v":847.28,"d":"€847"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340612 - 09340611","BERLINER STRAßE","28,10","29,10","Not Implemented yet",{"$nulls":3},"250","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,30","BDD","C","25,00",null,null,"Wasserspiegel trüb ","A"]
["3,70","BAF","C / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["5,80","BAH","C",null,"1 - 12",null,"Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) "]
["5,80","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":600,"d":"€600"},"Beton","kaum korrodiert"]
["9,60","BAF","C / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["9,60","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["13,00","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["27,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["27,30","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Stsan",{"v":800,"d":"€800"},"Steinzeug","gut"]
["27,40","BAB","B / A","2,00","9","JA","Rissbildung Riss in Längsrichtung"]
["28,10","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3783,"d":"€3,783"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J34:J45)","v":{"v":5183,"d":"€5,183"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H47/100)*J46","v":{"v":518.3000000000001,"d":"€518"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H48/100)*J46","v":{"v":259.15000000000003,"d":"€259"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H49/100)*J46","v":{"v":621.9599999999999,"d":"€622"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",28.1,5,{"$f":"H50*I50","v":{"v":140.5,"d":"€141"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",28.1,5,{"$f":"H51*I51","v":{"v":140.5,"d":"€141"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J46:J51)","v":{"v":6863.41,"d":"€6,863"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H53/100)*J52","v":{"v":1304.0479,"d":"€1,304"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J52:J53)","v":{"v":8167.457899999999,"d":"€8,167"}}]
[]
["Haltungsbewertung:"]
["Info: Haltung Beton, deutliche Alterserscheinigungen, sehr starke Betonkorrosion. Schlauchliner kurzfristig zu empfehlen. Stutzen nicht fachgerecht und undicht. Sanierung im Reparaturverfahren nicht zu empfehlen.                                                                                                                                                                                                  "]
[]
[]
[]
[]
["Sanierungsempfehlung:"," Renovation Schlauch"]
[]
["Hinweis:"]
["TV-Befahrung:","Sohle sichtbar:",30,"% Wasser in der Sohle"]
[null,null,"Sohle nicht einsehbar"]
[]
["Kanal gereinigt:",null,"nein"]

{"sheet":"09340612","index":11,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340612","BERLINER STRAßE","5,90","6,90","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BAB","B / A","2,00","11 - 1",null,"Rissbildung Riss in Längsrichtung","A"]
["0,20","BAB","B / B","5,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["0,80","BAB","B / A","2,00","11 - 1",null,"Rissbildung Riss in Längsrichtung","B"]
["5,70","BAB","C / B","10,00","12 - 12",null,"Rissbildung Klaffender Riss am Rohrumfang"]
["5,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.9,2,{"$f":"H15*I15","v":{"v":11.8,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.9,3,{"$f":"H16*I16","v":{"v":17.700000000000003,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":29.500000000000004,"d":"€30"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":5.605,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":35.105000000000004,"d":"€35"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340612","BERLINER STRAßE","5,90","6,90","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BAB","B / A","2,00","11 - 1",null,"Rissbildung Riss in Längsrichtung","A"]
["0,20","BAB","B / B","5,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["0,80","BAB","B / A","2,00","11 - 1",null,"Rissbildung Riss in Längsrichtung","B"]
["5,70","BAB","C / B","10,00","12 - 12",null,"Rissbildung Klaffender Riss am Rohrumfang"]
["5,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":1035,"d":"€1,035"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":1035,"d":"€1,035"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":103.5,"d":"€104"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":51.75,"d":"€52"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":124.19999999999999,"d":"€124"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.9,2,{"$f":"H38*I38","v":{"v":11.8,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.9,3,{"$f":"H39*I39","v":{"v":17.700000000000003,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":1343.95,"d":"€1,344"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":255.3505,"d":"€255"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":1599.3005,"d":"€1,599"}}]

{"sheet":"09340613","index":12,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340613","DÖHRENER WEG","7,00","8,00","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BDD","C","30,00",null,null,"Wasserspiegel trüb ","A"]
["5,40","BDD","C","15,00",null,null,"Wasserspiegel trüb ","C"]
["7,00","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["7,00","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",7,2,{"$f":"H14*I14","v":{"v":14,"d":"€14"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",7,3,{"$f":"H15*I15","v":{"v":21,"d":"€21"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":35,"d":"€35"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":6.65,"d":"€7"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":41.65,"d":"€42"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340613","DÖHRENER WEG","7,00","8,00","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BDD","C","30,00",null,null,"Wasserspiegel trüb ","A"]
["5,40","BDD","C","15,00",null,null,"Wasserspiegel trüb ","C"]
["7,00","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["7,00","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":1200,"d":"€1,200"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":1200,"d":"€1,200"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":120,"d":"€120"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":60,"d":"€60"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":144,"d":"€144"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",7,2,{"$f":"H36*I36","v":{"v":14,"d":"€14"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",7,3,{"$f":"H37*I37","v":{"v":21,"d":"€21"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":1559,"d":"€1,559"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":296.21,"d":"€296"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":1855.21,"d":"€1,855"}}]

{"sheet":"09342379","index":13,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342379","LEIPZIGER STRAßE","5,90","6,90","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["5,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.9,2,{"$f":"H11*I11","v":{"v":11.8,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.9,3,{"$f":"H12*I12","v":{"v":17.700000000000003,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":29.500000000000004,"d":"€30"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":5.605,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":35.105000000000004,"d":"€35"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342379","LEIPZIGER STRAßE","5,90","6,90","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["5,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":1035,"d":"€1,035"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":1035,"d":"€1,035"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":103.5,"d":"€104"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":51.75,"d":"€52"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":124.19999999999999,"d":"€124"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.9,2,{"$f":"H30*I30","v":{"v":11.8,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.9,3,{"$f":"H31*I31","v":{"v":17.700000000000003,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1343.95,"d":"€1,344"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":255.3505,"d":"€255"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1599.3005,"d":"€1,599"}}]

{"sheet":"09342380","index":14,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380","LEIPZIGER STRAßE","29,20","30,20","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,20","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["8,50","BDD","C","10,00",null,null,"Wasserspiegel trüb ","A"]
["14,20","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["17,70","BDD","C","20,00",null,null,"Wasserspiegel trüb ","A"]
["25,40","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["29,20","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["29,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29.2,2,{"$f":"H17*I17","v":{"v":58.4,"d":"€58"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29.2,3,{"$f":"H18*I18","v":{"v":87.6,"d":"€88"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":273,"d":"€273"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":51.87,"d":"€52"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":324.87,"d":"€325"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380","LEIPZIGER STRAßE","29,20","30,20","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,20","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["8,50","BDD","C","10,00",null,null,"Wasserspiegel trüb ","A"]
["14,20","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["17,70","BDD","C","20,00",null,null,"Wasserspiegel trüb ","A"]
["25,40","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["29,20","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["29,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3020,"d":"€3,020"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":3120,"d":"€3,120"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":312,"d":"€312"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":156,"d":"€156"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":374.4,"d":"€374"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29.2,2,{"$f":"H42*I42","v":{"v":58.4,"d":"€58"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29.2,3,{"$f":"H43*I43","v":{"v":87.6,"d":"€88"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":4108.400000000001,"d":"€4,108"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":780.5960000000001,"d":"€781"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":4888.996000000001,"d":"€4,889"}}]

{"sheet":"09342381","index":15,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381","LEIPZIGER STRAßE","29,20","30,20","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["22,10","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["28,20","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["28,60","BBC","C","10,00","10 - 2",null,"Ablagerungen hartes oder verdichtetes Material ",null,"Fräsen",{"v":50,"d":"€50"}]
["29,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29.2,2,{"$f":"H14*I14","v":{"v":58.4,"d":"€58"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29.2,3,{"$f":"H15*I15","v":{"v":87.6,"d":"€88"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":209.5,"d":"€210"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":39.805,"d":"€40"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":249.305,"d":"€249"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381","LEIPZIGER STRAßE","29,20","30,20","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["22,10","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["28,20","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["28,60","BBC","C","10,00","10 - 2",null,"Ablagerungen hartes oder verdichtetes Material ",null,"Fräsen",{"v":50,"d":"€50"}]
["29,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3020,"d":"€3,020"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":3070,"d":"€3,070"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":307,"d":"€307"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":153.5,"d":"€154"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":368.4,"d":"€368"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29.2,2,{"$f":"H36*I36","v":{"v":58.4,"d":"€58"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29.2,3,{"$f":"H37*I37","v":{"v":87.6,"d":"€88"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":4044.9,"d":"€4,045"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":768.5310000000001,"d":"€769"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":4813.4310000000005,"d":"€4,813"}}]

{"sheet":"09342382","index":16,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382","LEIPZIGER STRAßE","29,60","30,60","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["9,30","BAI","A / A",null,"4 - 8","JA","Einragendes Dichtungsmaterial Dichtring sichtbar verschoben, jedoch nicht in die Rohrleitung hineinragend",null,"Fräsen",{"v":50,"d":"€50"}]
["18,50","BAB","B / B","2,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["29,60","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29.6,2,{"$f":"H13*I13","v":{"v":59.2,"d":"€59"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29.6,3,{"$f":"H14*I14","v":{"v":88.80000000000001,"d":"€89"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":211.5,"d":"€212"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":40.185,"d":"€40"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":251.685,"d":"€252"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382","LEIPZIGER STRAßE","29,60","30,60","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["9,30","BAI","A / A",null,"4 - 8","JA","Einragendes Dichtungsmaterial Dichtring sichtbar verschoben, jedoch nicht in die Rohrleitung hineinragend"]
["18,50","BAB","B / B","2,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["29,60","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3060,"d":"€3,060"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":3060,"d":"€3,060"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":306,"d":"€306"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":153,"d":"€153"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":367.2,"d":"€367"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29.6,2,{"$f":"H34*I34","v":{"v":59.2,"d":"€59"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29.6,3,{"$f":"H35*I35","v":{"v":88.80000000000001,"d":"€89"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":4034.2,"d":"€4,034"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":766.4979999999999,"d":"€766"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":4800.697999999999,"d":"€4,801"}}]

{"sheet":"09342384","index":17,"n_rows":74,"n_cols":10,"rows_kept":74}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384","BERLINER STRAßE","30,60","31,60","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,60","BCA","A / A","150,00","11",null,"Anschluss Abzweig offen"]
["0,90","BAJ","B","10,00","7","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,10","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["2,40","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,90","BCA","A / A","150,00","11",null,"Anschluss Abzweig offen"]
["8,40","BCA","A / A","150,00","11",null,"Anschluss Abzweig offen"]
["9,70","BAJ","B","10,00","7","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["11,50","BAJ","B","15,00","5","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["11,50","BCA","A / A","150,00","11",null,"Anschluss Abzweig offen"]
["17,20","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["17,20","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["17,20","BBB","A","3,00","12 - 12",null,"Anhaftende Stoffe Inkrustation ",null,"Fräsen",{"v":50,"d":"€50"}]
["18,70","BAJ","B","10,00","7","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["19,80","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["21,20","BBC","C","2,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["23,20","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["25,80","BCA","A / A","150,00","11",null,"Anschluss Abzweig offen"]
["28,50","BCA","A / A","150,00","11",null,"Anschluss Abzweig offen"]
["28,50","BAI","A / B",null,"11 - 4","JA","Einragendes Dichtungsmaterial Dichtring einragend, aber nicht gebrochen - tiefster Punkt liegt oberhalb der horizontale Mittellinie",null,"Fräsen",{"v":50,"d":"€50"}]
["30,60","BBC","C","2,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["30,60","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J26)","v":{"v":600,"d":"€600"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H28/100)*J27","v":{"v":60,"d":"€60"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H29/100)*J27","v":{"v":30,"d":"€30"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H30/100)*J27","v":{"v":72,"d":"€72"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",30.6,2,{"$f":"H31*I31","v":{"v":61.2,"d":"€61"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",30.6,3,{"$f":"H32*I32","v":{"v":91.80000000000001,"d":"€92"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J27:J32)","v":{"v":915,"d":"€915"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H34/100)*J33","v":{"v":173.85,"d":"€174"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J33:J34)","v":{"v":1088.85,"d":"€1,089"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384","BERLINER STRAßE","30,60","31,60","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,60","BCA","A / A","150,00","11",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["0,90","BAJ","B","10,00","7","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,10","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["2,40","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,90","BCA","A / A","150,00","11",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["8,40","BCA","A / A","150,00","11",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["9,70","BAJ","B","10,00","7","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["11,50","BAJ","B","15,00","5","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["11,50","BCA","A / A","150,00","11",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["17,20","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["17,20","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["17,20","BBB","A","3,00","12 - 12",null,"Anhaftende Stoffe Inkrustation ",null,"Fräsen",{"v":50,"d":"€50"}]
["18,70","BAJ","B","10,00","7","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["19,80","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["21,20","BBC","C","2,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["23,20","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["25,80","BCA","A / A","150,00","11",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["28,50","BCA","A / A","150,00","11",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["28,50","BAI","A / B",null,"11 - 4","JA","Einragendes Dichtungsmaterial Dichtring einragend, aber nicht gebrochen - tiefster Punkt liegt oberhalb der horizontale Mittellinie"]
["30,60","BBC","C","2,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["30,60","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3160,"d":"€3,160"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J44:J65)","v":{"v":7630,"d":"€7,630"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H67/100)*J66","v":{"v":763,"d":"€763"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H68/100)*J66","v":{"v":381.5,"d":"€382"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H69/100)*J66","v":{"v":915.6,"d":"€916"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",30.6,2,{"$f":"H70*I70","v":{"v":61.2,"d":"€61"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",30.6,3,{"$f":"H71*I71","v":{"v":91.80000000000001,"d":"€92"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J66:J71)","v":{"v":9843.1,"d":"€9,843"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H73/100)*J72","v":{"v":1870.189,"d":"€1,870"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J72:J73)","v":{"v":11713.289,"d":"€11,713"}}]

{"sheet":"09342385","index":18,"n_rows":68,"n_cols":10,"rows_kept":68}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385","BERLINER STRAßE","42,30","43,30","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,70","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["3,20","BAJ","B","10,00","5","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["10,80","BAI","A / C",null,"11 - 4","JA","Einragendes Dichtungsmaterial Dichtring einragend, aber nicht gebrochen - tiefster Punkt liegt unterhalb der horizontale Mittellinie",null,"Fräsen",{"v":50,"d":"€50"}]
["13,80","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["18,30","BAJ","B","15,00","5","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["21,20","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["22,80","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["25,60","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["27,00","BAF","A / E",null,"12 - 12","JA","Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","A"]
["28,60","BAI","A / A",null,"12 - 12","JA","Einragendes Dichtungsmaterial Dichtring sichtbar verschoben, jedoch nicht in die Rohrleitung hineinragend",null,"Fräsen",{"v":50,"d":"€50"}]
["36,20","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["36,90","BAF","A / E",null,"12 - 12","JA","Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","C"]
["37,00","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["38,30","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["40,40","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["42,30","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["42,30","BAF","A / E",null,"12 - 12","JA","Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","B"]
["42,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J23)","v":{"v":600,"d":"€600"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H25/100)*J24","v":{"v":60,"d":"€60"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H26/100)*J24","v":{"v":30,"d":"€30"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H27/100)*J24","v":{"v":72,"d":"€72"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",42.3,2,{"$f":"H28*I28","v":{"v":84.6,"d":"€85"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",42.3,3,{"$f":"H29*I29","v":{"v":126.89999999999999,"d":"€127"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J24:J29)","v":{"v":973.5,"d":"€974"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H31/100)*J30","v":{"v":184.965,"d":"€185"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J30:J31)","v":{"v":1158.465,"d":"€1,158"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385","BERLINER STRAßE","42,30","43,30","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,70","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["3,20","BAJ","B","10,00","5","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["10,80","BAI","A / C",null,"11 - 4","JA","Einragendes Dichtungsmaterial Dichtring einragend, aber nicht gebrochen - tiefster Punkt liegt unterhalb der horizontale Mittellinie"]
["13,80","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["18,30","BAJ","B","15,00","5","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["21,20","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["22,80","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["25,60","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["27,00","BAF","A / E",null,"12 - 12","JA","Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","A"]
["28,60","BAI","A / A",null,"12 - 12","JA","Einragendes Dichtungsmaterial Dichtring sichtbar verschoben, jedoch nicht in die Rohrleitung hineinragend"]
["36,20","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["36,90","BAF","A / E",null,"12 - 12","JA","Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","C"]
["37,00","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["38,30","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["40,40","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["42,30","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["42,30","BAF","A / E",null,"12 - 12","JA","Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","B"]
["42,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":4330,"d":"€4,330"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J41:J59)","v":{"v":5320,"d":"€5,320"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H61/100)*J60","v":{"v":532,"d":"€532"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H62/100)*J60","v":{"v":266,"d":"€266"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H63/100)*J60","v":{"v":638.4,"d":"€638"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",42.3,2,{"$f":"H64*I64","v":{"v":84.6,"d":"€85"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",42.3,3,{"$f":"H65*I65","v":{"v":126.89999999999999,"d":"€127"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J60:J65)","v":{"v":6967.9,"d":"€6,968"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H67/100)*J66","v":{"v":1323.9009999999998,"d":"€1,324"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J66:J67)","v":{"v":8291.801,"d":"€8,292"}}]

{"sheet":"09342386","index":19,"n_rows":48,"n_cols":10,"rows_kept":48}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342386","LEIPZIGER STRAßE","20,40","21,40","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BAB","B / B","2,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["5,80","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["7,30","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["11,00","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["14,20","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["19,50","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["20,40","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["20,40","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J13)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H15/100)*J14","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H16/100)*J14","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H17/100)*J14","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",20.4,2,{"$f":"H18*I18","v":{"v":40.8,"d":"€41"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",20.4,3,{"$f":"H19*I19","v":{"v":61.199999999999996,"d":"€61"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J14:J19)","v":{"v":229,"d":"€229"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H21/100)*J20","v":{"v":43.51,"d":"€44"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J20:J21)","v":{"v":272.51,"d":"€273"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342386","LEIPZIGER STRAßE","20,40","21,40","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BAB","B / B","2,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["5,80","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["7,30","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["11,00","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["14,20","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["19,50","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["20,40","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["20,40","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":2782,"d":"€2,782"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J31:J39)","v":{"v":4842,"d":"€4,842"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":484.20000000000005,"d":"€484"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":242.10000000000002,"d":"€242"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":581.04,"d":"€581"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",20.4,2,{"$f":"H44*I44","v":{"v":40.8,"d":"€41"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",20.4,3,{"$f":"H45*I45","v":{"v":61.199999999999996,"d":"€61"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":6251.34,"d":"€6,251"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":1187.7546,"d":"€1,188"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":7439.0946,"d":"€7,439"}}]

{"sheet":"09342387","index":20,"n_rows":48,"n_cols":10,"rows_kept":48}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342387","LEIPZIGER STRAßE","21,90","22,90","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["5,80","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["9,00","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["14,30","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["17,20","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["20,90","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["21,60","BCA","A / A","200,00","6",null,"Anschluss Abzweig offen"]
["21,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J13)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H15/100)*J14","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H16/100)*J14","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H17/100)*J14","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",21.9,2,{"$f":"H18*I18","v":{"v":43.8,"d":"€44"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",21.9,3,{"$f":"H19*I19","v":{"v":65.69999999999999,"d":"€66"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J14:J19)","v":{"v":109.49999999999999,"d":"€110"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H21/100)*J20","v":{"v":20.804999999999996,"d":"€21"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J20:J21)","v":{"v":130.30499999999998,"d":"€130"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342387","LEIPZIGER STRAßE","21,90","22,90","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["5,80","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["9,00","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["14,30","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["17,20","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["20,90","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["21,60","BCA","A / A","200,00","6",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["21,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":2977,"d":"€2,977"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J31:J39)","v":{"v":6407,"d":"€6,407"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":640.7,"d":"€641"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":320.35,"d":"€320"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":768.8399999999999,"d":"€769"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",21.9,2,{"$f":"H44*I44","v":{"v":43.8,"d":"€44"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",21.9,3,{"$f":"H45*I45","v":{"v":65.69999999999999,"d":"€66"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":8246.390000000001,"d":"€8,246"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":1566.8141000000003,"d":"€1,567"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":9813.2041,"d":"€9,813"}}]

{"sheet":"09342668","index":21,"n_rows":66,"n_cols":10,"rows_kept":66}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668","LEIPZIGER STRAßE","29,00","30,00","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,80","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["3,60","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["5,00","BAJ","B","30,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["7,20","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["10,00","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["10,40","BDD","C","20,00",null,null,"Wasserspiegel trüb ","A"]
["12,30","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["12,30","BAH","B",null,"12 - 12",null,"Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) ",null,null,{"v":0,"d":"€0"}]
["12,80","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["12,80","BAP",null,null,"3 - 4",null,"Hohlraum sichtbar  "]
["12,80","BAH","B",null,"12 - 12","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) ",null,null,{"v":0,"d":"€0"}]
["14,50","BDD","C","20,00",null,null,"Wasserspiegel trüb ","B"]
["14,50","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["16,00","BAB","B / A","2,00","2",null,"Rissbildung Riss in Längsrichtung"]
["16,20","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["22,70","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["29,00","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J22)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H24/100)*J23","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H25/100)*J23","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H26/100)*J23","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29,2,{"$f":"H27*I27","v":{"v":58,"d":"€58"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29,3,{"$f":"H28*I28","v":{"v":87,"d":"€87"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J23:J28)","v":{"v":208.5,"d":"€209"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H30/100)*J29","v":{"v":39.615,"d":"€40"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J29:J30)","v":{"v":248.115,"d":"€248"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668","LEIPZIGER STRAßE","29,00","30,00","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,80","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["3,60","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["5,00","BAJ","B","30,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["7,20","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["10,00","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["10,40","BDD","C","20,00",null,null,"Wasserspiegel trüb ","A"]
["12,30","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["12,30","BAH","B",null,"12 - 12",null,"Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) "]
["12,80","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["12,80","BAP",null,null,"3 - 4",null,"Hohlraum sichtbar  "]
["12,80","BAH","B",null,"12 - 12","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) "]
["14,50","BDD","C","20,00",null,null,"Wasserspiegel trüb ","B"]
["14,50","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["16,00","BAB","B / A","2,00","2",null,"Rissbildung Riss in Längsrichtung"]
["16,20","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["22,70","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["29,00","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3000,"d":"€3,000"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J40:J57)","v":{"v":6480,"d":"€6,480"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H59/100)*J58","v":{"v":648,"d":"€648"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H60/100)*J58","v":{"v":324,"d":"€324"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H61/100)*J58","v":{"v":777.6,"d":"€778"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29,2,{"$f":"H62*I62","v":{"v":58,"d":"€58"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29,3,{"$f":"H63*I63","v":{"v":87,"d":"€87"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J58:J63)","v":{"v":8374.6,"d":"€8,375"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H65/100)*J64","v":{"v":1591.174,"d":"€1,591"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J64:J65)","v":{"v":9965.774000000001,"d":"€9,966"}}]

{"sheet":"09342668_1","index":22,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668_1","LEIPZIGER STRAßE","6,80","7,80","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,30","BAB","B / A","2,00","4 - 7",null,"Rissbildung Riss in Längsrichtung","A"]
["2,80","BCA","C / A","150,00","11",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["2,90","BAB","B / A","2,00","4 - 7",null,"Rissbildung Riss in Längsrichtung","B"]
["2,90","BAB","B / A","2,00","11",null,"Rissbildung Riss in Längsrichtung"]
["6,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["6,80","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.8,2,{"$f":"H16*I16","v":{"v":13.6,"d":"€14"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.8,3,{"$f":"H17*I17","v":{"v":20.4,"d":"€20"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":34,"d":"€34"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":6.46,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":40.46,"d":"€40"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668_1","LEIPZIGER STRAßE","6,80","7,80","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,30","BAB","B / A","2,00","4 - 7",null,"Rissbildung Riss in Längsrichtung","A"]
["2,80","BCA","C / A","150,00","11",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["2,90","BAB","B / A","2,00","4 - 7",null,"Rissbildung Riss in Längsrichtung","B"]
["2,90","BAB","B / A","2,00","11",null,"Rissbildung Riss in Längsrichtung"]
["6,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["6,80","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":490,"d":"€490"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":49,"d":"€49"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":24.5,"d":"€25"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":58.8,"d":"€59"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.8,2,{"$f":"H40*I40","v":{"v":13.6,"d":"€14"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.8,3,{"$f":"H41*I41","v":{"v":20.4,"d":"€20"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":656.3,"d":"€656"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":124.69699999999999,"d":"€125"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":780.997,"d":"€781"}}]

{"sheet":"09342669","index":23,"n_rows":62,"n_cols":10,"rows_kept":62}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342669","LEIPZIGER STRAßE","25,00","26,00","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,30","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["4,40","BAB","B / A","2,00","9",null,"Rissbildung Riss in Längsrichtung","A"]
["4,50","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["4,50","BAH","B",null,"12 - 12","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) ",null,null,{"v":0,"d":"€0"}]
["4,80","BAB","B / A","2,00","9",null,"Rissbildung Riss in Längsrichtung","B"]
["5,80","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["8,30","BAH","A",null,"7 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["8,30","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["11,20","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["14,70","BAP",null,null,"2 - 4",null,"Hohlraum sichtbar  "]
["14,70","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["14,70","BAH","B",null,"12 - 12","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) ",null,null,{"v":0,"d":"€0"}]
["20,80","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["23,80","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["25,00","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J20)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H22/100)*J21","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H23/100)*J21","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H24/100)*J21","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",25,2,{"$f":"H25*I25","v":{"v":50,"d":"€50"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",25,3,{"$f":"H26*I26","v":{"v":75,"d":"€75"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J21:J26)","v":{"v":125,"d":"€125"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H28/100)*J27","v":{"v":23.75,"d":"€24"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J27:J28)","v":{"v":148.75,"d":"€149"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342669","LEIPZIGER STRAßE","25,00","26,00","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,30","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["4,40","BAB","B / A","2,00","9",null,"Rissbildung Riss in Längsrichtung","A"]
["4,50","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["4,50","BAH","B",null,"12 - 12","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) "]
["4,80","BAB","B / A","2,00","9",null,"Rissbildung Riss in Längsrichtung","B"]
["5,80","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["8,30","BAH","A",null,"7 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["8,30","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["11,20","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["14,70","BAP",null,null,"2 - 4",null,"Hohlraum sichtbar  "]
["14,70","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["14,70","BAH","B",null,"12 - 12","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) "]
["20,80","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["23,80","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["25,00","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3380,"d":"€3,380"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J38:J53)","v":{"v":6320,"d":"€6,320"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H55/100)*J54","v":{"v":632,"d":"€632"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H56/100)*J54","v":{"v":316,"d":"€316"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H57/100)*J54","v":{"v":758.4,"d":"€758"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",25,2,{"$f":"H58*I58","v":{"v":50,"d":"€50"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",25,3,{"$f":"H59*I59","v":{"v":75,"d":"€75"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J54:J59)","v":{"v":8151.4,"d":"€8,151"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H61/100)*J60","v":{"v":1548.7659999999998,"d":"€1,549"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J60:J61)","v":{"v":9700.166,"d":"€9,700"}}]

{"sheet":"09342670","index":24,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342670","LEIPZIGER STRAßE","3,40","4,40","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,70","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["2,30","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["2,90","BAP",null,null,"3 - 9","JA","Hohlraum sichtbar  "]
["2,90","BAC","B","60,00","12 - 12","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["3,40","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.4,2,{"$f":"H15*I15","v":{"v":6.8,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.4,3,{"$f":"H16*I16","v":{"v":10.2,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":17,"d":"€17"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":3.23,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":20.23,"d":"€20"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342670","LEIPZIGER STRAßE","3,40","4,40","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,70","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["2,30","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["2,90","BAP",null,null,"3 - 9","JA","Hohlraum sichtbar  "]
["2,90","BAC","B","60,00","12 - 12","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["3,40","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":660,"d":"€660"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":1640,"d":"€1,640"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":164,"d":"€164"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":82,"d":"€82"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":196.79999999999998,"d":"€197"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.4,2,{"$f":"H38*I38","v":{"v":6.8,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.4,3,{"$f":"H39*I39","v":{"v":10.2,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":2099.8,"d":"€2,100"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":398.96200000000005,"d":"€399"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":2498.762,"d":"€2,499"}}]

{"sheet":"09342671","index":25,"n_rows":80,"n_cols":10,"rows_kept":80}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671","LEIPZIGER STRAßE","47,80","48,80","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BDD","C","20,00",null,null,"Wasserspiegel trüb ","A"]
["9,40","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["13,20","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["13,20","BAH","B",null,"12 - 12","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) ",null,null,{"v":0,"d":"€0"}]
["14,50","BBF","A",null,"2 - 10","JA","Infiltration Schwitzen "]
["18,60","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["19,90","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["20,90","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["22,50","BDD","C","5,00",null,null,"Wasserspiegel trüb ","A"]
["23,10","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["23,40","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["23,40","BAH","A",null,"12 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["29,50","BCA","A / A","150,00","2",null,"Anschluss Abzweig offen"]
["33,40","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["33,40","BAH","C",null,"11 - 1","JA","Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) ",null,"Fräsen,Hut",{"v":450,"d":"€450"}]
["34,30","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["39,30","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["40,00","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["43,00","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["43,00","BAH","B",null,"12 - 12","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) ",null,null,{"v":0,"d":"€0"}]
["46,20","BDD","C","10,00",null,null,"Wasserspiegel trüb ","A"]
["47,80","BDD","C","5,00",null,null,"Wasserspiegel trüb ","B"]
["47,80","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["47,80","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J29)","v":{"v":450,"d":"€450"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":45,"d":"€45"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":22.5,"d":"€23"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":54,"d":"€54"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",47.8,2,{"$f":"H34*I34","v":{"v":95.6,"d":"€96"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",47.8,3,{"$f":"H35*I35","v":{"v":143.39999999999998,"d":"€143"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":810.5,"d":"€811"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":153.995,"d":"€154"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":964.495,"d":"€964"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671","LEIPZIGER STRAßE","47,80","48,80","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BDD","C","20,00",null,null,"Wasserspiegel trüb ","A"]
["9,40","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["13,20","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["13,20","BAH","B",null,"12 - 12","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) "]
["14,50","BBF","A",null,"2 - 10","JA","Infiltration Schwitzen "]
["18,60","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["19,90","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["20,90","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["22,50","BDD","C","5,00",null,null,"Wasserspiegel trüb ","A"]
["23,10","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["23,40","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["23,40","BAH","A",null,"12 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["29,50","BCA","A / A","150,00","2",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["33,40","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["33,40","BAH","C",null,"11 - 1","JA","Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) "]
["34,30","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["39,30","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["40,00","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["43,00","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["43,00","BAH","B",null,"12 - 12","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) "]
["46,20","BDD","C","10,00",null,null,"Wasserspiegel trüb ","A"]
["47,80","BDD","C","5,00",null,null,"Wasserspiegel trüb ","B"]
["47,80","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["47,80","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":4880,"d":"€4,880"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J47:J71)","v":{"v":8800,"d":"€8,800"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H73/100)*J72","v":{"v":880,"d":"€880"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H74/100)*J72","v":{"v":440,"d":"€440"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H75/100)*J72","v":{"v":1056,"d":"€1,056"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",47.8,2,{"$f":"H76*I76","v":{"v":95.6,"d":"€96"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",47.8,3,{"$f":"H77*I77","v":{"v":143.39999999999998,"d":"€143"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J72:J77)","v":{"v":11415,"d":"€11,415"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H79/100)*J78","v":{"v":2168.85,"d":"€2,169"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J78:J79)","v":{"v":13583.85,"d":"€13,584"}}]

{"sheet":"09342829","index":26,"n_rows":134,"n_cols":10,"rows_kept":134}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829","BERLINER STRAßE","62,00","62,80","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["0,00","BAB","B / C","2,00","12 - 12",null,"Rissbildung Riss komplexe Rissbildung","A"]
["1,20","BAB","B / C","2,00","12 - 12",null,"Rissbildung Riss komplexe Rissbildung","B"]
["2,00","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["5,30","BAN",null,null,"4 - 8",null,"Poröses Rohr  ","A"]
["7,90","BDD","C","3,00",null,null,"Wasserspiegel trüb ","B"]
["10,20","BAN",null,null,"4 - 8",null,"Poröses Rohr  ","C"]
["10,20","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["13,20","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["14,80","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["15,90","BAB","B / A","2,00","3 - 4",null,"Rissbildung Riss in Längsrichtung","A"]
["16,00","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["16,00","BAG",null,"10,00","9 - 12",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["16,00","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["16,10","BAB","B / A","2,00","3 - 4",null,"Rissbildung Riss in Längsrichtung","B"]
["17,20","BDD","C","20,00",null,null,"Wasserspiegel trüb ","C"]
["17,40","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["20,10","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["24,60","BAC","B","300,00","7 - 9",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["24,60","BAP",null,null,"7 - 9",null,"Hohlraum sichtbar  "]
["24,60","BAF","I / E",null,"7 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["24,70","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["26,10","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["26,30","BAG",null,"15,00","8 - 11",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["26,30","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["28,80","BDD","C","20,00",null,null,"Wasserspiegel trüb ","B"]
["33,50","BAG",null,"20,00","9 - 12",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["33,50","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["33,50","BAH","C",null,"12 - 12",null,"Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) ",null,"Fräsen,Hut",{"v":450,"d":"€450"}]
["35,20","BAF","I / E",null,"2 - 4",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["35,30","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["35,30","BCA","C / A","150,00","11",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["39,00","BAB","B / A","3,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","A"]
["40,10","BAB","B / A","3,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","B"]
["42,60","BAG",null,"10,00","9 - 11",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["42,60","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["44,70","BAF","I / E",null,"3 - 5",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["44,70","BAP",null,null,"3 - 5",null,"Hohlraum sichtbar  "]
["44,70","BAG",null,"10,00","9 - 11",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["44,70","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["51,50","BAF","I / E",null,"6 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["51,50","BAP",null,null,"6 - 9",null,"Hohlraum sichtbar  "]
["51,60","BCA","C / A","125,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["52,90","BAB","B / B","3,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["53,40","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["60,70","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["60,80","BAC","B","50,00","8 - 9",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["60,80","BAP",null,null,"8 - 9",null,"Hohlraum sichtbar  "]
["61,40","BAN",null,null,"4 - 8",null,"Poröses Rohr  ","B"]
["61,40","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["62,00","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J56)","v":{"v":700,"d":"€700"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H58/100)*J57","v":{"v":70,"d":"€70"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H59/100)*J57","v":{"v":35,"d":"€35"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H60/100)*J57","v":{"v":84,"d":"€84"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",62,2,{"$f":"H61*I61","v":{"v":124,"d":"€124"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",62,3,{"$f":"H62*I62","v":{"v":186,"d":"€186"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J57:J62)","v":{"v":1199,"d":"€1,199"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H64/100)*J63","v":{"v":227.81,"d":"€228"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J63:J64)","v":{"v":1426.81,"d":"€1,427"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829","BERLINER STRAßE","62,00","62,80","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["0,00","BAB","B / C","2,00","12 - 12",null,"Rissbildung Riss komplexe Rissbildung","A"]
["1,20","BAB","B / C","2,00","12 - 12",null,"Rissbildung Riss komplexe Rissbildung","B"]
["2,00","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["5,30","BAN",null,null,"4 - 8",null,"Poröses Rohr  ","A"]
["7,90","BDD","C","3,00",null,null,"Wasserspiegel trüb ","B"]
["10,20","BAN",null,null,"4 - 8",null,"Poröses Rohr  ","C"]
["10,20","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["13,20","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["14,80","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["15,90","BAB","B / A","2,00","3 - 4",null,"Rissbildung Riss in Längsrichtung","A"]
["16,00","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["16,00","BAG",null,"10,00","9 - 12",null,"Einragender Anschluss  "]
["16,00","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["16,10","BAB","B / A","2,00","3 - 4",null,"Rissbildung Riss in Längsrichtung","B"]
["17,20","BDD","C","20,00",null,null,"Wasserspiegel trüb ","C"]
["17,40","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["20,10","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["24,60","BAC","B","300,00","7 - 9",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["24,60","BAP",null,null,"7 - 9",null,"Hohlraum sichtbar  "]
["24,60","BAF","I / E",null,"7 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["24,70","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["26,10","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["26,30","BAG",null,"15,00","8 - 11",null,"Einragender Anschluss  "]
["26,30","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["28,80","BDD","C","20,00",null,null,"Wasserspiegel trüb ","B"]
["33,50","BAG",null,"20,00","9 - 12",null,"Einragender Anschluss  "]
["33,50","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["33,50","BAH","C",null,"12 - 12",null,"Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) "]
["35,20","BAF","I / E",null,"2 - 4",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["35,30","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["35,30","BCA","C / A","150,00","11",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["39,00","BAB","B / A","3,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","A"]
["40,10","BAB","B / A","3,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","B"]
["42,60","BAG",null,"10,00","9 - 11",null,"Einragender Anschluss  "]
["42,60","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["44,70","BAF","I / E",null,"3 - 5",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["44,70","BAP",null,null,"3 - 5",null,"Hohlraum sichtbar  "]
["44,70","BAG",null,"10,00","9 - 11",null,"Einragender Anschluss  "]
["44,70","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["51,50","BAF","I / E",null,"6 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["51,50","BAP",null,null,"6 - 9",null,"Hohlraum sichtbar  "]
["51,60","BCA","C / A","125,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["52,90","BAB","B / B","3,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["53,40","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["60,70","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["60,80","BAC","B","50,00","8 - 9",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["60,80","BAP",null,null,"8 - 9",null,"Hohlraum sichtbar  "]
["61,40","BAN",null,null,"4 - 8",null,"Poröses Rohr  ","B"]
["61,40","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["62,00","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":6280,"d":"€6,280"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J74:J125)","v":{"v":11670,"d":"€11,670"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H127/100)*J126","v":{"v":1167,"d":"€1,167"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H128/100)*J126","v":{"v":583.5,"d":"€584"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H129/100)*J126","v":{"v":1400.3999999999999,"d":"€1,400"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",62,2,{"$f":"H130*I130","v":{"v":124,"d":"€124"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",62,3,{"$f":"H131*I131","v":{"v":186,"d":"€186"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J126:J131)","v":{"v":15130.9,"d":"€15,131"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H133/100)*J132","v":{"v":2874.871,"d":"€2,875"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J132:J133)","v":{"v":18005.771,"d":"€18,006"}}]

{"sheet":"09342831","index":27,"n_rows":92,"n_cols":10,"rows_kept":92}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831","LEIPZIGER STRAßE","42,30","43,30","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["1,20","BAJ","C","10,00","6","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,20","BAJ","B","20,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,10","BAC","A","200,00","12 - 12",null,"Rohrbruch / Einsturz Bruch "]
["2,10","BAO",null,null,"12 - 12",null,"Boden sichtbar  "]
["4,00","BBA","B","5,00","6 - 8","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,00","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["8,50","BAH","B",null,"2 - 10",null,"Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) ",null,null,{"v":0,"d":"€0"}]
["8,50","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["15,00","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["15,00","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["15,00","BAC","A","300,00","10 - 2","JA","Rohrbruch / Einsturz Bruch "]
["15,10","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["15,60","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["15,60","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["21,70","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["21,70","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["22,40","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["22,40","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["28,60","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["28,60","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["29,10","BAC","B","100,00","7 - 9","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["29,10","BAP",null,null,"7 - 9","JA","Hohlraum sichtbar  "]
["29,20","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["35,50","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["35,50","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["36,00","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["41,60","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["42,30","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["42,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J35)","v":{"v":150,"d":"€150"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",42.3,2,{"$f":"H40*I40","v":{"v":84.6,"d":"€85"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",42.3,3,{"$f":"H41*I41","v":{"v":126.89999999999999,"d":"€127"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":402,"d":"€402"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":76.38,"d":"€76"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":478.38,"d":"€478"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831","LEIPZIGER STRAßE","42,30","43,30","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["1,20","BAJ","C","10,00","6","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,20","BAJ","B","20,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,10","BAC","A","200,00","12 - 12",null,"Rohrbruch / Einsturz Bruch "]
["2,10","BAO",null,null,"12 - 12",null,"Boden sichtbar  "]
["4,00","BBA","B","5,00","6 - 8","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,00","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["8,50","BAH","B",null,"2 - 10",null,"Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) "]
["8,50","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["15,00","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["15,00","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["15,00","BAC","A","300,00","10 - 2","JA","Rohrbruch / Einsturz Bruch "]
["15,10","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["15,60","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["15,60","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["21,70","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["21,70","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["22,40","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["22,40","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["28,60","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["28,60","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["29,10","BAC","B","100,00","7 - 9","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["29,10","BAP",null,null,"7 - 9","JA","Hohlraum sichtbar  "]
["29,20","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["35,50","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["35,50","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["36,00","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["41,60","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["42,30","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["42,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":4330,"d":"€4,330"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J53:J83)","v":{"v":9380,"d":"€9,380"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H85/100)*J84","v":{"v":938,"d":"€938"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H86/100)*J84","v":{"v":469,"d":"€469"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H87/100)*J84","v":{"v":1125.6,"d":"€1,126"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",42.3,2,{"$f":"H88*I88","v":{"v":84.6,"d":"€85"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",42.3,3,{"$f":"H89*I89","v":{"v":126.89999999999999,"d":"€127"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J84:J89)","v":{"v":12124.1,"d":"€12,124"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H91/100)*J90","v":{"v":2303.579,"d":"€2,304"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J90:J91)","v":{"v":14427.679,"d":"€14,428"}}]

{"sheet":"09342832","index":28,"n_rows":86,"n_cols":10,"rows_kept":86}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832","LEIPZIGER STRAßE","42,90","43,60","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","A / E",null,"4 - 8",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","A"]
["1,20","BAC","A","300,00","8 - 4",null,"Rohrbruch / Einsturz Bruch "]
["4,10","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["4,80","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["8,40","BAH","C",null,"3 - 9","JA","Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) ",null,"Fräsen,Hut",{"v":450,"d":"€450"}]
["8,40","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["8,40","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["14,60","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["14,80","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["14,80","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["15,50","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["15,50","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["21,90","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["21,90","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["22,50","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["22,50","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["28,60","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["28,70","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["29,20","BAH","C",null,"2 - 10","JA","Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) ",null,"Fräsen,Hut",{"v":450,"d":"€450"}]
["29,20","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["35,20","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["35,90","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["35,90","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["41,90","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["42,20","BAF","A / E",null,"4 - 8",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","B"]
["42,20","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["42,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J32)","v":{"v":900,"d":"€900"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H34/100)*J33","v":{"v":90,"d":"€90"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H35/100)*J33","v":{"v":45,"d":"€45"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H36/100)*J33","v":{"v":108,"d":"€108"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",42.9,2,{"$f":"H37*I37","v":{"v":85.8,"d":"€86"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",42.9,3,{"$f":"H38*I38","v":{"v":128.7,"d":"€129"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J33:J38)","v":{"v":1357.5,"d":"€1,358"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H40/100)*J39","v":{"v":257.925,"d":"€258"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J39:J40)","v":{"v":1615.425,"d":"€1,615"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832","LEIPZIGER STRAßE","42,90","43,60","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","A / E",null,"4 - 8",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","A"]
["1,20","BAC","A","300,00","8 - 4",null,"Rohrbruch / Einsturz Bruch "]
["4,10","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["4,80","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["8,40","BAH","C",null,"3 - 9","JA","Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) "]
["8,40","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["8,40","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["14,60","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["14,80","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["14,80","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["15,50","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["15,50","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["21,90","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["21,90","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["22,50","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["22,50","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["28,60","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["28,70","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["29,20","BAH","C",null,"2 - 10","JA","Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) "]
["29,20","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["35,20","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["35,90","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["35,90","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["41,90","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["42,20","BAF","A / E",null,"4 - 8",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","B"]
["42,20","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["42,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":4360,"d":"€4,360"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J50:J77)","v":{"v":9260,"d":"€9,260"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H79/100)*J78","v":{"v":926,"d":"€926"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H80/100)*J78","v":{"v":463,"d":"€463"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H81/100)*J78","v":{"v":1111.2,"d":"€1,111"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",42.9,2,{"$f":"H82*I82","v":{"v":85.8,"d":"€86"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",42.9,3,{"$f":"H83*I83","v":{"v":128.7,"d":"€129"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J78:J83)","v":{"v":11974.7,"d":"€11,975"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H85/100)*J84","v":{"v":2275.193,"d":"€2,275"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J84:J85)","v":{"v":14249.893,"d":"€14,250"}}]

{"sheet":"09342833","index":29,"n_rows":80,"n_cols":10,"rows_kept":80}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342833","LEIPZIGER STRAßE","41,20","42,20","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,80","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["3,70","BAB","B / A","2,00","4 - 8","JA","Rissbildung Riss in Längsrichtung"]
["3,70","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,30","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["5,70","BAB","B / A","2,00","9","JA","Rissbildung Riss in Längsrichtung"]
["7,80","BAC","B","60,00","3 - 9","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["7,80","BAP",null,null,"4 - 6","JA","Hohlraum sichtbar  "]
["8,50","BAH","B",null,"2 - 10","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) ",null,null,{"v":0,"d":"€0"}]
["8,50","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["8,80","BAC","A","200,00","8 - 10",null,"Rohrbruch / Einsturz Bruch "]
["10,80","BAB","B / A","2,00","3","JA","Rissbildung Riss in Längsrichtung"]
["12,20","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["12,50","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["13,40","BAB","B / B","2,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["15,30","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["15,50","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["22,40","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["22,40","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["29,10","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["29,30","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["36,00","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["40,10","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["40,30","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["41,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J29)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",41.2,2,{"$f":"H34*I34","v":{"v":82.4,"d":"€82"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",41.2,3,{"$f":"H35*I35","v":{"v":123.60000000000001,"d":"€124"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":269.5,"d":"€270"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":51.205,"d":"€51"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":320.705,"d":"€321"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342833","LEIPZIGER STRAßE","41,20","42,20","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,80","BAF","E / E",null,"2 - 10",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["3,70","BAB","B / A","2,00","4 - 8","JA","Rissbildung Riss in Längsrichtung"]
["3,70","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,30","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["5,70","BAB","B / A","2,00","9","JA","Rissbildung Riss in Längsrichtung"]
["7,80","BAC","B","60,00","3 - 9","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["7,80","BAP",null,null,"4 - 6","JA","Hohlraum sichtbar  "]
["8,50","BAH","B",null,"2 - 10","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) "]
["8,50","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["8,80","BAC","A","200,00","8 - 10",null,"Rohrbruch / Einsturz Bruch "]
["10,80","BAB","B / A","2,00","3","JA","Rissbildung Riss in Längsrichtung"]
["12,20","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["12,50","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["13,40","BAB","B / B","2,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["15,30","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["15,50","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["22,40","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["22,40","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["29,10","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["29,30","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["36,00","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["40,10","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["40,30","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["41,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":4220,"d":"€4,220"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J47:J71)","v":{"v":7210,"d":"€7,210"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H73/100)*J72","v":{"v":721,"d":"€721"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H74/100)*J72","v":{"v":360.5,"d":"€361"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H75/100)*J72","v":{"v":865.1999999999999,"d":"€865"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",41.2,2,{"$f":"H76*I76","v":{"v":82.4,"d":"€82"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",41.2,3,{"$f":"H77*I77","v":{"v":123.60000000000001,"d":"€124"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J72:J77)","v":{"v":9362.7,"d":"€9,363"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H79/100)*J78","v":{"v":1778.9130000000002,"d":"€1,779"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J78:J79)","v":{"v":11141.613000000001,"d":"€11,142"}}]

{"sheet":"09342834","index":30,"n_rows":80,"n_cols":10,"rows_kept":80}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834","LEIPZIGER STRAßE","29,30","30,30","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["0,80","BAP",null,null,"1 - 5",null,"Hohlraum sichtbar  "]
["0,80","BBA","B","2,00","1 - 5",null,"Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,80","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["0,80","BAH","C",null,"12 - 12","JA","Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) ",null,"Fräsen,Hut",{"v":450,"d":"€450"}]
["2,50","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["3,90","BAB","B / A","1,00","3",null,"Rissbildung Riss in Längsrichtung"]
["4,10","BBA","B","1,00","2 - 4",null,"Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,10","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["4,10","BAH","B",null,"12 - 12",null,"Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) ",null,null,{"v":0,"d":"€0"}]
["7,80","BAI","Z","3,00","1 - 4","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["9,60","BAP",null,null,"1 - 5",null,"Hohlraum sichtbar  "]
["9,60","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["9,60","BAH","B",null,"12 - 12","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) ",null,null,{"v":0,"d":"€0"}]
["10,90","BDD","C","10,00",null,null,"Wasserspiegel trüb ","C"]
["13,10","BBA","B","2,00","2 - 4",null,"Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["13,10","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["13,80","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["14,60","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["19,40","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["22,60","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["28,90","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["28,90","BAH","B",null,"12 - 12","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) ",null,null,{"v":0,"d":"€0"}]
["29,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J29)","v":{"v":650,"d":"€650"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":65,"d":"€65"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":32.5,"d":"€33"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":78,"d":"€78"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29.3,2,{"$f":"H34*I34","v":{"v":58.6,"d":"€59"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29.3,3,{"$f":"H35*I35","v":{"v":87.9,"d":"€88"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":972,"d":"€972"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":184.68,"d":"€185"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":1156.68,"d":"€1,157"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834","LEIPZIGER STRAßE","29,30","30,30","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["0,80","BAP",null,null,"1 - 5",null,"Hohlraum sichtbar  "]
["0,80","BBA","B","2,00","1 - 5",null,"Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,80","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["0,80","BAH","C",null,"12 - 12","JA","Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) "]
["2,50","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["3,90","BAB","B / A","1,00","3",null,"Rissbildung Riss in Längsrichtung"]
["4,10","BBA","B","1,00","2 - 4",null,"Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,10","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["4,10","BAH","B",null,"12 - 12",null,"Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) "]
["7,80","BAI","Z","3,00","1 - 4","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["9,60","BAP",null,null,"1 - 5",null,"Hohlraum sichtbar  "]
["9,60","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["9,60","BAH","B",null,"12 - 12","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) "]
["10,90","BDD","C","10,00",null,null,"Wasserspiegel trüb ","C"]
["13,10","BBA","B","2,00","2 - 4",null,"Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["13,10","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["13,80","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["14,60","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["19,40","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["22,60","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["28,90","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["28,90","BAH","B",null,"12 - 12","JA","Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) "]
["29,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3030,"d":"€3,030"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J47:J71)","v":{"v":7590,"d":"€7,590"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H73/100)*J72","v":{"v":759,"d":"€759"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H74/100)*J72","v":{"v":379.5,"d":"€380"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H75/100)*J72","v":{"v":910.8,"d":"€911"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29.3,2,{"$f":"H76*I76","v":{"v":58.6,"d":"€59"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29.3,3,{"$f":"H77*I77","v":{"v":87.9,"d":"€88"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J72:J77)","v":{"v":9785.8,"d":"€9,786"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H79/100)*J78","v":{"v":1859.302,"d":"€1,859"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J78:J79)","v":{"v":11645.101999999999,"d":"€11,645"}}]

{"sheet":"09342838","index":31,"n_rows":168,"n_cols":10,"rows_kept":168}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838","BERLINER STRAßE","62,40","63,40","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["2,20","BAI","Z","5,00","2 - 10","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,20","BAI","Z","3,00","1 - 5","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,20","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["3,20","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["5,20","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,20","BBE","D","10,00","11 - 6","JA","Andere Hindernisse Gegenstand ragt durch die Wand ein "]
["7,20","BDD","C","20,00",null,null,"Wasserspiegel trüb ","A"]
["7,20","BAI","Z","5,00","2 - 6","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["11,20","BAI","Z","5,00","2 - 8","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["11,40","BAN",null,null,"4 - 8",null,"Poröses Rohr  ","A"]
["11,40","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["14,30","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["15,40","BDD","C","25,00",null,null,"Wasserspiegel trüb ","C"]
["16,00","BAF","I / E",null,"6 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["16,00","BAP",null,null,"6 - 9",null,"Hohlraum sichtbar  "]
["16,00","BAG",null,"5,00","9 - 12",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["16,00","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["16,00","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["16,50","BDD","C","40,00",null,null,"Wasserspiegel trüb ","C"]
["17,30","BBA","B","2,00","8 - 10","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["17,30","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["18,30","BAI","Z","3,00","10 - 4","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["19,20","BAI","Z","3,00","4 - 9","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["20,70","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["23,90","BDD","C","20,00",null,null,"Wasserspiegel trüb ","A"]
["24,50","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["24,50","BAH","C",null,"12 - 4","JA","Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) ",null,"Fräsen,Hut",{"v":450,"d":"€450"}]
["26,20","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["30,80","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["33,30","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["33,60","BAN",null,null,"4 - 8",null,"Poröses Rohr  ","C"]
["33,70","BAG",null,"10,00","9 - 12",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["33,70","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["33,70","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["34,80","BAB","B / A","3,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","A"]
["35,30","BAH","A",null,"10 - 2",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["35,30","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["38,90","BAB","B / A","3,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","B"]
["42,40","BAN",null,null,"4 - 8",null,"Poröses Rohr  ","C"]
["42,40","BAP",null,null,"6 - 10",null,"Hohlraum sichtbar  "]
["42,40","BAF","I / E",null,"6 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["42,50","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["44,20","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["45,70","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["46,40","BAJ","B","20,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["51,40","BAI","Z","3,00","8 - 10","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["51,70","BAP",null,null,"3 - 9","JA","Hohlraum sichtbar  "]
["51,70","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["51,70","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["51,70","BAH","C",null,"12 - 12","JA","Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) ",null,"Fräsen,Hut",{"v":450,"d":"€450"}]
["52,40","BAP",null,null,"4 - 8","JA","Hohlraum sichtbar  "]
["52,40","BAI","Z","3,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["53,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["53,00","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["53,10","BAF","I / E",null,"2 - 4",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["53,20","BAG",null,"10,00","9 - 12",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["53,20","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["53,20","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["57,30","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["59,40","BBE","C","20,00","4 - 8","JA","Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["60,70","BAF","I / E",null,"8 - 10",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["60,70","BAP",null,null,"8 - 9",null,"Hohlraum sichtbar  "]
["60,70","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["61,20","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["61,20","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","B"]
["62,10","BAB","B / B","3,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["62,40","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J73)","v":{"v":1600,"d":"€1,600"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H75/100)*J74","v":{"v":160,"d":"€160"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H76/100)*J74","v":{"v":80,"d":"€80"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H77/100)*J74","v":{"v":192,"d":"€192"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",62.4,2,{"$f":"H78*I78","v":{"v":124.8,"d":"€125"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",62.4,3,{"$f":"H79*I79","v":{"v":187.2,"d":"€187"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J74:J79)","v":{"v":2344,"d":"€2,344"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H81/100)*J80","v":{"v":445.36,"d":"€445"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J80:J81)","v":{"v":2789.36,"d":"€2,789"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838","BERLINER STRAßE","62,40","63,40","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["2,20","BAI","Z","5,00","2 - 10","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["3,20","BAI","Z","3,00","1 - 5","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["3,20","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["3,20","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["5,20","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,20","BBE","D","10,00","11 - 6","JA","Andere Hindernisse Gegenstand ragt durch die Wand ein "]
["7,20","BDD","C","20,00",null,null,"Wasserspiegel trüb ","A"]
["7,20","BAI","Z","5,00","2 - 6","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["11,20","BAI","Z","5,00","2 - 8","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["11,40","BAN",null,null,"4 - 8",null,"Poröses Rohr  ","A"]
["11,40","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["14,30","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["15,40","BDD","C","25,00",null,null,"Wasserspiegel trüb ","C"]
["16,00","BAF","I / E",null,"6 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["16,00","BAP",null,null,"6 - 9",null,"Hohlraum sichtbar  "]
["16,00","BAG",null,"5,00","9 - 12",null,"Einragender Anschluss  "]
["16,00","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["16,00","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["16,50","BDD","C","40,00",null,null,"Wasserspiegel trüb ","C"]
["17,30","BBA","B","2,00","8 - 10","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["17,30","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["18,30","BAI","Z","3,00","10 - 4","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["19,20","BAI","Z","3,00","4 - 9","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["20,70","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["23,90","BDD","C","20,00",null,null,"Wasserspiegel trüb ","A"]
["24,50","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["24,50","BAH","C",null,"12 - 4","JA","Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) "]
["26,20","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["30,80","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["33,30","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["33,60","BAN",null,null,"4 - 8",null,"Poröses Rohr  ","C"]
["33,70","BAG",null,"10,00","9 - 12",null,"Einragender Anschluss  "]
["33,70","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["33,70","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["34,80","BAB","B / A","3,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","A"]
["35,30","BAH","A",null,"10 - 2",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["35,30","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["38,90","BAB","B / A","3,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","B"]
["42,40","BAN",null,null,"4 - 8",null,"Poröses Rohr  ","C"]
["42,40","BAP",null,null,"6 - 10",null,"Hohlraum sichtbar  "]
["42,40","BAF","I / E",null,"6 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["42,50","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["44,20","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["45,70","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["46,40","BAJ","B","20,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["51,40","BAI","Z","3,00","8 - 10","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["51,70","BAP",null,null,"3 - 9","JA","Hohlraum sichtbar  "]
["51,70","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["51,70","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["51,70","BAH","C",null,"12 - 12","JA","Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) "]
["52,40","BAP",null,null,"4 - 8","JA","Hohlraum sichtbar  "]
["52,40","BAI","Z","3,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["53,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["53,00","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["53,10","BAF","I / E",null,"2 - 4",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["53,20","BAG",null,"10,00","9 - 12",null,"Einragender Anschluss  "]
["53,20","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["53,20","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["57,30","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["59,40","BBE","C","20,00","4 - 8","JA","Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["60,70","BAF","I / E",null,"8 - 10",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["60,70","BAP",null,null,"8 - 9",null,"Hohlraum sichtbar  "]
["60,70","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["61,20","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["61,20","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","B"]
["62,10","BAB","B / B","3,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["62,40","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":6340,"d":"€6,340"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J91:J159)","v":{"v":11880,"d":"€11,880"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H161/100)*J160","v":{"v":1188,"d":"€1,188"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H162/100)*J160","v":{"v":594,"d":"€594"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H163/100)*J160","v":{"v":1425.6,"d":"€1,426"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",62.4,2,{"$f":"H164*I164","v":{"v":124.8,"d":"€125"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",62.4,3,{"$f":"H165*I165","v":{"v":187.2,"d":"€187"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J160:J165)","v":{"v":15399.6,"d":"€15,400"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H167/100)*J166","v":{"v":2925.924,"d":"€2,926"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J166:J167)","v":{"v":18325.524,"d":"€18,326"}}]

{"sheet":"09342839","index":32,"n_rows":228,"n_cols":10,"rows_kept":228}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839","BERLINER STRAßE","62,50","63,50","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","AED","PP",{"$nulls":3},"Grundlagen änderung  "]
["1,20","BAA","A","3,00","10 - 1",null,"Verformung vertikal "]
["1,20","BCB","Z",null,"12 - 12",null,"Punktuelle Reparatur anderes grabenloses Reparaturverfahren ","A"]
["1,50","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["1,50","BCB","Z",null,"12 - 12",null,"Punktuelle Reparatur anderes grabenloses Reparaturverfahren ","B"]
["3,30","BBF","A",null,"12 - 12","JA","Infiltration Schwitzen "]
["5,40","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","A"]
["5,50","BAC","B","300,00","1 - 6",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["5,50","BAP",null,null,"1 - 5",null,"Hohlraum sichtbar  "]
["5,50","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["5,60","BAB","B / A","2,00","6",null,"Rissbildung Riss in Längsrichtung","A"]
["6,30","BAI","Z","5,00","2 - 10","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,30","BAB","B / A","2,00","6",null,"Rissbildung Riss in Längsrichtung","B"]
["7,30","BBF","A",null,"12 - 12","JA","Infiltration Schwitzen "]
["9,60","BBD","A","2,00","3 - 6",null,"Eindringen von Bodenmaterial Sand "]
["9,60","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["9,80","BAF","E / E",null,"8 - 4",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["9,80","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["9,80","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["10,50","BAC","B","300,00","12 - 6",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["10,50","BBD","B","25,00","12 - 6",null,"Eindringen von Bodenmaterial Torf "]
["10,50","BAP",null,null,"12 - 6",null,"Hohlraum sichtbar  "]
["10,90","BAP",null,null,"9 - 12",null,"Hohlraum sichtbar  "]
["10,90","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["10,90","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","A"]
["14,30","BAI","Z","5,00","2 - 10","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["16,20","BAG",null,"20,00","9 - 11",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["16,20","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["16,20","BAH","C",null,"12 - 12","JA","Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) ",null,"Fräsen,Hut",{"v":450,"d":"€450"}]
["16,60","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["17,50","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["20,60","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","C"]
["21,60","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","C"]
["21,60","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","A"]
["24,80","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["26,70","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["29,50","BAC","B","500,00","11 - 6",null,"Rohrbruch / Einsturz Fehlen von Teilen ","A"]
["29,80","BAC","B","500,00","11 - 6",null,"Rohrbruch / Einsturz Fehlen von Teilen ","B"]
["31,50","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["33,50","BAB","B / A","2,00","11","JA","Rissbildung Riss in Längsrichtung"]
["33,60","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["33,60","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["34,50","BAB","B / A","2,00","2","JA","Rissbildung Riss in Längsrichtung"]
["34,50","BAI","Z","3,00","2 - 4","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["35,20","BAB","B / A","3,00","4 - 5",null,"Rissbildung Riss in Längsrichtung","A"]
["35,40","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["35,90","BAB","B / A","3,00","4 - 5",null,"Rissbildung Riss in Längsrichtung","B"]
["35,90","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["35,90","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","C"]
["35,90","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","C"]
["35,90","BBD","A","15,00","12 - 7",null,"Eindringen von Bodenmaterial Sand "]
["37,50","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["39,40","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["39,40","BAF","E / E",null,"8 - 4",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["39,40","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","B"]
["39,40","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","B"]
["39,40","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","B"]
["40,50","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["41,10","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["41,10","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","A"]
["42,80","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["42,80","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["43,50","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","A"]
["43,50","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","A"]
["44,60","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["45,10","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["45,10","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","C"]
["46,00","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","C"]
["49,60","BAI","Z","3,00","12 - 4","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["51,80","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["51,80","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["52,50","AED","PP",{"$nulls":3},"Grundlagen änderung  "]
["52,50","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["52,50","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","B"]
["52,50","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","B"]
["52,50","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","B"]
["52,70","BCA","A / A","150,00","11",null,"Anschluss Abzweig offen"]
["54,50","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["55,60","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","A"]
["55,70","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","A"]
["56,80","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","C"]
["56,80","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","A"]
["57,10","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","C"]
["57,10","BAC","B","100,00","12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["58,00","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["58,00","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","C"]
["60,60","BAI","Z","10,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["60,90","BBA","B","3,00","8 - 9",null,"Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["60,90","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["61,50","BBA","B","2,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["61,50","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["61,90","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["61,90","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","C"]
["61,90","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","C"]
["62,50","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","B"]
["62,50","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","B"]
["62,50","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","B"]
["62,50","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J103)","v":{"v":1000,"d":"€1,000"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H105/100)*J104","v":{"v":100,"d":"€100"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H106/100)*J104","v":{"v":50,"d":"€50"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H107/100)*J104","v":{"v":120,"d":"€120"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",62.5,2,{"$f":"H108*I108","v":{"v":125,"d":"€125"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",62.5,3,{"$f":"H109*I109","v":{"v":187.5,"d":"€188"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J104:J109)","v":{"v":1582.5,"d":"€1,583"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H111/100)*J110","v":{"v":300.675,"d":"€301"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J110:J111)","v":{"v":1883.175,"d":"€1,883"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839","BERLINER STRAßE","62,50","63,50","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","AED","PP",{"$nulls":3},"Grundlagen änderung  "]
["1,20","BAA","A","3,00","10 - 1",null,"Verformung vertikal "]
["1,20","BCB","Z",null,"12 - 12",null,"Punktuelle Reparatur anderes grabenloses Reparaturverfahren ","A"]
["1,50","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["1,50","BCB","Z",null,"12 - 12",null,"Punktuelle Reparatur anderes grabenloses Reparaturverfahren ","B"]
["3,30","BBF","A",null,"12 - 12","JA","Infiltration Schwitzen "]
["5,40","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","A"]
["5,50","BAC","B","300,00","1 - 6",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["5,50","BAP",null,null,"1 - 5",null,"Hohlraum sichtbar  "]
["5,50","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["5,60","BAB","B / A","2,00","6",null,"Rissbildung Riss in Längsrichtung","A"]
["6,30","BAI","Z","5,00","2 - 10","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["6,30","BAB","B / A","2,00","6",null,"Rissbildung Riss in Längsrichtung","B"]
["7,30","BBF","A",null,"12 - 12","JA","Infiltration Schwitzen "]
["9,60","BBD","A","2,00","3 - 6",null,"Eindringen von Bodenmaterial Sand "]
["9,60","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["9,80","BAF","E / E",null,"8 - 4",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["9,80","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["9,80","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["10,50","BAC","B","300,00","12 - 6",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["10,50","BBD","B","25,00","12 - 6",null,"Eindringen von Bodenmaterial Torf "]
["10,50","BAP",null,null,"12 - 6",null,"Hohlraum sichtbar  "]
["10,90","BAP",null,null,"9 - 12",null,"Hohlraum sichtbar  "]
["10,90","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["10,90","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","A"]
["14,30","BAI","Z","5,00","2 - 10","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["16,20","BAG",null,"20,00","9 - 11",null,"Einragender Anschluss  "]
["16,20","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["16,20","BAH","C",null,"12 - 12","JA","Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) "]
["16,60","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["17,50","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["20,60","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","C"]
["21,60","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","C"]
["21,60","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","A"]
["24,80","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["26,70","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["29,50","BAC","B","500,00","11 - 6",null,"Rohrbruch / Einsturz Fehlen von Teilen ","A"]
["29,80","BAC","B","500,00","11 - 6",null,"Rohrbruch / Einsturz Fehlen von Teilen ","B"]
["31,50","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["33,50","BAB","B / A","2,00","11","JA","Rissbildung Riss in Längsrichtung"]
["33,60","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["33,60","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["34,50","BAB","B / A","2,00","2","JA","Rissbildung Riss in Längsrichtung"]
["34,50","BAI","Z","3,00","2 - 4","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["35,20","BAB","B / A","3,00","4 - 5",null,"Rissbildung Riss in Längsrichtung","A"]
["35,40","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["35,90","BAB","B / A","3,00","4 - 5",null,"Rissbildung Riss in Längsrichtung","B"]
["35,90","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["35,90","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","C"]
["35,90","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","C"]
["35,90","BBD","A","15,00","12 - 7",null,"Eindringen von Bodenmaterial Sand "]
["37,50","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["39,40","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["39,40","BAF","E / E",null,"8 - 4",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["39,40","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","B"]
["39,40","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","B"]
["39,40","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","B"]
["40,50","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["41,10","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["41,10","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","A"]
["42,80","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["42,80","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["43,50","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","A"]
["43,50","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","A"]
["44,60","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["45,10","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["45,10","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","C"]
["46,00","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","C"]
["49,60","BAI","Z","3,00","12 - 4","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["51,80","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["51,80","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["52,50","AED","PP",{"$nulls":3},"Grundlagen änderung  "]
["52,50","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["52,50","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","B"]
["52,50","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","B"]
["52,50","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","B"]
["52,70","BCA","A / A","150,00","11",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["54,50","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["55,60","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","A"]
["55,70","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","A"]
["56,80","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","C"]
["56,80","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","A"]
["57,10","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","C"]
["57,10","BAC","B","100,00","12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["58,00","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["58,00","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","C"]
["60,60","BAI","Z","10,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["60,90","BBA","B","3,00","8 - 9",null,"Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["60,90","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["61,50","BBA","B","2,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["61,50","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["61,90","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","C"]
["61,90","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","C"]
["61,90","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","C"]
["62,50","BAN",null,null,"12 - 12",null,"Poröses Rohr  ","B"]
["62,50","BAC","B",null,"12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen ","B"]
["62,50","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  ","B"]
["62,50","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":6350,"d":"€6,350"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J121:J219)","v":{"v":11890,"d":"€11,890"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H221/100)*J220","v":{"v":1189,"d":"€1,189"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H222/100)*J220","v":{"v":594.5,"d":"€595"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H223/100)*J220","v":{"v":1426.8,"d":"€1,427"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",62.5,2,{"$f":"H224*I224","v":{"v":125,"d":"€125"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",62.5,3,{"$f":"H225*I225","v":{"v":187.5,"d":"€188"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J220:J225)","v":{"v":15412.8,"d":"€15,413"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H227/100)*J226","v":{"v":2928.432,"d":"€2,928"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J226:J227)","v":{"v":18341.232,"d":"€18,341"}}]

{"sheet":"09342840","index":33,"n_rows":86,"n_cols":10,"rows_kept":86}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342840","BERLINER STRAßE","62,70","63,70","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["1,30","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["1,30","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["2,30","BAF","I / E",null,"7 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["2,30","BAP",null,null,"7 - 9",null,"Hohlraum sichtbar  "]
["2,30","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["5,50","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["9,80","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["9,80","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["22,80","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["37,00","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["38,00","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["39,70","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["41,70","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["42,80","BAF","I / E",null,"4 - 6",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["45,50","BBA","B","1,00","11 - 1",null,"Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["48,30","BAB","B / A","3,00","11 - 2",null,"Rissbildung Riss in Längsrichtung","A"]
["48,50","BAB","B / A","3,00","11 - 2",null,"Rissbildung Riss in Längsrichtung","B"]
["50,80","BAF","I / E",null,"2 - 4",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["50,80","BAP",null,null,"2 - 4",null,"Hohlraum sichtbar  "]
["53,20","BAB","B / A","3,00","4 - 5",null,"Rissbildung Riss in Längsrichtung","A"]
["53,40","BCA","A / A","150,00","10",null,"Anschluss Abzweig offen"]
["53,60","BAB","B / A","3,00","4 - 5",null,"Rissbildung Riss in Längsrichtung","B"]
["59,80","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["61,30","BAF","E / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["62,70","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["62,70","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J32)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H34/100)*J33","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H35/100)*J33","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H36/100)*J33","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",62.7,2,{"$f":"H37*I37","v":{"v":125.4,"d":"€125"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",62.7,3,{"$f":"H38*I38","v":{"v":188.10000000000002,"d":"€188"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J33:J38)","v":{"v":440.5,"d":"€441"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H40/100)*J39","v":{"v":83.69500000000001,"d":"€84"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J39:J40)","v":{"v":524.195,"d":"€524"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342840","BERLINER STRAßE","62,70","63,70","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["1,30","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["1,30","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["2,30","BAF","I / E",null,"7 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["2,30","BAP",null,null,"7 - 9",null,"Hohlraum sichtbar  "]
["2,30","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["5,50","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["9,80","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["9,80","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["22,80","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["37,00","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["38,00","BDD","C","15,00",null,null,"Wasserspiegel trüb ","A"]
["39,70","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["41,70","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["42,80","BAF","I / E",null,"4 - 6",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["45,50","BBA","B","1,00","11 - 1",null,"Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["48,30","BAB","B / A","3,00","11 - 2",null,"Rissbildung Riss in Längsrichtung","A"]
["48,50","BAB","B / A","3,00","11 - 2",null,"Rissbildung Riss in Längsrichtung","B"]
["50,80","BAF","I / E",null,"2 - 4",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["50,80","BAP",null,null,"2 - 4",null,"Hohlraum sichtbar  "]
["53,20","BAB","B / A","3,00","4 - 5",null,"Rissbildung Riss in Längsrichtung","A"]
["53,40","BCA","A / A","150,00","10",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["53,60","BAB","B / A","3,00","4 - 5",null,"Rissbildung Riss in Längsrichtung","B"]
["59,80","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["61,30","BAF","E / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["62,70","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["62,70","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":6370,"d":"€6,370"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J50:J77)","v":{"v":8430,"d":"€8,430"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H79/100)*J78","v":{"v":843,"d":"€843"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H80/100)*J78","v":{"v":421.5,"d":"€422"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H81/100)*J78","v":{"v":1011.5999999999999,"d":"€1,012"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",62.7,2,{"$f":"H82*I82","v":{"v":125.4,"d":"€125"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",62.7,3,{"$f":"H83*I83","v":{"v":188.10000000000002,"d":"€188"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J78:J83)","v":{"v":11019.6,"d":"€11,020"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H85/100)*J84","v":{"v":2093.724,"d":"€2,094"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J84:J85)","v":{"v":13113.324,"d":"€13,113"}}]

{"sheet":"09343175","index":34,"n_rows":64,"n_cols":10,"rows_kept":64}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09343175","BERLINER STRAßE","31,80","56,91","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["7,70","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["11,40","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["15,00","BAG",null,"20,00","1 - 5",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["15,00","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["15,00","BBE","C","10,00","3 - 6",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["18,10","BBA","C","5,00","1 - 5","JA","Wurzeln komplexes Wurzelwerk ",null,"Fräsen",{"v":50,"d":"€50"}]
["20,40","BAF","E / E",null,"10 - 2",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["21,70","BDD","C","10,00",null,null,"Wasserspiegel trüb ","A"]
["23,30","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["26,00","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["31,20","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["31,20","BAH","C",null,"12 - 12",null,"Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) ",null,"Fräsen,Hut",{"v":450,"d":"€450"}]
["31,20","BAG",null,"25,00","12 - 6",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["31,80","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["31,80","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["31,80","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J21)","v":{"v":700,"d":"€700"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H23/100)*J22","v":{"v":70,"d":"€70"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H24/100)*J22","v":{"v":35,"d":"€35"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H25/100)*J22","v":{"v":84,"d":"€84"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",31.8,2,{"$f":"H26*I26","v":{"v":63.6,"d":"€64"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",31.8,3,{"$f":"H27*I27","v":{"v":95.4,"d":"€95"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J22:J27)","v":{"v":1048,"d":"€1,048"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H29/100)*J28","v":{"v":199.12,"d":"€199"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J28:J29)","v":{"v":1247.12,"d":"€1,247"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09343175","BERLINER STRAßE","31,80","56,91","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["7,70","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["11,40","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["15,00","BAG",null,"20,00","1 - 5",null,"Einragender Anschluss  "]
["15,00","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["15,00","BBE","C","10,00","3 - 6",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["18,10","BBA","C","5,00","1 - 5","JA","Wurzeln komplexes Wurzelwerk ",null,"Fräsen",{"v":50,"d":"€50"}]
["20,40","BAF","E / E",null,"10 - 2",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["21,70","BDD","C","10,00",null,null,"Wasserspiegel trüb ","A"]
["23,30","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["26,00","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["31,20","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["31,20","BAH","C",null,"12 - 12",null,"Schadhafter Anschluss am Umfang des Anschlusses ist teilweise ein Spalt (Anschluss unvollständig eingebunden) "]
["31,20","BAG",null,"25,00","12 - 6",null,"Einragender Anschluss  "]
["31,80","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["31,80","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["31,80","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J39:J55)","v":{"v":1620,"d":"€1,620"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H57/100)*J56","v":{"v":162,"d":"€162"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H58/100)*J56","v":{"v":81,"d":"€81"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H59/100)*J56","v":{"v":194.4,"d":"€194"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",31.8,2,{"$f":"H60*I60","v":{"v":63.6,"d":"€64"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",31.8,3,{"$f":"H61*I61","v":{"v":95.4,"d":"€95"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J56:J61)","v":{"v":2216.4,"d":"€2,216"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H63/100)*J62","v":{"v":421.11600000000004,"d":"€421"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J62:J63)","v":{"v":2637.516,"d":"€2,638"}}]

{"sheet":"09345300","index":35,"n_rows":82,"n_cols":10,"rows_kept":82}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345300","BERLINER STRAßE","57,20","58,20","Not Implemented yet",{"$nulls":3},"250","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,20","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,40","BAG",null,"15,00","1 - 5",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,40","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["14,60","BAG",null,"15,00","1 - 5",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["14,60","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["22,90","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["25,30","BAG",null,"10,00","1 - 5",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["25,30","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["34,60","BAG",null,"10,00","1 - 4",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["34,60","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["36,60","BAF","E / E",null,"5 - 7",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["37,20","BAF","E / E",null,"5 - 7",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["40,60","BBA","B","1,00","5 - 8",null,"Wurzeln einzelne feine Wurzeln ","A","Fräsen",{"v":50,"d":"€50"}]
["41,50","BBA","B","1,00","5 - 8","JA","Wurzeln einzelne feine Wurzeln ","B","Fräsen",{"v":50,"d":"€50"}]
["42,30","BBA","C","5,00","4 - 6","JA","Wurzeln komplexes Wurzelwerk ",null,"Fräsen",{"v":50,"d":"€50"}]
["43,60","BBE","C","15,00","4 - 7",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["43,70","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["43,70","BAH","A",null,"12 - 6",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["44,00","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["44,40","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["47,50","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["50,50","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["51,60","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["56,80","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["57,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J30)","v":{"v":550,"d":"€550"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H32/100)*J31","v":{"v":55,"d":"€55"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H33/100)*J31","v":{"v":27.5,"d":"€28"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H34/100)*J31","v":{"v":66,"d":"€66"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",57.2,2,{"$f":"H35*I35","v":{"v":114.4,"d":"€114"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",57.2,3,{"$f":"H36*I36","v":{"v":171.60000000000002,"d":"€172"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J31:J36)","v":{"v":984.5,"d":"€985"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H38/100)*J37","v":{"v":187.055,"d":"€187"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J37:J38)","v":{"v":1171.555,"d":"€1,172"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345300","BERLINER STRAßE","57,20","58,20","Not Implemented yet",{"$nulls":3},"250","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,20","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,40","BAG",null,"15,00","1 - 5",null,"Einragender Anschluss  "]
["5,40","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["14,60","BAG",null,"15,00","1 - 5",null,"Einragender Anschluss  "]
["14,60","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["22,90","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["25,30","BAG",null,"10,00","1 - 5",null,"Einragender Anschluss  "]
["25,30","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["34,60","BAG",null,"10,00","1 - 4",null,"Einragender Anschluss  "]
["34,60","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["36,60","BAF","E / E",null,"5 - 7",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["37,20","BAF","E / E",null,"5 - 7",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["40,60","BBA","B","1,00","5 - 8",null,"Wurzeln einzelne feine Wurzeln ","A","Fräsen",{"v":50,"d":"€50"}]
["41,50","BBA","B","1,00","5 - 8","JA","Wurzeln einzelne feine Wurzeln ","B","Fräsen",{"v":50,"d":"€50"}]
["42,30","BBA","C","5,00","4 - 6","JA","Wurzeln komplexes Wurzelwerk ",null,"Fräsen",{"v":50,"d":"€50"}]
["43,60","BBE","C","15,00","4 - 7",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["43,70","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["43,70","BAH","A",null,"12 - 6",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["44,00","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["44,40","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["47,50","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["50,50","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["51,60","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["56,80","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["57,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":5820,"d":"€5,820"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J48:J73)","v":{"v":8620,"d":"€8,620"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H75/100)*J74","v":{"v":862,"d":"€862"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H76/100)*J74","v":{"v":431,"d":"€431"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H77/100)*J74","v":{"v":1034.3999999999999,"d":"€1,034"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",57.2,2,{"$f":"H78*I78","v":{"v":114.4,"d":"€114"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",57.2,3,{"$f":"H79*I79","v":{"v":171.60000000000002,"d":"€172"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J74:J79)","v":{"v":11233.4,"d":"€11,233"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H81/100)*J80","v":{"v":2134.346,"d":"€2,134"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J80:J81)","v":{"v":13367.746,"d":"€13,368"}}]

{"sheet":"09345333","index":36,"n_rows":66,"n_cols":10,"rows_kept":66}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333","BERLINER STRAßE","31,00","32,00","Not Implemented yet",{"$nulls":3},"250","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["5,40","BDD","C","15,00",null,null,"Wasserspiegel trüb "]
["5,40","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,40","BAJ","B","25,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["9,50","BAC","A","600,00","1 - 5",null,"Rohrbruch / Einsturz Bruch ","A"]
["9,80","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["9,80","BAG",null,"20,00","12 - 4",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["10,20","BAC","A","600,00","1 - 5",null,"Rohrbruch / Einsturz Bruch ","B"]
["16,00","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["16,90","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["19,60","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["21,00","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["23,30","BAC","B","300,00","2 - 6",null,"Rohrbruch / Einsturz Fehlen von Teilen ","A"]
["23,30","BBE","D","50,00","12 - 6",null,"Andere Hindernisse Gegenstand ragt durch die Wand ein "]
["23,50","BAC","B","300,00","2 - 6",null,"Rohrbruch / Einsturz Fehlen von Teilen ","B"]
["26,00","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["31,00","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J22)","v":{"v":150,"d":"€150"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H24/100)*J23","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H25/100)*J23","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H26/100)*J23","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",31,2,{"$f":"H27*I27","v":{"v":62,"d":"€62"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",31,3,{"$f":"H28*I28","v":{"v":93,"d":"€93"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J23:J28)","v":{"v":345.5,"d":"€346"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H30/100)*J29","v":{"v":65.645,"d":"€66"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J29:J30)","v":{"v":411.145,"d":"€411"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333","BERLINER STRAßE","31,00","32,00","Not Implemented yet",{"$nulls":3},"250","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["5,40","BDD","C","15,00",null,null,"Wasserspiegel trüb "]
["5,40","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,40","BAJ","B","25,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["9,50","BAC","A","600,00","1 - 5",null,"Rohrbruch / Einsturz Bruch ","A"]
["9,80","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["9,80","BAG",null,"20,00","12 - 4",null,"Einragender Anschluss  "]
["10,20","BAC","A","600,00","1 - 5",null,"Rohrbruch / Einsturz Bruch ","B"]
["16,00","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["16,90","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["19,60","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["21,00","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["23,30","BAC","B","300,00","2 - 6",null,"Rohrbruch / Einsturz Fehlen von Teilen ","A"]
["23,30","BBE","D","50,00","12 - 6",null,"Andere Hindernisse Gegenstand ragt durch die Wand ein "]
["23,50","BAC","B","300,00","2 - 6",null,"Rohrbruch / Einsturz Fehlen von Teilen ","B"]
["26,00","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["31,00","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3200,"d":"€3,200"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J40:J57)","v":{"v":5750,"d":"€5,750"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H59/100)*J58","v":{"v":575,"d":"€575"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H60/100)*J58","v":{"v":287.5,"d":"€288"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H61/100)*J58","v":{"v":690,"d":"€690"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",31,2,{"$f":"H62*I62","v":{"v":62,"d":"€62"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",31,3,{"$f":"H63*I63","v":{"v":93,"d":"€93"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J58:J63)","v":{"v":7457.5,"d":"€7,458"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H65/100)*J64","v":{"v":1416.925,"d":"€1,417"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J64:J65)","v":{"v":8874.425,"d":"€8,874"}}]

{"sheet":"09345333_1","index":37,"n_rows":84,"n_cols":10,"rows_kept":84}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333_1","BERLINER STRAßE","47,30","48,30","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["1,30","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,30","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["5,70","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["5,70","BAH","A",null,"12 - 4",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["12,30","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["15,00","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["15,00","BAH","A",null,"12 - 4",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["15,50","BDD","C","10,00",null,null,"Wasserspiegel trüb ","A"]
["18,00","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["22,70","BAG",null,"20,00","1 - 5",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["22,70","BCA","C / A","125,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["25,10","BAH","A",null,"1 - 5",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["25,10","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["27,50","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["34,80","BAB","B / A","2,00","2","JA","Rissbildung Riss in Längsrichtung"]
["34,80","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["34,80","BAH","A",null,"12 - 4",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["37,70","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["38,80","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["39,80","BAF","I / E",null,"4 - 8","JA","Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["44,00","BAH","A",null,"1 - 5",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["44,00","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["46,80","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["46,80","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["47,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J31)","v":{"v":150,"d":"€150"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",47.3,2,{"$f":"H36*I36","v":{"v":94.6,"d":"€95"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",47.3,3,{"$f":"H37*I37","v":{"v":141.89999999999998,"d":"€142"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":427,"d":"€427"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":81.13,"d":"€81"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":508.13,"d":"€508"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333_1","BERLINER STRAßE","47,30","48,30","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["1,30","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["2,30","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["5,70","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["5,70","BAH","A",null,"12 - 4",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["12,30","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["15,00","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["15,00","BAH","A",null,"12 - 4",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["15,50","BDD","C","10,00",null,null,"Wasserspiegel trüb ","A"]
["18,00","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["22,70","BAG",null,"20,00","1 - 5",null,"Einragender Anschluss  "]
["22,70","BCA","C / A","125,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["25,10","BAH","A",null,"1 - 5",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["25,10","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["27,50","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["34,80","BAB","B / A","2,00","2","JA","Rissbildung Riss in Längsrichtung"]
["34,80","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["34,80","BAH","A",null,"12 - 4",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["37,70","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["38,80","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["39,80","BAF","I / E",null,"4 - 8","JA","Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["44,00","BAH","A",null,"1 - 5",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["44,00","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["46,80","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["46,80","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["47,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":4830,"d":"€4,830"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J49:J75)","v":{"v":7820,"d":"€7,820"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H77/100)*J76","v":{"v":782,"d":"€782"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H78/100)*J76","v":{"v":391,"d":"€391"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H79/100)*J76","v":{"v":938.4,"d":"€938"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",47.3,2,{"$f":"H80*I80","v":{"v":94.6,"d":"€95"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",47.3,3,{"$f":"H81*I81","v":{"v":141.89999999999998,"d":"€142"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J76:J81)","v":{"v":10167.9,"d":"€10,168"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H83/100)*J82","v":{"v":1931.9009999999998,"d":"€1,932"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J82:J83)","v":{"v":12099.801,"d":"€12,100"}}]

{"sheet":"09345334","index":38,"n_rows":62,"n_cols":10,"rows_kept":62}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345334","LEIPZIGER STRAßE","29,40","30,40","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,50","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["1,50","BAJ","B","30,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,40","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["14,30","BAI","Z","3,00","2 - 6","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["15,00","BCA","C / A","150,00","1",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["16,80","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["16,80","BAH","E",null,"3 - 9",null,"Schadhafter Anschluss Anschluss verstopft ",null,null,{"v":0,"d":"€0"}]
["16,80","BBE","D","20,00","3 - 6",null,"Andere Hindernisse Gegenstand ragt durch die Wand ein "]
["26,30","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["26,30","BAC","A","900,00","12 - 12",null,"Rohrbruch / Einsturz Bruch ","A"]
["26,60","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["26,80","BAC","A","900,00","12 - 12",null,"Rohrbruch / Einsturz Bruch ","B"]
["27,40","BAB","B / A","2,00","10 - 1",null,"Rissbildung Riss in Längsrichtung","A"]
["28,00","BAB","B / A","2,00","10 - 1",null,"Rissbildung Riss in Längsrichtung","B"]
["29,40","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J20)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H22/100)*J21","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H23/100)*J21","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H24/100)*J21","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29.4,2,{"$f":"H25*I25","v":{"v":58.8,"d":"€59"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29.4,3,{"$f":"H26*I26","v":{"v":88.19999999999999,"d":"€88"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J21:J26)","v":{"v":274,"d":"€274"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H28/100)*J27","v":{"v":52.06,"d":"€52"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J27:J28)","v":{"v":326.06,"d":"€326"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345334","LEIPZIGER STRAßE","29,40","30,40","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,50","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["1,50","BAJ","B","30,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,40","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["14,30","BAI","Z","3,00","2 - 6","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["15,00","BCA","C / A","150,00","1",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["16,80","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["16,80","BAH","E",null,"3 - 9",null,"Schadhafter Anschluss Anschluss verstopft "]
["16,80","BBE","D","20,00","3 - 6",null,"Andere Hindernisse Gegenstand ragt durch die Wand ein "]
["26,30","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["26,30","BAC","A","900,00","12 - 12",null,"Rohrbruch / Einsturz Bruch ","A"]
["26,60","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["26,80","BAC","A","900,00","12 - 12",null,"Rohrbruch / Einsturz Bruch ","B"]
["27,40","BAB","B / A","2,00","10 - 1",null,"Rissbildung Riss in Längsrichtung","A"]
["28,00","BAB","B / A","2,00","10 - 1",null,"Rissbildung Riss in Längsrichtung","B"]
["29,40","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3040,"d":"€3,040"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J38:J53)","v":{"v":6030,"d":"€6,030"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H55/100)*J54","v":{"v":603,"d":"€603"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H56/100)*J54","v":{"v":301.5,"d":"€302"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H57/100)*J54","v":{"v":723.6,"d":"€724"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29.4,2,{"$f":"H58*I58","v":{"v":58.8,"d":"€59"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29.4,3,{"$f":"H59*I59","v":{"v":88.19999999999999,"d":"€88"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J54:J59)","v":{"v":7805.1,"d":"€7,805"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H61/100)*J60","v":{"v":1482.969,"d":"€1,483"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J60:J61)","v":{"v":9288.069,"d":"€9,288"}}]

{"sheet":"09345335","index":39,"n_rows":60,"n_cols":10,"rows_kept":60}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345335","LEIPZIGER STRAßE","48,70","49,70","Not Implemented yet",{"$nulls":3},"250","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["19,60","BAG",null,"10,00","8 - 10",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["19,60","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["21,00","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["25,80","BBE","H","5,00","12 - 6",null,"Andere Hindernisse Gegenstand/Objekt in den Rohrkörper eingebaut "]
["26,10","BAG",null,"10,00","8 - 10",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["26,10","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["32,70","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["39,20","BAH","E",null,"6 - 9",null,"Schadhafter Anschluss Anschluss verstopft ",null,null,{"v":0,"d":"€0"}]
["39,20","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["45,90","BBE","D","20,00","7 - 9",null,"Andere Hindernisse Gegenstand ragt durch die Wand ein "]
["45,90","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["47,90","BAH","E",null,"3 - 9",null,"Schadhafter Anschluss Anschluss verstopft ",null,null,{"v":0,"d":"€0"}]
["47,90","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["48,70","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J19)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H21/100)*J20","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H22/100)*J20","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H23/100)*J20","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",48.7,2,{"$f":"H24*I24","v":{"v":97.4,"d":"€97"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",48.7,3,{"$f":"H25*I25","v":{"v":146.10000000000002,"d":"€146"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J20:J25)","v":{"v":370.5,"d":"€371"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H27/100)*J26","v":{"v":70.395,"d":"€70"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J26:J27)","v":{"v":440.895,"d":"€441"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345335","LEIPZIGER STRAßE","48,70","49,70","Not Implemented yet",{"$nulls":3},"250","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["19,60","BAG",null,"10,00","8 - 10",null,"Einragender Anschluss  "]
["19,60","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["21,00","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["25,80","BBE","H","5,00","12 - 6",null,"Andere Hindernisse Gegenstand/Objekt in den Rohrkörper eingebaut "]
["26,10","BAG",null,"10,00","8 - 10",null,"Einragender Anschluss  "]
["26,10","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["32,70","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["39,20","BAH","E",null,"6 - 9",null,"Schadhafter Anschluss Anschluss verstopft "]
["39,20","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["45,90","BBE","D","20,00","7 - 9",null,"Andere Hindernisse Gegenstand ragt durch die Wand ein "]
["45,90","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["47,90","BAH","E",null,"3 - 9",null,"Schadhafter Anschluss Anschluss verstopft "]
["47,90","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["48,70","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":4970,"d":"€4,970"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J37:J51)","v":{"v":8400,"d":"€8,400"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H53/100)*J52","v":{"v":840,"d":"€840"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H54/100)*J52","v":{"v":420,"d":"€420"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H55/100)*J52","v":{"v":1008,"d":"€1,008"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",48.7,2,{"$f":"H56*I56","v":{"v":97.4,"d":"€97"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",48.7,3,{"$f":"H57*I57","v":{"v":146.10000000000002,"d":"€146"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J52:J57)","v":{"v":10911.5,"d":"€10,912"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H59/100)*J58","v":{"v":2073.185,"d":"€2,073"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J58:J59)","v":{"v":12984.685,"d":"€12,985"}}]

{"sheet":"09345336","index":40,"n_rows":62,"n_cols":10,"rows_kept":62}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345336","LEIPZIGER STRAßE","36,60","37,60","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,20","BBA","B","1,00","9 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,90","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["4,90","BAH","A",null,"12 - 4",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["5,10","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["5,10","BAH","E",null,"3 - 9",null,"Schadhafter Anschluss Anschluss verstopft ",null,null,{"v":0,"d":"€0"}]
["5,20","BAB","B / A","2,00","2 - 3","JA","Rissbildung Riss in Längsrichtung"]
["12,50","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["12,50","BAB","B / A","2,00","12",null,"Rissbildung Riss in Längsrichtung"]
["13,80","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["13,80","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["17,00","BCA","C / A","200,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["25,90","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["25,90","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["35,50","BAC","B","60,00","3 - 9","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["36,60","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J20)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H22/100)*J21","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H23/100)*J21","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H24/100)*J21","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",36.6,2,{"$f":"H25*I25","v":{"v":73.2,"d":"€73"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",36.6,3,{"$f":"H26*I26","v":{"v":109.80000000000001,"d":"€110"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J21:J26)","v":{"v":246.5,"d":"€247"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H28/100)*J27","v":{"v":46.835,"d":"€47"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J27:J28)","v":{"v":293.335,"d":"€293"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345336","LEIPZIGER STRAßE","36,60","37,60","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,20","BBA","B","1,00","9 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,90","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["4,90","BAH","A",null,"12 - 4",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["5,10","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["5,10","BAH","E",null,"3 - 9",null,"Schadhafter Anschluss Anschluss verstopft "]
["5,20","BAB","B / A","2,00","2 - 3","JA","Rissbildung Riss in Längsrichtung"]
["12,50","BCA","C / A","150,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["12,50","BAB","B / A","2,00","12",null,"Rissbildung Riss in Längsrichtung"]
["13,80","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["13,80","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["17,00","BCA","C / A","200,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["25,90","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["25,90","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["35,50","BAC","B","60,00","3 - 9","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["36,60","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3760,"d":"€3,760"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J38:J53)","v":{"v":6750,"d":"€6,750"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H55/100)*J54","v":{"v":675,"d":"€675"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H56/100)*J54","v":{"v":337.5,"d":"€338"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H57/100)*J54","v":{"v":810,"d":"€810"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",36.6,2,{"$f":"H58*I58","v":{"v":73.2,"d":"€73"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",36.6,3,{"$f":"H59*I59","v":{"v":109.80000000000001,"d":"€110"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J54:J59)","v":{"v":8755.5,"d":"€8,756"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H61/100)*J60","v":{"v":1663.545,"d":"€1,664"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J60:J61)","v":{"v":10419.045,"d":"€10,419"}}]

{"sheet":"09345337","index":41,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345337","LEIPZIGER STRAßE","5,00","6,00","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["5,00","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5,2,{"$f":"H11*I11","v":{"v":10,"d":"€10"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5,3,{"$f":"H12*I12","v":{"v":15,"d":"€15"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":25,"d":"€25"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":4.75,"d":"€5"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":29.75,"d":"€30"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345337","LEIPZIGER STRAßE","5,00","6,00","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["5,00","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":900,"d":"€900"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":900,"d":"€900"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":90,"d":"€90"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":45,"d":"€45"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":108,"d":"€108"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5,2,{"$f":"H30*I30","v":{"v":10,"d":"€10"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5,3,{"$f":"H31*I31","v":{"v":15,"d":"€15"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1168,"d":"€1,168"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":221.92000000000002,"d":"€222"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1389.92,"d":"€1,390"}}]

{"sheet":"09345338","index":42,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345338","LEIPZIGER STRAßE","29,20","30,20","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,40","BCA","C / A","150,00","1",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["4,40","BAH","A",null,"12 - 4",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["5,40","BAF","E / E",null,"3 - 7",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["9,00","BCA","B / A","150,00","1",null,"Anschluss Sattelanschluss – gebohrt offen"]
["9,00","BAG",null,"5,00","12 - 3",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["12,70","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["29,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29.2,2,{"$f":"H17*I17","v":{"v":58.4,"d":"€58"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29.2,3,{"$f":"H18*I18","v":{"v":87.6,"d":"€88"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":209.5,"d":"€210"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":39.805,"d":"€40"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":249.305,"d":"€249"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345338","LEIPZIGER STRAßE","29,20","30,20","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,40","BCA","C / A","150,00","1",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["4,40","BAH","A",null,"12 - 4",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["5,40","BAF","E / E",null,"3 - 7",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["9,00","BCA","B / A","150,00","1",null,"Anschluss Sattelanschluss – gebohrt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["9,00","BAG",null,"5,00","12 - 3",null,"Einragender Anschluss  "]
["12,70","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["29,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3020,"d":"€3,020"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":4490,"d":"€4,490"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":449,"d":"€449"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":224.5,"d":"€225"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":538.8,"d":"€539"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29.2,2,{"$f":"H42*I42","v":{"v":58.4,"d":"€58"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29.2,3,{"$f":"H43*I43","v":{"v":87.6,"d":"€88"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":5848.3,"d":"€5,848"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":1111.1770000000001,"d":"€1,111"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":6959.477000000001,"d":"€6,959"}}]

{"sheet":"09345339","index":43,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345339","LEIPZIGER STRAßE","29,20","30,20","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["8,60","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["8,60","BAH","D",null,"12 - 12",null,"Schadhafter Anschluss Anschluss beschädigt ",null,null,{"v":0,"d":"€0"}]
["12,50","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["12,50","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["28,60","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["28,60","BAH","A",null,"12 - 3",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["29,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29.2,2,{"$f":"H17*I17","v":{"v":58.4,"d":"€58"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29.2,3,{"$f":"H18*I18","v":{"v":87.6,"d":"€88"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":146,"d":"€146"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":27.740000000000002,"d":"€28"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":173.74,"d":"€174"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345339","LEIPZIGER STRAßE","29,20","30,20","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["8,60","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["8,60","BAH","D",null,"12 - 12",null,"Schadhafter Anschluss Anschluss beschädigt "]
["12,50","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["12,50","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["28,60","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["28,60","BAH","A",null,"12 - 3",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["29,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3020,"d":"€3,020"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":4490,"d":"€4,490"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":449,"d":"€449"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":224.5,"d":"€225"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":538.8,"d":"€539"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29.2,2,{"$f":"H42*I42","v":{"v":58.4,"d":"€58"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29.2,3,{"$f":"H43*I43","v":{"v":87.6,"d":"€88"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":5848.3,"d":"€5,848"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":1111.1770000000001,"d":"€1,111"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":6959.477000000001,"d":"€6,959"}}]

{"sheet":"09345340","index":44,"n_rows":54,"n_cols":10,"rows_kept":54}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345340","LEIPZIGER STRAßE","29,20","30,20","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["11,10","BBA","C","10,00","12 - 12","JA","Wurzeln komplexes Wurzelwerk ",null,"Fräsen",{"v":50,"d":"€50"}]
["12,10","BBA","C","10,00","12 - 12","JA","Wurzeln komplexes Wurzelwerk ",null,"Fräsen",{"v":50,"d":"€50"}]
["12,80","BBA","C","10,00","6 - 8",null,"Wurzeln komplexes Wurzelwerk ",null,"Fräsen",{"v":50,"d":"€50"}]
["12,90","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["14,10","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["15,10","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["16,20","BBA","B","3,00","1 - 7","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["23,20","BBA","B","3,00","3 - 6","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["24,20","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["25,60","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["29,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J16)","v":{"v":400,"d":"€400"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H18/100)*J17","v":{"v":40,"d":"€40"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H19/100)*J17","v":{"v":20,"d":"€20"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H20/100)*J17","v":{"v":48,"d":"€48"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29.2,2,{"$f":"H21*I21","v":{"v":58.4,"d":"€58"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29.2,3,{"$f":"H22*I22","v":{"v":87.6,"d":"€88"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J17:J22)","v":{"v":654,"d":"€654"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H24/100)*J23","v":{"v":124.26,"d":"€124"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J23:J24)","v":{"v":778.26,"d":"€778"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345340","LEIPZIGER STRAßE","29,20","30,20","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["11,10","BBA","C","10,00","12 - 12","JA","Wurzeln komplexes Wurzelwerk ",null,"Fräsen",{"v":50,"d":"€50"}]
["12,10","BBA","C","10,00","12 - 12","JA","Wurzeln komplexes Wurzelwerk ",null,"Fräsen",{"v":50,"d":"€50"}]
["12,80","BBA","C","10,00","6 - 8",null,"Wurzeln komplexes Wurzelwerk ",null,"Fräsen",{"v":50,"d":"€50"}]
["12,90","BCA","C / A","200,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["14,10","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["15,10","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["16,20","BBA","B","3,00","1 - 7","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["23,20","BBA","B","3,00","3 - 6","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["24,20","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["25,60","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["29,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3020,"d":"€3,020"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J34:J45)","v":{"v":3910,"d":"€3,910"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H47/100)*J46","v":{"v":391,"d":"€391"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H48/100)*J46","v":{"v":195.5,"d":"€196"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H49/100)*J46","v":{"v":469.2,"d":"€469"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",29.2,2,{"$f":"H50*I50","v":{"v":58.4,"d":"€58"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",29.2,3,{"$f":"H51*I51","v":{"v":87.6,"d":"€88"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J46:J51)","v":{"v":5111.7,"d":"€5,112"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H53/100)*J52","v":{"v":971.223,"d":"€971"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J52:J53)","v":{"v":6082.923,"d":"€6,083"}}]

{"sheet":"09345341","index":45,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345341","LEIPZIGER STRAßE","0,20","1,20","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H12*I12","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H13*I13","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345341","LEIPZIGER STRAßE","0,20","1,20","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H32*I32","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H33*I33","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09345342","index":46,"n_rows":56,"n_cols":10,"rows_kept":56}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345342","LEIPZIGER STRAßE","36,20","37,20","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["17,90","BBA","B","2,00","6 - 8","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["19,00","BBA","B","2,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["19,90","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["21,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["22,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["23,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["24,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","A","Fräsen",{"v":50,"d":"€50"}]
["27,00","BBA","B","10,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","C","Fräsen",{"v":50,"d":"€50"}]
["29,80","BBA","B","20,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","C","Fräsen",{"v":50,"d":"€50"}]
["34,00","BBA","B","10,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","C","Fräsen",{"v":50,"d":"€50"}]
["35,20","BBA","B","10,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","B","Fräsen",{"v":50,"d":"€50"}]
["36,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J17)","v":{"v":550,"d":"€550"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H19/100)*J18","v":{"v":55,"d":"€55"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H20/100)*J18","v":{"v":27.5,"d":"€28"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H21/100)*J18","v":{"v":66,"d":"€66"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",36.2,2,{"$f":"H22*I22","v":{"v":72.4,"d":"€72"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",36.2,3,{"$f":"H23*I23","v":{"v":108.60000000000001,"d":"€109"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J18:J23)","v":{"v":879.5,"d":"€880"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H25/100)*J24","v":{"v":167.105,"d":"€167"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J24:J25)","v":{"v":1046.605,"d":"€1,047"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345342","LEIPZIGER STRAßE","36,20","37,20","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["17,90","BBA","B","2,00","6 - 8","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["19,00","BBA","B","2,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["19,90","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["21,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["22,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["23,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["24,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","A","Fräsen",{"v":50,"d":"€50"}]
["27,00","BBA","B","10,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","C","Fräsen",{"v":50,"d":"€50"}]
["29,80","BBA","B","20,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","C","Fräsen",{"v":50,"d":"€50"}]
["34,00","BBA","B","10,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","C","Fräsen",{"v":50,"d":"€50"}]
["35,20","BBA","B","10,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","B","Fräsen",{"v":50,"d":"€50"}]
["36,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3720.0000000000005,"d":"€3,720"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J35:J47)","v":{"v":4270,"d":"€4,270"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H49/100)*J48","v":{"v":427,"d":"€427"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H50/100)*J48","v":{"v":213.5,"d":"€214"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H51/100)*J48","v":{"v":512.4,"d":"€512"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",36.2,2,{"$f":"H52*I52","v":{"v":72.4,"d":"€72"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",36.2,3,{"$f":"H53*I53","v":{"v":108.60000000000001,"d":"€109"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J48:J53)","v":{"v":5603.9,"d":"€5,604"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H55/100)*J54","v":{"v":1064.741,"d":"€1,065"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J54:J55)","v":{"v":6668.641,"d":"€6,669"}}]

{"sheet":"09345342_1","index":47,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345342_1","LEIPZIGER STRAßE","22,80","23,80","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["22,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["22,80","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",22.8,2,{"$f":"H12*I12","v":{"v":45.6,"d":"€46"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",22.8,3,{"$f":"H13*I13","v":{"v":68.4,"d":"€68"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":114,"d":"€114"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":21.66,"d":"€22"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":135.66,"d":"€136"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345342_1","LEIPZIGER STRAßE","22,80","23,80","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["22,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["22,80","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3094,"d":"€3,094"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":3094,"d":"€3,094"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":309.40000000000003,"d":"€309"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":154.70000000000002,"d":"€155"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":371.28,"d":"€371"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",22.8,2,{"$f":"H32*I32","v":{"v":45.6,"d":"€46"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",22.8,3,{"$f":"H33*I33","v":{"v":68.4,"d":"€68"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":4043.38,"d":"€4,043"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":768.2422,"d":"€768"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":4811.6222,"d":"€4,812"}}]

{"sheet":"09345455","index":48,"n_rows":112,"n_cols":10,"rows_kept":112}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345455","BERLINER STRAßE","57,60","58,61","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,40","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,20","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,30","BAI","Z","10,00","1 - 9","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,30","BAI","Z","15,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,30","BAI","Z","10,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["7,20","BBA","B","2,00","2 - 4","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["7,20","BAI","Z","10,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["8,20","BAI","Z","15,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["9,20","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["10,20","BAG",null,"10,00","11 - 1",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["10,20","BCA","C / A","80,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["10,20","BAB","B / C","3,00","12 - 6",null,"Rissbildung Riss komplexe Rissbildung"]
["15,30","BBA","B","2,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["16,30","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["17,40","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["18,60","BAG",null,"20,00","11 - 1",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["18,60","BCA","C / A","80,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["20,30","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["22,40","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["25,40","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["26,40","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["26,70","BAH","A",null,"10 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["26,70","BAG",null,"20,00","10 - 1",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["26,70","BCA","C / A","80,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["27,40","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["28,50","BBA","B","10,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["29,50","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["30,50","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","A","Fräsen",{"v":50,"d":"€50"}]
["34,90","BAG",null,"10,00","10 - 12",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["34,90","BAH","A",null,"10 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["34,90","BCA","C / A","80,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["43,10","BAH","A",null,"8 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["43,10","BCA","C / A","80,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["49,50","BDD","C","10,00",null,null,"Wasserspiegel trüb ","A"]
["51,40","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["51,40","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["51,40","BCA","C / A","80,00","11",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["57,60","BAC","B","100,00","4 - 7","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["57,60","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","B","Fräsen",{"v":50,"d":"€50"}]
["57,60","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J45)","v":{"v":1250,"d":"€1,250"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H47/100)*J46","v":{"v":125,"d":"€125"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H48/100)*J46","v":{"v":62.5,"d":"€63"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H49/100)*J46","v":{"v":150,"d":"€150"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",57.6,2,{"$f":"H50*I50","v":{"v":115.2,"d":"€115"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",57.6,3,{"$f":"H51*I51","v":{"v":172.8,"d":"€173"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J46:J51)","v":{"v":1875.5,"d":"€1,876"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H53/100)*J52","v":{"v":356.345,"d":"€356"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J52:J53)","v":{"v":2231.8450000000003,"d":"€2,232"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345455","BERLINER STRAßE","57,60","58,61","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,40","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["2,20","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["4,30","BAI","Z","10,00","1 - 9","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["5,30","BAI","Z","15,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["6,30","BAI","Z","10,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["7,20","BBA","B","2,00","2 - 4","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["7,20","BAI","Z","10,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["8,20","BAI","Z","15,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["9,20","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["10,20","BAG",null,"10,00","11 - 1",null,"Einragender Anschluss  "]
["10,20","BCA","C / A","80,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["10,20","BAB","B / C","3,00","12 - 6",null,"Rissbildung Riss komplexe Rissbildung"]
["15,30","BBA","B","2,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["16,30","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["17,40","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["18,60","BAG",null,"20,00","11 - 1",null,"Einragender Anschluss  "]
["18,60","BCA","C / A","80,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["20,30","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["22,40","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["25,40","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["26,40","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["26,70","BAH","A",null,"10 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["26,70","BAG",null,"20,00","10 - 1",null,"Einragender Anschluss  "]
["26,70","BCA","C / A","80,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["27,40","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["28,50","BBA","B","10,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["29,50","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["30,50","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","A","Fräsen",{"v":50,"d":"€50"}]
["34,90","BAG",null,"10,00","10 - 12",null,"Einragender Anschluss  "]
["34,90","BAH","A",null,"10 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["34,90","BCA","C / A","80,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["43,10","BAH","A",null,"8 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["43,10","BCA","C / A","80,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["49,50","BDD","C","10,00",null,null,"Wasserspiegel trüb ","A"]
["51,40","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["51,40","BAH","A",null,"9 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["51,40","BCA","C / A","80,00","11",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["57,60","BAC","B","100,00","4 - 7","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["57,60","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","B","Fräsen",{"v":50,"d":"€50"}]
["57,60","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":5861,"d":"€5,861"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J63:J103)","v":{"v":9501,"d":"€9,501"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H105/100)*J104","v":{"v":950.1,"d":"€950"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H106/100)*J104","v":{"v":475.05,"d":"€475"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H107/100)*J104","v":{"v":1140.12,"d":"€1,140"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",57.6,2,{"$f":"H108*I108","v":{"v":115.2,"d":"€115"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",57.6,3,{"$f":"H109*I109","v":{"v":172.8,"d":"€173"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J104:J109)","v":{"v":12354.27,"d":"€12,354"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H111/100)*J110","v":{"v":2347.3113000000003,"d":"€2,347"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J110:J111)","v":{"v":14701.581300000002,"d":"€14,702"}}]

{"sheet":"09345487","index":49,"n_rows":62,"n_cols":10,"rows_kept":62}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345487","BERLINER STRAßE","31,60","32,60","Not Implemented yet",{"$nulls":3},"250","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,80","BBA","B","5,00","3 - 9","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,90","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["7,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["8,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["9,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","A","Fräsen",{"v":50,"d":"€50"}]
["10,70","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["13,80","BAB","B / D","5,00","2 - 7",null,"Rissbildung Riss gewundene oder spiralförmige Rissbildung"]
["13,90","BCA","C / A","200,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["19,90","BBA","A","10,00","6 - 8","JA","Wurzeln Pfahlwurzel ",null,"Fräsen",{"v":50,"d":"€50"}]
["23,00","BBA","B","10,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","C","Fräsen",{"v":50,"d":"€50"}]
["30,30","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["31,10","BBA","B","10,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","B","Fräsen",{"v":50,"d":"€50"}]
["31,60","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J20)","v":{"v":500,"d":"€500"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H22/100)*J21","v":{"v":50,"d":"€50"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H23/100)*J21","v":{"v":25,"d":"€25"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H24/100)*J21","v":{"v":60,"d":"€60"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",31.6,2,{"$f":"H25*I25","v":{"v":63.2,"d":"€63"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",31.6,3,{"$f":"H26*I26","v":{"v":94.80000000000001,"d":"€95"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J21:J26)","v":{"v":793,"d":"€793"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H28/100)*J27","v":{"v":150.67000000000002,"d":"€151"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J27:J28)","v":{"v":943.6700000000001,"d":"€944"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345487","BERLINER STRAßE","31,60","32,60","Not Implemented yet",{"$nulls":3},"250","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,80","BBA","B","5,00","3 - 9","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,90","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["7,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["8,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["9,00","BBA","B","5,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","A","Fräsen",{"v":50,"d":"€50"}]
["10,70","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["13,80","BAB","B / D","5,00","2 - 7",null,"Rissbildung Riss gewundene oder spiralförmige Rissbildung"]
["13,90","BCA","C / A","200,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["19,90","BBA","A","10,00","6 - 8","JA","Wurzeln Pfahlwurzel ",null,"Fräsen",{"v":50,"d":"€50"}]
["23,00","BBA","B","10,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","C","Fräsen",{"v":50,"d":"€50"}]
["30,30","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["31,10","BBA","B","10,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ","B","Fräsen",{"v":50,"d":"€50"}]
["31,60","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3260,"d":"€3,260"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J38:J53)","v":{"v":4250,"d":"€4,250"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H55/100)*J54","v":{"v":425,"d":"€425"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H56/100)*J54","v":{"v":212.5,"d":"€213"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H57/100)*J54","v":{"v":510,"d":"€510"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",31.6,2,{"$f":"H58*I58","v":{"v":63.2,"d":"€63"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",31.6,3,{"$f":"H59*I59","v":{"v":94.80000000000001,"d":"€95"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J54:J59)","v":{"v":5555.5,"d":"€5,556"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H61/100)*J60","v":{"v":1055.545,"d":"€1,056"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J60:J61)","v":{"v":6611.045,"d":"€6,611"}}]

{"sheet":"09345488","index":50,"n_rows":54,"n_cols":10,"rows_kept":54}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345488","LEIPZIGER STRAßE","35,80","36,80","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["9,10","BAH","A",null,"8 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["9,10","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["9,30","BAB","B / A","2,00","10",null,"Rissbildung Riss in Längsrichtung"]
["15,40","BAH","A",null,"8 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["15,40","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["26,00","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["26,00","BAH","B",null,"12 - 12",null,"Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) ",null,null,{"v":0,"d":"€0"}]
["26,00","BAH","A",null,"12 - 5",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["26,60","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["28,20","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["35,80","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J16)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H18/100)*J17","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H19/100)*J17","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H20/100)*J17","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",35.8,2,{"$f":"H21*I21","v":{"v":71.6,"d":"€72"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",35.8,3,{"$f":"H22*I22","v":{"v":107.39999999999999,"d":"€107"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J17:J22)","v":{"v":179,"d":"€179"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H24/100)*J23","v":{"v":34.01,"d":"€34"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J23:J24)","v":{"v":213.01,"d":"€213"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345488","LEIPZIGER STRAßE","35,80","36,80","Not Implemented yet",{"$nulls":3},"300","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["9,10","BAH","A",null,"8 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["9,10","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["9,30","BAB","B / A","2,00","10",null,"Rissbildung Riss in Längsrichtung"]
["15,40","BAH","A",null,"8 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["15,40","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["26,00","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["26,00","BAH","B",null,"12 - 12",null,"Schadhafter Anschluss Spalt zwischen dem Ende des Anschlusses und der Rohrleitung (Zurückliegende Anschluss) "]
["26,00","BAH","A",null,"12 - 5",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["26,60","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["28,20","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["35,80","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":3679.9999999999995,"d":"€3,680"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J34:J45)","v":{"v":5150,"d":"€5,150"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H47/100)*J46","v":{"v":515,"d":"€515"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H48/100)*J46","v":{"v":257.5,"d":"€258"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H49/100)*J46","v":{"v":618,"d":"€618"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",35.8,2,{"$f":"H50*I50","v":{"v":71.6,"d":"€72"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",35.8,3,{"$f":"H51*I51","v":{"v":107.39999999999999,"d":"€107"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J46:J51)","v":{"v":6719.5,"d":"€6,720"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H53/100)*J52","v":{"v":1276.705,"d":"€1,277"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J52:J53)","v":{"v":7996.205,"d":"€7,996"}}]

{"sheet":"09345577","index":51,"n_rows":54,"n_cols":10,"rows_kept":54}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345577","BERLINER STRAßE","11,80","12,00","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,70","BAF","E / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["2,80","BAF","E / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["2,80","BAF","I / E",null,"5 - 7",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["2,90","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["5,80","BAF","E / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["8,20","BAF","E / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["9,70","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["11,30","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["11,30","BAH","D",null,"12 - 12",null,"Schadhafter Anschluss Anschluss beschädigt ",null,null,{"v":0,"d":"€0"}]
["11,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["11,80","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J16)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H18/100)*J17","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H19/100)*J17","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H20/100)*J17","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",11.8,2,{"$f":"H21*I21","v":{"v":23.6,"d":"€24"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",11.8,3,{"$f":"H22*I22","v":{"v":35.400000000000006,"d":"€35"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J17:J22)","v":{"v":122.5,"d":"€123"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H24/100)*J23","v":{"v":23.275,"d":"€23"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J23:J24)","v":{"v":145.775,"d":"€146"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345577","BERLINER STRAßE","11,80","12,00","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,70","BAF","E / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["2,80","BAF","E / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["2,80","BAF","I / E",null,"5 - 7",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["2,90","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["5,80","BAF","E / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["8,20","BAF","E / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["9,70","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["11,30","BCA","C / A","150,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["11,30","BAH","D",null,"12 - 12",null,"Schadhafter Anschluss Anschluss beschädigt "]
["11,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["11,80","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":1800,"d":"€1,800"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J34:J45)","v":{"v":2830,"d":"€2,830"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H47/100)*J46","v":{"v":283,"d":"€283"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H48/100)*J46","v":{"v":141.5,"d":"€142"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H49/100)*J46","v":{"v":339.59999999999997,"d":"€340"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",11.8,2,{"$f":"H50*I50","v":{"v":23.6,"d":"€24"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",11.8,3,{"$f":"H51*I51","v":{"v":35.400000000000006,"d":"€35"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J46:J51)","v":{"v":3653.1,"d":"€3,653"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H53/100)*J52","v":{"v":694.0889999999999,"d":"€694"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J52:J53)","v":{"v":4347.189,"d":"€4,347"}}]

{"sheet":"09345819","index":52,"n_rows":100,"n_cols":10,"rows_kept":100}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345819","LEIPZIGER STRAßE","45,40","46,40","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["6,70","BAF","C / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["10,30","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["10,50","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["10,70","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["10,70","BAO",null,null,"4 - 8",null,"Boden sichtbar  "]
["10,70","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["17,00","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["17,00","BAF","C / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["17,80","BCA","A / A","150,00","2",null,"Anschluss Abzweig offen"]
["18,50","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["18,60","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["24,60","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["24,80","BAC","C",null,"3 - 9",null,"Rohrbruch / Einsturz Einsturz ","A"]
["24,80","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["25,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["25,20","BAC","C",null,"3 - 9",null,"Rohrbruch / Einsturz Einsturz ","B"]
["31,30","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["31,30","BAC","C",null,"4 - 8",null,"Rohrbruch / Einsturz Einsturz ","A"]
["31,30","BAO",null,null,"4 - 8",null,"Boden sichtbar  ","A"]
["31,40","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["31,60","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["31,60","BAC","C",null,"4 - 8",null,"Rohrbruch / Einsturz Einsturz ","B"]
["31,60","BAO",null,null,"4 - 8",null,"Boden sichtbar  ","B"]
["38,90","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["39,00","BAC","C",null,"4 - 8",null,"Rohrbruch / Einsturz Einsturz ","A"]
["39,00","BAO",null,null,"4 - 8",null,"Boden sichtbar  ","A"]
["39,10","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["39,20","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["39,20","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["39,20","BAC","C",null,"4 - 8",null,"Rohrbruch / Einsturz Einsturz ","B"]
["39,20","BAO",null,null,"4 - 8",null,"Boden sichtbar  ","B"]
["39,70","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["45,40","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["45,40","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J39)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",45.4,2,{"$f":"H44*I44","v":{"v":90.8,"d":"€91"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",45.4,3,{"$f":"H45*I45","v":{"v":136.2,"d":"€136"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":227,"d":"€227"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":43.13,"d":"€43"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":270.13,"d":"€270"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345819","LEIPZIGER STRAßE","45,40","46,40","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["6,70","BAF","C / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["10,30","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["10,50","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["10,70","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["10,70","BAO",null,null,"4 - 8",null,"Boden sichtbar  "]
["10,70","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["17,00","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["17,00","BAF","C / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["17,80","BCA","A / A","150,00","2",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["18,50","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["18,60","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["24,60","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["24,80","BAC","C",null,"3 - 9",null,"Rohrbruch / Einsturz Einsturz ","A"]
["24,80","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["25,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["25,20","BAC","C",null,"3 - 9",null,"Rohrbruch / Einsturz Einsturz ","B"]
["31,30","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["31,30","BAC","C",null,"4 - 8",null,"Rohrbruch / Einsturz Einsturz ","A"]
["31,30","BAO",null,null,"4 - 8",null,"Boden sichtbar  ","A"]
["31,40","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["31,60","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["31,60","BAC","C",null,"4 - 8",null,"Rohrbruch / Einsturz Einsturz ","B"]
["31,60","BAO",null,null,"4 - 8",null,"Boden sichtbar  ","B"]
["38,90","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["39,00","BAC","C",null,"4 - 8",null,"Rohrbruch / Einsturz Einsturz ","A"]
["39,00","BAO",null,null,"4 - 8",null,"Boden sichtbar  ","A"]
["39,10","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["39,20","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["39,20","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["39,20","BAC","C",null,"4 - 8",null,"Rohrbruch / Einsturz Einsturz ","B"]
["39,20","BAO",null,null,"4 - 8",null,"Boden sichtbar  ","B"]
["39,70","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["45,40","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["45,40","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":4640,"d":"€4,640"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J57:J91)","v":{"v":7090,"d":"€7,090"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H93/100)*J92","v":{"v":709,"d":"€709"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H94/100)*J92","v":{"v":354.5,"d":"€355"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H95/100)*J92","v":{"v":850.8,"d":"€851"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",45.4,2,{"$f":"H96*I96","v":{"v":90.8,"d":"€91"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",45.4,3,{"$f":"H97*I97","v":{"v":136.2,"d":"€136"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J92:J97)","v":{"v":9231.3,"d":"€9,231"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H99/100)*J98","v":{"v":1753.947,"d":"€1,754"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J98:J99)","v":{"v":10985.247,"d":"€10,985"}}]

{"sheet":"09345820","index":53,"n_rows":98,"n_cols":10,"rows_kept":98}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345820","LEIPZIGER STRAßE","45,00","46,00","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["6,20","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["10,20","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["10,20","BAO",null,null,"4 - 8",null,"Boden sichtbar  "]
["10,40","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["10,50","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["10,50","BAO",null,null,"4 - 8",null,"Boden sichtbar  "]
["17,70","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["17,70","BAO",null,null,"4 - 8",null,"Boden sichtbar  ","A"]
["17,80","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["18,00","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["18,00","BAO",null,null,"4 - 8",null,"Boden sichtbar  ","B"]
["20,10","BBA","B","3,00","4 - 8","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["21,10","BBA","B","3,00","3 - 9","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["24,30","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["24,30","BAO",null,null,"3 - 9",null,"Boden sichtbar  ","A"]
["24,40","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["24,60","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["24,60","BAO",null,null,"3 - 9",null,"Boden sichtbar  ","B"]
["25,80","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["31,80","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["31,80","BAO",null,null,"3 - 9",null,"Boden sichtbar  ","A"]
["31,90","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["32,10","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["32,10","BAO",null,null,"3 - 9",null,"Boden sichtbar  ","B"]
["38,20","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["38,20","BAO",null,null,"3 - 9",null,"Boden sichtbar  ","A"]
["38,20","BBA","B","5,00","4 - 8",null,"Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["38,40","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["38,50","BAO",null,null,"3 - 9",null,"Boden sichtbar  ","B"]
["38,50","BAF","I / E",null,"12 - 12",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["38,50","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  "]
["44,60","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["45,00","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J38)","v":{"v":150,"d":"€150"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H40/100)*J39","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H41/100)*J39","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H42/100)*J39","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",45,2,{"$f":"H43*I43","v":{"v":90,"d":"€90"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",45,3,{"$f":"H44*I44","v":{"v":135,"d":"€135"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J39:J44)","v":{"v":415.5,"d":"€416"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H46/100)*J45","v":{"v":78.94500000000001,"d":"€79"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J45:J46)","v":{"v":494.445,"d":"€494"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345820","LEIPZIGER STRAßE","45,00","46,00","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["6,20","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["10,20","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["10,20","BAO",null,null,"4 - 8",null,"Boden sichtbar  "]
["10,40","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["10,50","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["10,50","BAO",null,null,"4 - 8",null,"Boden sichtbar  "]
["17,70","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["17,70","BAO",null,null,"4 - 8",null,"Boden sichtbar  ","A"]
["17,80","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["18,00","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["18,00","BAO",null,null,"4 - 8",null,"Boden sichtbar  ","B"]
["20,10","BBA","B","3,00","4 - 8","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["21,10","BBA","B","3,00","3 - 9","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["24,30","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["24,30","BAO",null,null,"3 - 9",null,"Boden sichtbar  ","A"]
["24,40","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["24,60","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["24,60","BAO",null,null,"3 - 9",null,"Boden sichtbar  ","B"]
["25,80","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["31,80","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["31,80","BAO",null,null,"3 - 9",null,"Boden sichtbar  ","A"]
["31,90","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["32,10","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["32,10","BAO",null,null,"3 - 9",null,"Boden sichtbar  ","B"]
["38,20","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["38,20","BAO",null,null,"3 - 9",null,"Boden sichtbar  ","A"]
["38,20","BBA","B","5,00","4 - 8",null,"Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["38,40","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["38,50","BAO",null,null,"3 - 9",null,"Boden sichtbar  ","B"]
["38,50","BAF","I / E",null,"12 - 12",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["38,50","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  "]
["44,60","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["45,00","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":4600,"d":"€4,600"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J56:J89)","v":{"v":7200,"d":"€7,200"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H91/100)*J90","v":{"v":720,"d":"€720"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H92/100)*J90","v":{"v":360,"d":"€360"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H93/100)*J90","v":{"v":864,"d":"€864"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",45,2,{"$f":"H94*I94","v":{"v":90,"d":"€90"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",45,3,{"$f":"H95*I95","v":{"v":135,"d":"€135"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J90:J95)","v":{"v":9369,"d":"€9,369"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H97/100)*J96","v":{"v":1780.1100000000001,"d":"€1,780"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J96:J97)","v":{"v":11149.11,"d":"€11,149"}}]

{"sheet":"09345821","index":54,"n_rows":60,"n_cols":10,"rows_kept":60}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345821","LEIPZIGER STRAßE","44,50","45,50","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["6,40","BAI","Z","5,00","11 - 1","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["11,20","BAH","A",null,"8 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["11,20","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["18,40","BBE","C","10,00","6 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["18,40","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["18,40","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["25,10","BAH","A",null,"8 - 11",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["25,10","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["32,00","BAH","A",null,"8 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["32,00","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["38,90","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["44,50","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["44,50","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J19)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H21/100)*J20","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H22/100)*J20","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H23/100)*J20","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",44.5,2,{"$f":"H24*I24","v":{"v":89,"d":"€89"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",44.5,3,{"$f":"H25*I25","v":{"v":133.5,"d":"€134"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J20:J25)","v":{"v":286,"d":"€286"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H27/100)*J26","v":{"v":54.34,"d":"€54"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J26:J27)","v":{"v":340.34000000000003,"d":"€340"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345821","LEIPZIGER STRAßE","44,50","45,50","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["6,40","BAI","Z","5,00","11 - 1","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["11,20","BAH","A",null,"8 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["11,20","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["18,40","BBE","C","10,00","6 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["18,40","BAH","A",null,"8 - 1",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["18,40","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["25,10","BAH","A",null,"8 - 11",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["25,10","BCA","C / A","150,00","10",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["32,00","BAH","A",null,"8 - 12",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["32,00","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["38,90","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["44,50","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["44,50","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":4550,"d":"€4,550"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J37:J51)","v":{"v":7000,"d":"€7,000"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H53/100)*J52","v":{"v":700,"d":"€700"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H54/100)*J52","v":{"v":350,"d":"€350"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H55/100)*J52","v":{"v":840,"d":"€840"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",44.5,2,{"$f":"H56*I56","v":{"v":89,"d":"€89"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",44.5,3,{"$f":"H57*I57","v":{"v":133.5,"d":"€134"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J52:J57)","v":{"v":9112.5,"d":"€9,113"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H59/100)*J58","v":{"v":1731.375,"d":"€1,731"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J58:J59)","v":{"v":10843.875,"d":"€10,844"}}]

{"sheet":"09340048SE03","index":55,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340048SE03","BERLINER STRAßE","1,40","1,60","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,40","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.4,2,{"$f":"H11*I11","v":{"v":2.8,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.4,3,{"$f":"H12*I12","v":{"v":4.199999999999999,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":6.999999999999999,"d":"€7"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":1.3299999999999998,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":8.329999999999998,"d":"€8"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340048SE03","BERLINER STRAßE","1,40","1,60","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,40","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.4,2,{"$f":"H30*I30","v":{"v":2.8,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.4,3,{"$f":"H31*I31","v":{"v":4.199999999999999,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":6.999999999999999,"d":"€7"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":1.3299999999999998,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":8.329999999999998,"d":"€8"}}]

{"sheet":"09340049SE02","index":56,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340049SE02","BERLINER STRAßE","1,30","1,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.3,2,{"$f":"H11*I11","v":{"v":2.6,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.3,3,{"$f":"H12*I12","v":{"v":3.9000000000000004,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":6.5,"d":"€7"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":1.235,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":7.735,"d":"€8"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340049SE02","BERLINER STRAßE","1,30","1,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.3,2,{"$f":"H30*I30","v":{"v":2.6,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.3,3,{"$f":"H31*I31","v":{"v":3.9000000000000004,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":6.5,"d":"€7"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":1.235,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":7.735,"d":"€8"}}]

{"sheet":"09340052SE02","index":57,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340052SE02","BERLINER STRAßE","1,50","1,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,50","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.5,2,{"$f":"H11*I11","v":{"v":3,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.5,3,{"$f":"H12*I12","v":{"v":4.5,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":7.5,"d":"€8"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":1.425,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":8.925,"d":"€9"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340052SE02","BERLINER STRAßE","1,50","1,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,50","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.5,2,{"$f":"H30*I30","v":{"v":3,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.5,3,{"$f":"H31*I31","v":{"v":4.5,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":7.5,"d":"€8"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":1.425,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":8.925,"d":"€9"}}]

{"sheet":"09340053RR02","index":58,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340053RR02","BERLINER STRAßE","7,50","7,50","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,30","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["4,50","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["7,50","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["7,50","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",7.5,2,{"$f":"H14*I14","v":{"v":15,"d":"€15"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",7.5,3,{"$f":"H15*I15","v":{"v":22.5,"d":"€23"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":37.5,"d":"€38"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":7.125,"d":"€7"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":44.625,"d":"€45"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340053RR02","BERLINER STRAßE","7,50","7,50","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,30","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["4,50","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["7,50","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["7,50","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",7.5,2,{"$f":"H36*I36","v":{"v":15,"d":"€15"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",7.5,3,{"$f":"H37*I37","v":{"v":22.5,"d":"€23"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":37.5,"d":"€38"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":7.125,"d":"€7"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":44.625,"d":"€45"}}]

{"sheet":"09340053SE01","index":59,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340053SE01","BERLINER STRAßE","1,90","2,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.9,2,{"$f":"H11*I11","v":{"v":3.8,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.9,3,{"$f":"H12*I12","v":{"v":5.699999999999999,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":9.5,"d":"€10"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":1.805,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":11.305,"d":"€11"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340053SE01","BERLINER STRAßE","1,90","2,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.9,2,{"$f":"H30*I30","v":{"v":3.8,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.9,3,{"$f":"H31*I31","v":{"v":5.699999999999999,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":9.5,"d":"€10"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":1.805,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":11.305,"d":"€11"}}]

{"sheet":"09340054SE01","index":60,"n_rows":56,"n_cols":10,"rows_kept":56}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340054SE01","BERLINER STRAßE","22,00","22,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["1,00","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["1,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","C"]
["2,70","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["3,20","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["9,40","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["9,40","BBD","A","10,00","4 - 6",null,"Eindringen von Bodenmaterial Sand "]
["19,80","BBE","C","10,00","3 - 6","JA","Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["21,70","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["22,00","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["22,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["22,00","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J17)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H19/100)*J18","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H20/100)*J18","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H21/100)*J18","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",22,2,{"$f":"H22*I22","v":{"v":44,"d":"€44"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",22,3,{"$f":"H23*I23","v":{"v":66,"d":"€66"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J18:J23)","v":{"v":110,"d":"€110"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H25/100)*J24","v":{"v":20.9,"d":"€21"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J24:J25)","v":{"v":130.9,"d":"€131"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340054SE01","BERLINER STRAßE","22,00","22,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["1,00","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["1,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","C"]
["2,70","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["3,20","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["9,40","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","C"]
["9,40","BBD","A","10,00","4 - 6",null,"Eindringen von Bodenmaterial Sand "]
["19,80","BBE","C","10,00","3 - 6","JA","Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["21,70","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["22,00","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["22,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["22,00","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J35:J47)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H49/100)*J48","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H50/100)*J48","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H51/100)*J48","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",22,2,{"$f":"H52*I52","v":{"v":44,"d":"€44"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",22,3,{"$f":"H53*I53","v":{"v":66,"d":"€66"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J48:J53)","v":{"v":110,"d":"€110"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H55/100)*J54","v":{"v":20.9,"d":"€21"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J54:J55)","v":{"v":130.9,"d":"€131"}}]

{"sheet":"09340054SE02","index":61,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340054SE02","BERLINER STRAßE","2,10","2,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["0,10","BAB","B / B","5,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["0,10","BBF","B",null,"12 - 12",null,"Infiltration Tropfen "]
["0,90","BAC","B","50,00","4 - 8","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["0,90","BAP",null,null,"4 - 8","JA","Hohlraum sichtbar  "]
["2,10","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["2,10","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.1,2,{"$f":"H17*I17","v":{"v":4.2,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.1,3,{"$f":"H18*I18","v":{"v":6.300000000000001,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":10.5,"d":"€11"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":1.995,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":12.495000000000001,"d":"€12"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340054SE02","BERLINER STRAßE","2,10","2,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["0,10","BAB","B / B","5,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["0,10","BBF","B",null,"12 - 12",null,"Infiltration Tropfen "]
["0,90","BAC","B","50,00","4 - 8","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["0,90","BAP",null,null,"4 - 8","JA","Hohlraum sichtbar  "]
["2,10","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["2,10","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.1,2,{"$f":"H42*I42","v":{"v":4.2,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.1,3,{"$f":"H43*I43","v":{"v":6.300000000000001,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":10.5,"d":"€11"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":1.995,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":12.495000000000001,"d":"€12"}}]

{"sheet":"09340056GA04","index":62,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340056GA04","BERLINER STRAßE","3,30","3,30","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,40","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,80","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["2,90","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["3,30","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.3,2,{"$f":"H15*I15","v":{"v":6.6,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.3,3,{"$f":"H16*I16","v":{"v":9.899999999999999,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":16.5,"d":"€17"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":3.1350000000000002,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":19.635,"d":"€20"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340056GA04","BERLINER STRAßE","3,30","3,30","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,40","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,80","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["2,90","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["3,30","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.3,2,{"$f":"H38*I38","v":{"v":6.6,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.3,3,{"$f":"H39*I39","v":{"v":9.899999999999999,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":16.5,"d":"€17"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":3.1350000000000002,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":19.635,"d":"€20"}}]

{"sheet":"09340056GA06","index":63,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340056GA06","BERLINER STRAßE","2,20","2,20","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / B","30,00","7",null,"Krümmung der Leitung nach links nach unten"]
["0,30","BCC","B / Y","30,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,50","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,10","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["1,60","BBE","C","20,00","12 - 12","JA","Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["2,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.2,2,{"$f":"H16*I16","v":{"v":4.4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.2,3,{"$f":"H17*I17","v":{"v":6.6000000000000005,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":11,"d":"€11"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":2.09,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":13.09,"d":"€13"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340056GA06","BERLINER STRAßE","2,20","2,20","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / B","30,00","7",null,"Krümmung der Leitung nach links nach unten"]
["0,30","BCC","B / Y","30,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,50","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,10","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["1,60","BBE","C","20,00","12 - 12","JA","Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["2,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.2,2,{"$f":"H40*I40","v":{"v":4.4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.2,3,{"$f":"H41*I41","v":{"v":6.6000000000000005,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":11,"d":"€11"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":2.09,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":13.09,"d":"€13"}}]

{"sheet":"09340056NN01","index":64,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340056NN01","BERLINER STRAßE","1,30","1,30","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / B","30,00","4",null,"Krümmung der Leitung nach rechts nach unten"]
["0,40","BCC","A / Y","15,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,60","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["0,90","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["1,30","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.3,2,{"$f":"H15*I15","v":{"v":2.6,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.3,3,{"$f":"H16*I16","v":{"v":3.9000000000000004,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":6.5,"d":"€7"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":1.235,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":7.735,"d":"€8"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340056NN01","BERLINER STRAßE","1,30","1,30","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / B","30,00","4",null,"Krümmung der Leitung nach rechts nach unten"]
["0,40","BCC","A / Y","15,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,60","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["0,90","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["1,30","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.3,2,{"$f":"H38*I38","v":{"v":2.6,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.3,3,{"$f":"H39*I39","v":{"v":3.9000000000000004,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":6.5,"d":"€7"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":1.235,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":7.735,"d":"€8"}}]

{"sheet":"09340056SE02","index":65,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340056SE02","BERLINER STRAßE","2,30","2,50","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,40","BCC","B / B","45,00","4",null,"Krümmung der Leitung nach rechts nach unten"]
["0,70","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["0,70","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.3,2,{"$f":"H14*I14","v":{"v":4.6,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.3,3,{"$f":"H15*I15","v":{"v":6.8999999999999995,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":11.5,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":2.185,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":13.685,"d":"€14"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340056SE02","BERLINER STRAßE","2,30","2,50","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,40","BCC","B / B","45,00","4",null,"Krümmung der Leitung nach rechts nach unten"]
["0,70","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["0,70","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.3,2,{"$f":"H36*I36","v":{"v":4.6,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.3,3,{"$f":"H37*I37","v":{"v":6.8999999999999995,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":11.5,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":2.185,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":13.685,"d":"€14"}}]

{"sheet":"09340056SE03","index":66,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340056SE03","BERLINER STRAßE","10,40","10,60","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,40","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["0,50","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,00","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["10,40","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",10.4,2,{"$f":"H15*I15","v":{"v":20.8,"d":"€21"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",10.4,3,{"$f":"H16*I16","v":{"v":31.200000000000003,"d":"€31"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":52,"d":"€52"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":9.88,"d":"€10"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":61.88,"d":"€62"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340056SE03","BERLINER STRAßE","10,40","10,60","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,40","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["0,50","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,00","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["10,40","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",10.4,2,{"$f":"H38*I38","v":{"v":20.8,"d":"€21"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",10.4,3,{"$f":"H39*I39","v":{"v":31.200000000000003,"d":"€31"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":52,"d":"€52"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":9.88,"d":"€10"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":61.88,"d":"€62"}}]

{"sheet":"09340056SE05","index":67,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340056SE05","BERLINER STRAßE","2,10","2,30","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["0,20","BCC","B / Y","30,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,40","BCC","B / Y","30,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,50","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,20","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["1,80","BAJ","A","100,00","12 - 12","JA","Verschobene Verbindung in längsrichtung ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,10","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.1,2,{"$f":"H17*I17","v":{"v":4.2,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.1,3,{"$f":"H18*I18","v":{"v":6.300000000000001,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":74,"d":"€74"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":14.06,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":88.06,"d":"€88"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340056SE05","BERLINER STRAßE","2,10","2,30","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["0,20","BCC","B / Y","30,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,40","BCC","B / Y","30,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,50","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,20","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["1,80","BAJ","A","100,00","12 - 12","JA","Verschobene Verbindung in längsrichtung ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,10","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.1,2,{"$f":"H42*I42","v":{"v":4.2,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.1,3,{"$f":"H43*I43","v":{"v":6.300000000000001,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":74,"d":"€74"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":14.06,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":88.06,"d":"€88"}}]

{"sheet":"09340585GA01","index":68,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585GA01","BERLINER STRAßE","1,80","1,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,80","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,80","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["1,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.8,2,{"$f":"H15*I15","v":{"v":3.6,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.8,3,{"$f":"H16*I16","v":{"v":5.4,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":9,"d":"€9"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":1.71,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":10.71,"d":"€11"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585GA01","BERLINER STRAßE","1,80","1,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,80","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,80","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["1,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.8,2,{"$f":"H38*I38","v":{"v":3.6,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.8,3,{"$f":"H39*I39","v":{"v":5.4,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":9,"d":"€9"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":1.71,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":10.71,"d":"€11"}}]

{"sheet":"09340585GA02","index":69,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585GA02","BERLINER STRAßE","1,20","1,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,10","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,20","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,20","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["1,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.2,2,{"$f":"H16*I16","v":{"v":2.4,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.2,3,{"$f":"H17*I17","v":{"v":3.5999999999999996,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":69.5,"d":"€70"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":13.205,"d":"€13"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":82.705,"d":"€83"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585GA02","BERLINER STRAßE","1,20","1,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,10","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,20","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,20","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["1,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.2,2,{"$f":"H40*I40","v":{"v":2.4,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.2,3,{"$f":"H41*I41","v":{"v":3.5999999999999996,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":69.5,"d":"€70"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":13.205,"d":"€13"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":82.705,"d":"€83"}}]

{"sheet":"09340585GA04","index":70,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585GA04","BERLINER STRAßE","1,30","1,30","Not Implemented yet",{"$nulls":3},"100","PVC"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,00","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,20","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,30","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["1,30","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.3,2,{"$f":"H15*I15","v":{"v":2.6,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.3,3,{"$f":"H16*I16","v":{"v":3.9000000000000004,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":6.5,"d":"€7"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":1.235,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":7.735,"d":"€8"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585GA04","BERLINER STRAßE","1,30","1,30","Not Implemented yet",{"$nulls":3},"100","PVC"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,00","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,20","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,30","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["1,30","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.3,2,{"$f":"H38*I38","v":{"v":2.6,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.3,3,{"$f":"H39*I39","v":{"v":3.9000000000000004,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":6.5,"d":"€7"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":1.235,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":7.735,"d":"€8"}}]

{"sheet":"09340585GA06","index":71,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585GA06","BERLINER STRAßE","1,90","1,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,20","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,90","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["1,90","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,90","BAB","B / D","2,00","9 - 3",null,"Rissbildung Riss gewundene oder spiralförmige Rissbildung"]
["1,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.9,2,{"$f":"H17*I17","v":{"v":3.8,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.9,3,{"$f":"H18*I18","v":{"v":5.699999999999999,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":73,"d":"€73"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":13.870000000000001,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":86.87,"d":"€87"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585GA06","BERLINER STRAßE","1,90","1,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,20","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,90","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["1,90","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,90","BAB","B / D","2,00","9 - 3",null,"Rissbildung Riss gewundene oder spiralförmige Rissbildung"]
["1,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.9,2,{"$f":"H42*I42","v":{"v":3.8,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.9,3,{"$f":"H43*I43","v":{"v":5.699999999999999,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":73,"d":"€73"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":13.870000000000001,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":86.87,"d":"€87"}}]

{"sheet":"09340585GA08","index":72,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585GA08","BERLINER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"100","PVC"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,90","BCC","Y / A","15,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,00","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["1,00","BCC","Y / B","15,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H14*I14","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H15*I15","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":6.545,"d":"€7"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585GA08","BERLINER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"100","PVC"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,90","BCC","Y / A","15,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,00","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["1,00","BCC","Y / B","15,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H36*I36","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H37*I37","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":6.545,"d":"€7"}}]

{"sheet":"09340585GA09","index":73,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585GA09","BERLINER STRAßE","1,80","1,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["0,10","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,40","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,70","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,70","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["1,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.8,2,{"$f":"H17*I17","v":{"v":3.6,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.8,3,{"$f":"H18*I18","v":{"v":5.4,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":136,"d":"€136"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":25.84,"d":"€26"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":161.84,"d":"€162"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585GA09","BERLINER STRAßE","1,80","1,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["0,10","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,40","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,70","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,70","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["1,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.8,2,{"$f":"H42*I42","v":{"v":3.6,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.8,3,{"$f":"H43*I43","v":{"v":5.4,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":136,"d":"€136"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":25.84,"d":"€26"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":161.84,"d":"€162"}}]

{"sheet":"09340585GA10","index":74,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585GA10","BERLINER STRAßE","2,20","2,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["0,30","BBC","C","3,00","5 - 7",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["1,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,80","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,80","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["2,20","BBC","C","3,00","5 - 7",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["2,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.2,2,{"$f":"H17*I17","v":{"v":4.4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.2,3,{"$f":"H18*I18","v":{"v":6.6000000000000005,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":138,"d":"€138"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":26.22,"d":"€26"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":164.22,"d":"€164"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585GA10","BERLINER STRAßE","2,20","2,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["0,30","BBC","C","3,00","5 - 7",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["1,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,80","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,80","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["2,20","BBC","C","3,00","5 - 7",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["2,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.2,2,{"$f":"H42*I42","v":{"v":4.4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.2,3,{"$f":"H43*I43","v":{"v":6.6000000000000005,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":138,"d":"€138"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":26.22,"d":"€26"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":164.22,"d":"€164"}}]

{"sheet":"09340585NN05","index":75,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585NN05","BERLINER STRAßE","1,80","1,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,20","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,80","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,80","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["1,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.8,2,{"$f":"H16*I16","v":{"v":3.6,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.8,3,{"$f":"H17*I17","v":{"v":5.4,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":72.5,"d":"€73"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":13.775,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":86.275,"d":"€86"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585NN05","BERLINER STRAßE","1,80","1,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,20","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,80","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,80","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["1,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.8,2,{"$f":"H40*I40","v":{"v":3.6,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.8,3,{"$f":"H41*I41","v":{"v":5.4,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":72.5,"d":"€73"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":13.775,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":86.275,"d":"€86"}}]

{"sheet":"09340585NN11","index":76,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585NN11","BERLINER STRAßE","0,30","0,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BBE","C","10,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["0,30","BBE","C","90,00","12 - 12",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["0,30","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.3,2,{"$f":"H13*I13","v":{"v":0.6,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.3,3,{"$f":"H14*I14","v":{"v":0.8999999999999999,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":1.5,"d":"€2"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":0.28500000000000003,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":1.7850000000000001,"d":"€2"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585NN11","BERLINER STRAßE","0,30","0,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BBE","C","10,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["0,30","BBE","C","90,00","12 - 12",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["0,30","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.3,2,{"$f":"H34*I34","v":{"v":0.6,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.3,3,{"$f":"H35*I35","v":{"v":0.8999999999999999,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":1.5,"d":"€2"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":0.28500000000000003,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":1.7850000000000001,"d":"€2"}}]

{"sheet":"09340585RR03","index":77,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585RR03","BERLINER STRAßE","1,80","1,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,80","BAJ","A","30,00","12 - 12","JA","Verschobene Verbindung in längsrichtung ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,20","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,20","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["1,60","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,80","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,80","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.8,2,{"$f":"H16*I16","v":{"v":3.6,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.8,3,{"$f":"H17*I17","v":{"v":5.4,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":72.5,"d":"€73"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":13.775,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":86.275,"d":"€86"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585RR03","BERLINER STRAßE","1,80","1,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,80","BAJ","A","30,00","12 - 12","JA","Verschobene Verbindung in längsrichtung ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,20","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,20","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["1,60","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,80","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,80","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.8,2,{"$f":"H40*I40","v":{"v":3.6,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.8,3,{"$f":"H41*I41","v":{"v":5.4,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":72.5,"d":"€73"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":13.775,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":86.275,"d":"€86"}}]

{"sheet":"09340585RR07","index":78,"n_rows":48,"n_cols":10,"rows_kept":48}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585RR07","BERLINER STRAßE","2,30","2,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","BAC","A","50,00","12 - 12","JA","Rohrbruch / Einsturz Bruch "]
["1,60","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,60","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["1,60","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,90","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,10","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,20","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J13)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H15/100)*J14","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H16/100)*J14","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H17/100)*J14","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.3,2,{"$f":"H18*I18","v":{"v":4.6,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.3,3,{"$f":"H19*I19","v":{"v":6.8999999999999995,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J14:J19)","v":{"v":11.5,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H21/100)*J20","v":{"v":2.185,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J20:J21)","v":{"v":13.685,"d":"€14"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340585RR07","BERLINER STRAßE","2,30","2,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","BAC","A","50,00","12 - 12","JA","Rohrbruch / Einsturz Bruch "]
["1,60","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,60","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["1,60","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,90","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,10","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,20","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J31:J39)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.3,2,{"$f":"H44*I44","v":{"v":4.6,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.3,3,{"$f":"H45*I45","v":{"v":6.8999999999999995,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":11.5,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":2.185,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":13.685,"d":"€14"}}]

{"sheet":"09340611RS03","index":79,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340611RS03","BERLINER STRAßE","6,40","7,30","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,10","BCC","A / Y","15,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["4,10","BCC","A / Y","15,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["6,40","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.4,2,{"$f":"H13*I13","v":{"v":12.8,"d":"€13"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.4,3,{"$f":"H14*I14","v":{"v":19.200000000000003,"d":"€19"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":32,"d":"€32"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":6.08,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":38.08,"d":"€38"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340611RS03","BERLINER STRAßE","6,40","7,30","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,10","BCC","A / Y","15,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["4,10","BCC","A / Y","15,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["6,40","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.4,2,{"$f":"H34*I34","v":{"v":12.8,"d":"€13"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.4,3,{"$f":"H35*I35","v":{"v":19.200000000000003,"d":"€19"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":32,"d":"€32"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":6.08,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":38.08,"d":"€38"}}]

{"sheet":"09340611SE02","index":80,"n_rows":50,"n_cols":10,"rows_kept":50}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340611SE02","BERLINER STRAßE","3,20","3,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","A / Y","30,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["0,20","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["1,10","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["1,40","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["2,10","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["2,20","BBE","C","40,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["2,90","BCC","A / A","30,00","10",null,"Krümmung der Leitung nach links nach oben"]
["3,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J14)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H16/100)*J15","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H17/100)*J15","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H18/100)*J15","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H19*I19","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H20*I20","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J15:J20)","v":{"v":16,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H22/100)*J21","v":{"v":3.04,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J21:J22)","v":{"v":19.04,"d":"€19"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09340611SE02","BERLINER STRAßE","3,20","3,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","A / Y","30,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["0,20","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["1,10","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["1,40","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["2,10","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["2,20","BBE","C","40,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["2,90","BCC","A / A","30,00","10",null,"Krümmung der Leitung nach links nach oben"]
["3,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J32:J41)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H43/100)*J42","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H44/100)*J42","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H45/100)*J42","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H46*I46","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H47*I47","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J42:J47)","v":{"v":16,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H49/100)*J48","v":{"v":3.04,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J48:J49)","v":{"v":19.04,"d":"€19"}}]

{"sheet":"09342380GA01","index":81,"n_rows":108,"n_cols":10,"rows_kept":108}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA01","LEIPZIGER STRAßE","49,40","49,90","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCA","C / A","200,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["4,90","BCA","A / A","100,00","3",null,"Anschluss Abzweig offen"]
["5,60","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["7,50","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["11,80","BCA","A / A","100,00","3",null,"Anschluss Abzweig offen"]
["12,40","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["12,60","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["14,30","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["18,70","BCA","A / A","100,00","3",null,"Anschluss Abzweig offen"]
["19,20","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["21,20","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["22,80","BDD","C","10,00",null,null,"Wasserspiegel trüb ","A"]
["22,80","BAB","A / A",null,"10 - 12",null,"Rissbildung Oberflächenriss (Haarriss) in Längsrichtung","A"]
["22,90","BAB","A / A",null,"10 - 12",null,"Rissbildung Oberflächenriss (Haarriss) in Längsrichtung","B"]
["24,80","BCA","A / A","100,00","3",null,"Anschluss Abzweig offen"]
["25,40","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["25,40","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["25,40","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["25,90","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["27,60","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["27,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["28,10","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["30,30","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["32,30","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen"]
["32,80","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["35,00","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["38,60","BCA","A / A","100,00","3",null,"Anschluss Abzweig offen"]
["39,20","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["41,50","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["45,00","BCA","A / A","100,00","3",null,"Anschluss Abzweig offen"]
["45,50","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["47,60","BBC","C","10,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["47,80","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["48,00","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["48,40","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["49,30","BBC","C","10,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["49,30","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["49,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J43)","v":{"v":200,"d":"€200"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H45/100)*J44","v":{"v":20,"d":"€20"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H46/100)*J44","v":{"v":10,"d":"€10"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H47/100)*J44","v":{"v":24,"d":"€24"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",49.4,2,{"$f":"H48*I48","v":{"v":98.8,"d":"€99"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",49.4,3,{"$f":"H49*I49","v":{"v":148.2,"d":"€148"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J44:J49)","v":{"v":501,"d":"€501"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H51/100)*J50","v":{"v":95.19,"d":"€95"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J50:J51)","v":{"v":596.19,"d":"€596"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA01","LEIPZIGER STRAßE","49,40","49,90","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCA","C / A","200,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["4,90","BCA","A / A","100,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["5,60","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["7,50","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["11,80","BCA","A / A","100,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["12,40","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["12,60","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["14,30","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["18,70","BCA","A / A","100,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["19,20","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["21,20","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["22,80","BDD","C","10,00",null,null,"Wasserspiegel trüb ","A"]
["22,80","BAB","A / A",null,"10 - 12",null,"Rissbildung Oberflächenriss (Haarriss) in Längsrichtung","A"]
["22,90","BAB","A / A",null,"10 - 12",null,"Rissbildung Oberflächenriss (Haarriss) in Längsrichtung","B"]
["24,80","BCA","A / A","100,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["25,40","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["25,40","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["25,40","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["25,90","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["27,60","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["27,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["28,10","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["30,30","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["32,30","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["32,80","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["35,00","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["38,60","BCA","A / A","100,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["39,20","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["41,50","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["45,00","BCA","A / A","100,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["45,50","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["47,60","BBC","C","10,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["47,80","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["48,00","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["48,40","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["49,30","BBC","C","10,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["49,30","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["49,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J61:J99)","v":{"v":10490,"d":"€10,490"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H101/100)*J100","v":{"v":1049,"d":"€1,049"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H102/100)*J100","v":{"v":524.5,"d":"€525"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H103/100)*J100","v":{"v":1258.8,"d":"€1,259"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",49.4,2,{"$f":"H104*I104","v":{"v":98.8,"d":"€99"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",49.4,3,{"$f":"H105*I105","v":{"v":148.2,"d":"€148"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J100:J105)","v":{"v":13569.3,"d":"€13,569"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H107/100)*J106","v":{"v":2578.167,"d":"€2,578"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J106:J107)","v":{"v":16147.466999999999,"d":"€16,147"}}]

{"sheet":"09342380GA03","index":82,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA03","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H12*I12","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H13*I13","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":5.95,"d":"€6"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA03","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H32*I32","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H33*I33","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":5.95,"d":"€6"}}]

{"sheet":"09342380GA04","index":83,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA04","LEIPZIGER STRAßE","2,60","2,60","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,20","BAJ","B","10,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.6,2,{"$f":"H13*I13","v":{"v":5.2,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.6,3,{"$f":"H14*I14","v":{"v":7.800000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":76.5,"d":"€77"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":14.535,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":91.035,"d":"€91"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA04","LEIPZIGER STRAßE","2,60","2,60","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,20","BAJ","B","10,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.6,2,{"$f":"H34*I34","v":{"v":5.2,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.6,3,{"$f":"H35*I35","v":{"v":7.800000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":76.5,"d":"€77"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":14.535,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":91.035,"d":"€91"}}]

{"sheet":"09342380GA05","index":84,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA05","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H12*I12","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H13*I13","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":17.255,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA05","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H32*I32","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H33*I33","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":17.255,"d":"€17"}}]

{"sheet":"09342380GA06","index":85,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA06","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H12*I12","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H13*I13","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":5.95,"d":"€6"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA06","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H32*I32","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H33*I33","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":5.95,"d":"€6"}}]

{"sheet":"09342380GA07","index":86,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA07","LEIPZIGER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H12*I12","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H13*I13","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":12.5,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.375,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":14.875,"d":"€15"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA07","LEIPZIGER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H32*I32","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H33*I33","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":12.5,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.375,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":14.875,"d":"€15"}}]

{"sheet":"09342380GA08","index":87,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA08","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H12*I12","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H13*I13","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":17.255,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA08","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H32*I32","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H33*I33","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":17.255,"d":"€17"}}]

{"sheet":"09342380GA09","index":88,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA09","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H12*I12","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H13*I13","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":5.95,"d":"€6"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA09","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H32*I32","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H33*I33","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":5.95,"d":"€6"}}]

{"sheet":"09342380GA10","index":89,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA10","LEIPZIGER STRAßE","2,20","2,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.2,2,{"$f":"H12*I12","v":{"v":4.4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.2,3,{"$f":"H13*I13","v":{"v":6.6000000000000005,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":11,"d":"€11"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.09,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":13.09,"d":"€13"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA10","LEIPZIGER STRAßE","2,20","2,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.2,2,{"$f":"H32*I32","v":{"v":4.4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.2,3,{"$f":"H33*I33","v":{"v":6.6000000000000005,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":11,"d":"€11"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.09,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":13.09,"d":"€13"}}]

{"sheet":"09342380GA11","index":90,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA11","LEIPZIGER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","A / Y","30,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["3,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H12*I12","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H13*I13","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":18.445,"d":"€18"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA11","LEIPZIGER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","A / Y","30,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["3,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H32*I32","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H33*I33","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":18.445,"d":"€18"}}]

{"sheet":"09342380GA12","index":91,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA12","LEIPZIGER STRAßE","1,20","1,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.2,2,{"$f":"H11*I11","v":{"v":2.4,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.2,3,{"$f":"H12*I12","v":{"v":3.5999999999999996,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":6,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":1.1400000000000001,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":7.140000000000001,"d":"€7"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA12","LEIPZIGER STRAßE","1,20","1,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.2,2,{"$f":"H30*I30","v":{"v":2.4,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.2,3,{"$f":"H31*I31","v":{"v":3.5999999999999996,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":6,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":1.1400000000000001,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":7.140000000000001,"d":"€7"}}]

{"sheet":"09342380GA13","index":92,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA13","LEIPZIGER STRAßE","2,00","2,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,00","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["2,00","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2,2,{"$f":"H14*I14","v":{"v":4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2,3,{"$f":"H15*I15","v":{"v":6,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":1.9,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":11.9,"d":"€12"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA13","LEIPZIGER STRAßE","2,00","2,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,00","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["2,00","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2,2,{"$f":"H36*I36","v":{"v":4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2,3,{"$f":"H37*I37","v":{"v":6,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":1.9,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":11.9,"d":"€12"}}]

{"sheet":"09342380GA14","index":93,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA14","LEIPZIGER STRAßE","4,10","4,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.1,2,{"$f":"H11*I11","v":{"v":8.2,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.1,3,{"$f":"H12*I12","v":{"v":12.299999999999999,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":20.5,"d":"€21"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":3.895,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":24.395,"d":"€24"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA14","LEIPZIGER STRAßE","4,10","4,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.1,2,{"$f":"H30*I30","v":{"v":8.2,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.1,3,{"$f":"H31*I31","v":{"v":12.299999999999999,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":20.5,"d":"€21"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":3.895,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":24.395,"d":"€24"}}]

{"sheet":"09342380GA15","index":94,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA15","LEIPZIGER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H11*I11","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H12*I12","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":6.545,"d":"€7"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA15","LEIPZIGER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H30*I30","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H31*I31","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":6.545,"d":"€7"}}]

{"sheet":"09342380GA17","index":95,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA17","LEIPZIGER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H12*I12","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H13*I13","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":12.5,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.375,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":14.875,"d":"€15"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA17","LEIPZIGER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H32*I32","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H33*I33","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":12.5,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.375,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":14.875,"d":"€15"}}]

{"sheet":"09342380GA18","index":96,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA18","LEIPZIGER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H11*I11","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H12*I12","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":6.545,"d":"€7"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA18","LEIPZIGER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H30*I30","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H31*I31","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":6.545,"d":"€7"}}]

{"sheet":"09342380GA20","index":97,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA20","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H12*I12","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H13*I13","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":17.255,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380GA20","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H32*I32","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H33*I33","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":17.255,"d":"€17"}}]

{"sheet":"09342380NN02","index":98,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380NN02","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380NN02","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09342380NN16","index":99,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380NN16","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380NN16","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09342380NN19","index":100,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380NN19","LEIPZIGER STRAßE","0,40","0,40","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,40","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.4,2,{"$f":"H11*I11","v":{"v":0.8,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.4,3,{"$f":"H12*I12","v":{"v":1.2000000000000002,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":2,"d":"€2"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.38,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":2.38,"d":"€2"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380NN19","LEIPZIGER STRAßE","0,40","0,40","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,40","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.4,2,{"$f":"H30*I30","v":{"v":0.8,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.4,3,{"$f":"H31*I31","v":{"v":1.2000000000000002,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":2,"d":"€2"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.38,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":2.38,"d":"€2"}}]

{"sheet":"09342380NN21","index":101,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380NN21","LEIPZIGER STRAßE","0,10","0,10","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.1,2,{"$f":"H11*I11","v":{"v":0.2,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.1,3,{"$f":"H12*I12","v":{"v":0.30000000000000004,"d":"€0"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":0.5,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.095,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":0.595,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380NN21","LEIPZIGER STRAßE","0,10","0,10","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.1,2,{"$f":"H30*I30","v":{"v":0.2,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.1,3,{"$f":"H31*I31","v":{"v":0.30000000000000004,"d":"€0"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":0.5,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.095,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":0.595,"d":"€1"}}]

{"sheet":"09342380NN22","index":102,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380NN22","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342380NN22","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09342381GA01","index":103,"n_rows":106,"n_cols":10,"rows_kept":106}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA01","LEIPZIGER STRAßE","49,30","49,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,50","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["0,50","BCA","A / A","200,00","6",null,"Anschluss Abzweig offen"]
["5,50","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["12,90","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen"]
["13,40","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["15,40","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["18,90","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen"]
["19,50","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["22,90","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["26,30","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen"]
["26,90","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["27,40","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["28,60","AED","GGG",{"$nulls":3},"Grundlagen änderung  ","A"]
["28,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["29,20","AED","STZ",{"$nulls":3},"Grundlagen änderung  ","B"]
["29,90","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["30,30","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["33,10","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen"]
["33,10","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["33,70","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["35,50","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["36,40","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["37,90","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["39,10","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen"]
["39,60","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["40,90","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["41,30","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["41,60","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["45,30","BBC","C","5,00","4 - 8","JA","Ablagerungen hartes oder verdichtetes Material ",null,"Fräsen",{"v":50,"d":"€50"}]
["45,50","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen"]
["46,00","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["48,10","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["48,40","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["48,70","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["49,20","BAC","A","80,00","2 - 5",null,"Rohrbruch / Einsturz Bruch "]
["49,30","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["49,30","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J42)","v":{"v":450,"d":"€450"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H44/100)*J43","v":{"v":45,"d":"€45"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H45/100)*J43","v":{"v":22.5,"d":"€23"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H46/100)*J43","v":{"v":54,"d":"€54"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",49.3,2,{"$f":"H47*I47","v":{"v":98.6,"d":"€99"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",49.3,3,{"$f":"H48*I48","v":{"v":147.89999999999998,"d":"€148"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J43:J48)","v":{"v":818,"d":"€818"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H50/100)*J49","v":{"v":155.42000000000002,"d":"€155"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J49:J50)","v":{"v":973.4200000000001,"d":"€973"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA01","LEIPZIGER STRAßE","49,30","49,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,50","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["0,50","BCA","A / A","200,00","6",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["5,50","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["12,90","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["13,40","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["15,40","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["18,90","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["19,50","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["22,90","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["26,30","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["26,90","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["27,40","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["28,60","AED","GGG",{"$nulls":3},"Grundlagen änderung  ","A"]
["28,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["29,20","AED","STZ",{"$nulls":3},"Grundlagen änderung  ","B"]
["29,90","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["30,30","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["33,10","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["33,10","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["33,70","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["35,50","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["36,40","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["37,90","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["39,10","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["39,60","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["40,90","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["41,30","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["41,60","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["45,30","BBC","C","5,00","4 - 8","JA","Ablagerungen hartes oder verdichtetes Material ",null,"Fräsen",{"v":50,"d":"€50"}]
["45,50","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["46,00","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["48,10","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["48,40","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["48,70","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["49,20","BAC","A","80,00","2 - 5",null,"Rohrbruch / Einsturz Bruch "]
["49,30","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["49,30","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J60:J97)","v":{"v":9270,"d":"€9,270"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H99/100)*J98","v":{"v":927,"d":"€927"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H100/100)*J98","v":{"v":463.5,"d":"€464"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H101/100)*J98","v":{"v":1112.3999999999999,"d":"€1,112"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",49.3,2,{"$f":"H102*I102","v":{"v":98.6,"d":"€99"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",49.3,3,{"$f":"H103*I103","v":{"v":147.89999999999998,"d":"€148"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J98:J103)","v":{"v":12019.4,"d":"€12,019"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H105/100)*J104","v":{"v":2283.686,"d":"€2,284"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J104:J105)","v":{"v":14303.086,"d":"€14,303"}}]

{"sheet":"09342381GA03","index":104,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA03","LEIPZIGER STRAßE","0,70","0,70","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.7,2,{"$f":"H12*I12","v":{"v":1.4,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.7,3,{"$f":"H13*I13","v":{"v":2.0999999999999996,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":3.4999999999999996,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.6649999999999999,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":4.164999999999999,"d":"€4"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA03","LEIPZIGER STRAßE","0,70","0,70","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.7,2,{"$f":"H32*I32","v":{"v":1.4,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.7,3,{"$f":"H33*I33","v":{"v":2.0999999999999996,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":3.4999999999999996,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.6649999999999999,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":4.164999999999999,"d":"€4"}}]

{"sheet":"09342381GA04","index":105,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA04","LEIPZIGER STRAßE","2,60","2,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.6,2,{"$f":"H12*I12","v":{"v":5.2,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.6,3,{"$f":"H13*I13","v":{"v":7.800000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":13,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.47,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":15.47,"d":"€15"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA04","LEIPZIGER STRAßE","2,60","2,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.6,2,{"$f":"H32*I32","v":{"v":5.2,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.6,3,{"$f":"H33*I33","v":{"v":7.800000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":13,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.47,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":15.47,"d":"€15"}}]

{"sheet":"09342381GA05","index":106,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA05","LEIPZIGER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAJ","B","10,00","11","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["3,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H13*I13","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H14*I14","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":79.5,"d":"€80"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":15.105,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":94.605,"d":"€95"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA05","LEIPZIGER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAJ","B","10,00","11","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["3,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H34*I34","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H35*I35","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":79.5,"d":"€80"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":15.105,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":94.605,"d":"€95"}}]

{"sheet":"09342381GA06","index":107,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA06","LEIPZIGER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H12*I12","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H13*I13","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":6.545,"d":"€7"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA06","LEIPZIGER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H32*I32","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H33*I33","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":6.545,"d":"€7"}}]

{"sheet":"09342381GA07","index":108,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA07","LEIPZIGER STRAßE","2,60","2,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.6,2,{"$f":"H12*I12","v":{"v":5.2,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.6,3,{"$f":"H13*I13","v":{"v":7.800000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":13,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.47,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":15.47,"d":"€15"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA07","LEIPZIGER STRAßE","2,60","2,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.6,2,{"$f":"H32*I32","v":{"v":5.2,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.6,3,{"$f":"H33*I33","v":{"v":7.800000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":13,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.47,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":15.47,"d":"€15"}}]

{"sheet":"09342381GA08","index":109,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA08","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H12*I12","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H13*I13","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":17.255,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA08","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H32*I32","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H33*I33","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":17.255,"d":"€17"}}]

{"sheet":"09342381GA09","index":110,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA09","LEIPZIGER STRAßE","0,80","0,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","30,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.8,2,{"$f":"H12*I12","v":{"v":1.6,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.8,3,{"$f":"H13*I13","v":{"v":2.4000000000000004,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":4,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.76,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":4.76,"d":"€5"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA09","LEIPZIGER STRAßE","0,80","0,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","30,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.8,2,{"$f":"H32*I32","v":{"v":1.6,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.8,3,{"$f":"H33*I33","v":{"v":2.4000000000000004,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":4,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.76,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":4.76,"d":"€5"}}]

{"sheet":"09342381GA10","index":111,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA10","LEIPZIGER STRAßE","2,20","2,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,40","BAJ","A","20,00","12 - 12","JA","Verschobene Verbindung in längsrichtung ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.2,2,{"$f":"H13*I13","v":{"v":4.4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.2,3,{"$f":"H14*I14","v":{"v":6.6000000000000005,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":74.5,"d":"€75"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":14.155,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":88.655,"d":"€89"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA10","LEIPZIGER STRAßE","2,20","2,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,40","BAJ","A","20,00","12 - 12","JA","Verschobene Verbindung in längsrichtung ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.2,2,{"$f":"H34*I34","v":{"v":4.4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.2,3,{"$f":"H35*I35","v":{"v":6.6000000000000005,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":74.5,"d":"€75"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":14.155,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":88.655,"d":"€89"}}]

{"sheet":"09342381GA11","index":112,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA11","LEIPZIGER STRAßE","3,70","3,70","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["3,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.7,2,{"$f":"H11*I11","v":{"v":7.4,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.7,3,{"$f":"H12*I12","v":{"v":11.100000000000001,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":18.5,"d":"€19"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":3.515,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":22.015,"d":"€22"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA11","LEIPZIGER STRAßE","3,70","3,70","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["3,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.7,2,{"$f":"H30*I30","v":{"v":7.4,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.7,3,{"$f":"H31*I31","v":{"v":11.100000000000001,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":18.5,"d":"€19"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":3.515,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":22.015,"d":"€22"}}]

{"sheet":"09342381GA12","index":113,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA12","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H12*I12","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H13*I13","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":5.355,"d":"€5"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA12","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H32*I32","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H33*I33","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":5.355,"d":"€5"}}]

{"sheet":"09342381GA13","index":114,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA13","LEIPZIGER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H12*I12","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H13*I13","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":12.5,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.375,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":14.875,"d":"€15"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA13","LEIPZIGER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H32*I32","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H33*I33","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":12.5,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.375,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":14.875,"d":"€15"}}]

{"sheet":"09342381GA14","index":115,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA14","LEIPZIGER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["3,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H12*I12","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H13*I13","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":16,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":3.04,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":19.04,"d":"€19"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA14","LEIPZIGER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["3,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H32*I32","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H33*I33","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":16,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":3.04,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":19.04,"d":"€19"}}]

{"sheet":"09342381GA15","index":116,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA15","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H12*I12","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H13*I13","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":5.95,"d":"€6"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA15","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H32*I32","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H33*I33","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":5.95,"d":"€6"}}]

{"sheet":"09342381GA16","index":117,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA16","LEIPZIGER STRAßE","2,60","2,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAF","A / E",null,"1 - 3",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.6,2,{"$f":"H13*I13","v":{"v":5.2,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.6,3,{"$f":"H14*I14","v":{"v":7.800000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":13,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":2.47,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":15.47,"d":"€15"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA16","LEIPZIGER STRAßE","2,60","2,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAF","A / E",null,"1 - 3",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.6,2,{"$f":"H34*I34","v":{"v":5.2,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.6,3,{"$f":"H35*I35","v":{"v":7.800000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":13,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":2.47,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":15.47,"d":"€15"}}]

{"sheet":"09342381GA17","index":118,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA17","LEIPZIGER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,40","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["1,50","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,80","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["3,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H14*I14","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H15*I15","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":143,"d":"€143"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":27.17,"d":"€27"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":170.17000000000002,"d":"€170"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA17","LEIPZIGER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,40","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["1,50","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,80","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["3,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H36*I36","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H37*I37","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":143,"d":"€143"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":27.17,"d":"€27"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":170.17000000000002,"d":"€170"}}]

{"sheet":"09342381GA18","index":119,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA18","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H11*I11","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H12*I12","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":5.355,"d":"€5"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA18","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H30*I30","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H31*I31","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":5.355,"d":"€5"}}]

{"sheet":"09342381GA19","index":120,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA19","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,50","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H12*I12","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H13*I13","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":17.255,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381GA19","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,50","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H32*I32","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H33*I33","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":17.255,"d":"€17"}}]

{"sheet":"09342381RS20","index":121,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381RS20","LEIPZIGER STRAßE","4,90","5,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCA","A / A","150,00","6",null,"Anschluss Abzweig offen"]
["4,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.9,2,{"$f":"H12*I12","v":{"v":9.8,"d":"€10"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.9,3,{"$f":"H13*I13","v":{"v":14.700000000000001,"d":"€15"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":24.5,"d":"€25"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":4.655,"d":"€5"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":29.155,"d":"€29"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342381RS20","LEIPZIGER STRAßE","4,90","5,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCA","A / A","150,00","6",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["4,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":490,"d":"€490"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":49,"d":"€49"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":24.5,"d":"€25"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":58.8,"d":"€59"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.9,2,{"$f":"H32*I32","v":{"v":9.8,"d":"€10"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.9,3,{"$f":"H33*I33","v":{"v":14.700000000000001,"d":"€15"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":646.8,"d":"€647"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":122.892,"d":"€123"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":769.692,"d":"€770"}}]

{"sheet":"09342382GA01","index":122,"n_rows":122,"n_cols":10,"rows_kept":122}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA01","LEIPZIGER STRAßE","50,40","50,90","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["0,50","BCA","A / A","200,00","6",null,"Anschluss Abzweig offen"]
["2,10","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["12,20","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen"]
["12,80","BCA","A / A","150,00","2",null,"Anschluss Abzweig offen"]
["13,30","BCA","A / A","150,00","11",null,"Anschluss Abzweig offen"]
["13,70","BBC","C","5,00","2 - 10",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["15,30","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["16,70","BBC","C","5,00","2 - 10",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["19,40","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen"]
["19,80","BBC","C","2,00","5 - 7",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["19,90","BCA","A / A","150,00","2",null,"Anschluss Abzweig offen"]
["20,50","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["22,10","BBC","C","10,00","5 - 7",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["22,50","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["25,90","BAF","A / E",null,"3 - 9",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["26,10","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["26,70","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen"]
["27,10","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["27,60","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["29,00","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["29,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["29,50","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["29,50","BBC","C",null,"5 - 7",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["31,00","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["32,20","BBC","C","8,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["33,00","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen"]
["33,50","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen"]
["34,00","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["35,80","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["36,70","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["39,70","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen"]
["40,20","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen"]
["40,70","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["42,40","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["46,20","BBC","C","10,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["46,40","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen"]
["46,90","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen"]
["47,50","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["48,90","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["49,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["49,50","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["50,40","BBC","C","10,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["50,40","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["50,40","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J50)","v":{"v":550,"d":"€550"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H52/100)*J51","v":{"v":55,"d":"€55"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H53/100)*J51","v":{"v":27.5,"d":"€28"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H54/100)*J51","v":{"v":66,"d":"€66"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",50.4,2,{"$f":"H55*I55","v":{"v":100.8,"d":"€101"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",50.4,3,{"$f":"H56*I56","v":{"v":151.2,"d":"€151"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J51:J56)","v":{"v":950.5,"d":"€951"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H58/100)*J57","v":{"v":180.595,"d":"€181"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J57:J58)","v":{"v":1131.095,"d":"€1,131"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA01","LEIPZIGER STRAßE","50,40","50,90","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["0,50","BCA","A / A","200,00","6",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["2,10","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["12,20","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["12,80","BCA","A / A","150,00","2",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["13,30","BCA","A / A","150,00","11",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["13,70","BBC","C","5,00","2 - 10",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["15,30","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["16,70","BBC","C","5,00","2 - 10",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["19,40","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["19,80","BBC","C","2,00","5 - 7",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["19,90","BCA","A / A","150,00","2",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["20,50","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["22,10","BBC","C","10,00","5 - 7",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["22,50","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["25,90","BAF","A / E",null,"3 - 9",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["26,10","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["26,70","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["27,10","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["27,60","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["29,00","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["29,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["29,50","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["29,50","BBC","C",null,"5 - 7",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["31,00","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["32,20","BBC","C","8,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["33,00","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["33,50","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["34,00","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["35,80","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["36,70","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["39,70","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["40,20","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["40,70","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["42,40","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["46,20","BBC","C","10,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["46,40","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["46,90","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["47,50","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["48,90","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["49,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["49,50","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["50,40","BBC","C","10,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["50,40","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["50,40","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J68:J113)","v":{"v":12310,"d":"€12,310"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H115/100)*J114","v":{"v":1231,"d":"€1,231"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H116/100)*J114","v":{"v":615.5,"d":"€616"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H117/100)*J114","v":{"v":1477.2,"d":"€1,477"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",50.4,2,{"$f":"H118*I118","v":{"v":100.8,"d":"€101"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",50.4,3,{"$f":"H119*I119","v":{"v":151.2,"d":"€151"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J114:J119)","v":{"v":15885.7,"d":"€15,886"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H121/100)*J120","v":{"v":3018.2830000000004,"d":"€3,018"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J120:J121)","v":{"v":18903.983,"d":"€18,904"}}]

{"sheet":"09342382GA04","index":123,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA04","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / B","45,00","4",null,"Krümmung der Leitung nach rechts nach unten"]
["0,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H12*I12","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H13*I13","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":5.355,"d":"€5"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA04","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / B","45,00","4",null,"Krümmung der Leitung nach rechts nach unten"]
["0,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H32*I32","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H33*I33","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":5.355,"d":"€5"}}]

{"sheet":"09342382GA05","index":124,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA05","LEIPZIGER STRAßE","2,60","2,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAC","A","150,00","5 - 10",null,"Rohrbruch / Einsturz Bruch "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,60","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["2,50","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["2,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.6,2,{"$f":"H15*I15","v":{"v":5.2,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.6,3,{"$f":"H16*I16","v":{"v":7.800000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":13,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":2.47,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":15.47,"d":"€15"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA05","LEIPZIGER STRAßE","2,60","2,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAC","A","150,00","5 - 10",null,"Rohrbruch / Einsturz Bruch "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,60","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["2,50","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["2,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.6,2,{"$f":"H38*I38","v":{"v":5.2,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.6,3,{"$f":"H39*I39","v":{"v":7.800000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":13,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":2.47,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":15.47,"d":"€15"}}]

{"sheet":"09342382GA06","index":125,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA06","LEIPZIGER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["3,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H12*I12","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H13*I13","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":18.445,"d":"€18"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA06","LEIPZIGER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["3,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H32*I32","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H33*I33","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":18.445,"d":"€18"}}]

{"sheet":"09342382GA08","index":126,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA08","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,50","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H13*I13","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H14*I14","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":68,"d":"€68"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":12.92,"d":"€13"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":80.92,"d":"€81"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA08","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,50","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H34*I34","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H35*I35","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":68,"d":"€68"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":12.92,"d":"€13"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":80.92,"d":"€81"}}]

{"sheet":"09342382GA09","index":127,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA09","LEIPZIGER STRAßE","2,00","2,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,70","BBE","C","60,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["2,00","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2,2,{"$f":"H13*I13","v":{"v":4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2,3,{"$f":"H14*I14","v":{"v":6,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":1.9,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":11.9,"d":"€12"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA09","LEIPZIGER STRAßE","2,00","2,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,70","BBE","C","60,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["2,00","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2,2,{"$f":"H34*I34","v":{"v":4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2,3,{"$f":"H35*I35","v":{"v":6,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":1.9,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":11.9,"d":"€12"}}]

{"sheet":"09342382GA10","index":128,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA10","LEIPZIGER STRAßE","3,00","3,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["3,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3,2,{"$f":"H12*I12","v":{"v":6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3,3,{"$f":"H13*I13","v":{"v":9,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.85,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":17.85,"d":"€18"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA10","LEIPZIGER STRAßE","3,00","3,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["3,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3,2,{"$f":"H32*I32","v":{"v":6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3,3,{"$f":"H33*I33","v":{"v":9,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.85,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":17.85,"d":"€18"}}]

{"sheet":"09342382GA12","index":129,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA12","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H12*I12","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H13*I13","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":5.95,"d":"€6"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA12","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H32*I32","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H33*I33","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":5.95,"d":"€6"}}]

{"sheet":"09342382GA13","index":130,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA13","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,10","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,40","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H12*I12","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H13*I13","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":16.065,"d":"€16"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA13","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,10","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,40","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H32*I32","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H33*I33","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":16.065,"d":"€16"}}]

{"sheet":"09342382GA14","index":131,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA14","LEIPZIGER STRAßE","3,40","3,40","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["3,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.4,2,{"$f":"H11*I11","v":{"v":6.8,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.4,3,{"$f":"H12*I12","v":{"v":10.2,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":17,"d":"€17"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":3.23,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":20.23,"d":"€20"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA14","LEIPZIGER STRAßE","3,40","3,40","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["3,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.4,2,{"$f":"H30*I30","v":{"v":6.8,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.4,3,{"$f":"H31*I31","v":{"v":10.2,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":17,"d":"€17"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":3.23,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":20.23,"d":"€20"}}]

{"sheet":"09342382GA16","index":132,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA16","LEIPZIGER STRAßE","0,80","0,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.8,2,{"$f":"H12*I12","v":{"v":1.6,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.8,3,{"$f":"H13*I13","v":{"v":2.4000000000000004,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":4,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.76,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":4.76,"d":"€5"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA16","LEIPZIGER STRAßE","0,80","0,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.8,2,{"$f":"H32*I32","v":{"v":1.6,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.8,3,{"$f":"H33*I33","v":{"v":2.4000000000000004,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":4,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.76,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":4.76,"d":"€5"}}]

{"sheet":"09342382GA17","index":133,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA17","LEIPZIGER STRAßE","2,20","2,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,70","BBE","C","60,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["2,20","BBE","C","60,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["2,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.2,2,{"$f":"H14*I14","v":{"v":4.4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.2,3,{"$f":"H15*I15","v":{"v":6.6000000000000005,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":11,"d":"€11"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":2.09,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":13.09,"d":"€13"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA17","LEIPZIGER STRAßE","2,20","2,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,70","BBE","C","60,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["2,20","BBE","C","60,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["2,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.2,2,{"$f":"H36*I36","v":{"v":4.4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.2,3,{"$f":"H37*I37","v":{"v":6.6000000000000005,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":11,"d":"€11"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":2.09,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":13.09,"d":"€13"}}]

{"sheet":"09342382GA18","index":134,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA18","LEIPZIGER STRAßE","3,00","3,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["3,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3,2,{"$f":"H12*I12","v":{"v":6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3,3,{"$f":"H13*I13","v":{"v":9,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.85,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":17.85,"d":"€18"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA18","LEIPZIGER STRAßE","3,00","3,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["3,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3,2,{"$f":"H32*I32","v":{"v":6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3,3,{"$f":"H33*I33","v":{"v":9,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.85,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":17.85,"d":"€18"}}]

{"sheet":"09342382GA20","index":135,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA20","LEIPZIGER STRAßE","0,80","0,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.8,2,{"$f":"H12*I12","v":{"v":1.6,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.8,3,{"$f":"H13*I13","v":{"v":2.4000000000000004,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":4,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.76,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":4.76,"d":"€5"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA20","LEIPZIGER STRAßE","0,80","0,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.8,2,{"$f":"H32*I32","v":{"v":1.6,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.8,3,{"$f":"H33*I33","v":{"v":2.4000000000000004,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":4,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.76,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":4.76,"d":"€5"}}]

{"sheet":"09342382GA21","index":136,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA21","LEIPZIGER STRAßE","2,60","2,60","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.6,2,{"$f":"H12*I12","v":{"v":5.2,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.6,3,{"$f":"H13*I13","v":{"v":7.800000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":13,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.47,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":15.47,"d":"€15"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA21","LEIPZIGER STRAßE","2,60","2,60","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.6,2,{"$f":"H32*I32","v":{"v":5.2,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.6,3,{"$f":"H33*I33","v":{"v":7.800000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":13,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.47,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":15.47,"d":"€15"}}]

{"sheet":"09342382GA22","index":137,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA22","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H12*I12","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H13*I13","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":17.255,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA22","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H32*I32","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H33*I33","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":17.255,"d":"€17"}}]

{"sheet":"09342382GA24","index":138,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA24","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H12*I12","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H13*I13","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":5.355,"d":"€5"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA24","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H32*I32","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H33*I33","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":5.355,"d":"€5"}}]

{"sheet":"09342382GA25","index":139,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA25","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H12*I12","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H13*I13","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":16.065,"d":"€16"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382GA25","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H32*I32","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H33*I33","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":16.065,"d":"€16"}}]

{"sheet":"09342382NN15","index":140,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382NN15","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382NN15","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09342382NN19","index":141,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382NN19","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382NN19","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09342382NN23","index":142,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382NN23","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382NN23","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09342382RV03","index":143,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382RV03","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H12*I12","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H13*I13","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":5.355,"d":"€5"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382RV03","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H32*I32","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H33*I33","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":5.355,"d":"€5"}}]

{"sheet":"09342382RV07","index":144,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382RV07","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,50","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,80","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["0,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H14*I14","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H15*I15","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":5.355,"d":"€5"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382RV07","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,50","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,80","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["0,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H36*I36","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H37*I37","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":5.355,"d":"€5"}}]

{"sheet":"09342382RV11","index":145,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382RV11","LEIPZIGER STRAßE","0,70","0,70","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,70","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.7,2,{"$f":"H12*I12","v":{"v":1.4,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.7,3,{"$f":"H13*I13","v":{"v":2.0999999999999996,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":3.4999999999999996,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.6649999999999999,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":4.164999999999999,"d":"€4"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342382RV11","LEIPZIGER STRAßE","0,70","0,70","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,70","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.7,2,{"$f":"H32*I32","v":{"v":1.4,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.7,3,{"$f":"H33*I33","v":{"v":2.0999999999999996,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":3.4999999999999996,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.6649999999999999,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":4.164999999999999,"d":"€4"}}]

{"sheet":"09342383GA01","index":146,"n_rows":124,"n_cols":10,"rows_kept":124}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA01","LEIPZIGER STRAßE","49,90","50,40","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["0,50","BCA","A / A","200,00","6",null,"Anschluss Abzweig offen"]
["2,30","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,50","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["9,50","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["12,60","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["13,10","BCA","A / A","100,00","2",null,"Anschluss Abzweig offen"]
["13,60","BCA","A / A","100,00","10",null,"Anschluss Abzweig offen"]
["15,70","BCA","A / A","100,00","10",null,"Anschluss Abzweig offen"]
["19,50","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["20,00","BCA","A / A","100,00","2",null,"Anschluss Abzweig offen"]
["20,50","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["22,50","BCA","A / A","100,00","10",null,"Anschluss Abzweig offen"]
["26,50","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen"]
["27,00","BCA","A / A","100,00","3",null,"Anschluss Abzweig offen"]
["27,50","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["28,00","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["28,00","BBC","C","10,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["28,30","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["29,30","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["29,60","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["32,70","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","A"]
["32,90","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen"]
["33,50","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen"]
["33,90","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["35,40","BBC","C","2,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["35,40","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","B"]
["35,70","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["38,20","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","A"]
["39,40","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen"]
["39,90","BBC","C","10,00","4 - 6",null,"Ablagerungen hartes oder verdichtetes Material ",null,"Fräsen",{"v":50,"d":"€50"}]
["40,00","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen"]
["40,40","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["41,80","BBC","C","2,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["42,10","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["42,40","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","B"]
["46,00","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","A"]
["46,30","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen"]
["46,80","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen"]
["47,40","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["48,30","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","B"]
["48,40","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["48,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["48,90","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["49,80","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["49,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J51)","v":{"v":400,"d":"€400"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H53/100)*J52","v":{"v":40,"d":"€40"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H54/100)*J52","v":{"v":20,"d":"€20"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H55/100)*J52","v":{"v":48,"d":"€48"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",49.9,2,{"$f":"H56*I56","v":{"v":99.8,"d":"€100"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",49.9,3,{"$f":"H57*I57","v":{"v":149.7,"d":"€150"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J52:J57)","v":{"v":757.5,"d":"€758"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H59/100)*J58","v":{"v":143.925,"d":"€144"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J58:J59)","v":{"v":901.425,"d":"€901"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA01","LEIPZIGER STRAßE","49,90","50,40","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["0,50","BCA","A / A","200,00","6",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["2,30","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,50","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["9,50","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["12,60","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["13,10","BCA","A / A","100,00","2",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["13,60","BCA","A / A","100,00","10",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["15,70","BCA","A / A","100,00","10",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["19,50","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["20,00","BCA","A / A","100,00","2",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["20,50","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["22,50","BCA","A / A","100,00","10",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["26,50","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["27,00","BCA","A / A","100,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["27,50","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["28,00","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["28,00","BBC","C","10,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["28,30","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["29,30","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["29,60","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["32,70","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","A"]
["32,90","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["33,50","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["33,90","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["35,40","BBC","C","2,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["35,40","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","B"]
["35,70","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["38,20","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","A"]
["39,40","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["39,90","BBC","C","10,00","4 - 6",null,"Ablagerungen hartes oder verdichtetes Material ",null,"Fräsen",{"v":50,"d":"€50"}]
["40,00","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["40,40","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["41,80","BBC","C","2,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["42,10","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["42,40","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","B"]
["46,00","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","A"]
["46,30","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["46,80","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["47,40","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["48,30","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","B"]
["48,40","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["48,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["48,90","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["49,80","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["49,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J69:J115)","v":{"v":12160,"d":"€12,160"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H117/100)*J116","v":{"v":1216,"d":"€1,216"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H118/100)*J116","v":{"v":608,"d":"€608"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H119/100)*J116","v":{"v":1459.2,"d":"€1,459"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",49.9,2,{"$f":"H120*I120","v":{"v":99.8,"d":"€100"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",49.9,3,{"$f":"H121*I121","v":{"v":149.7,"d":"€150"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J116:J121)","v":{"v":15692.7,"d":"€15,693"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H123/100)*J122","v":{"v":2981.6130000000003,"d":"€2,982"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J122:J123)","v":{"v":18674.313000000002,"d":"€18,674"}}]

{"sheet":"09342383GA04","index":147,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA04","LEIPZIGER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H12*I12","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H13*I13","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":6.545,"d":"€7"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA04","LEIPZIGER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H32*I32","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H33*I33","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":6.545,"d":"€7"}}]

{"sheet":"09342383GA05","index":148,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA05","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAJ","B","15,00","11","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,40","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H13*I13","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H14*I14","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":77,"d":"€77"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":14.63,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":91.63,"d":"€92"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA05","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAJ","B","15,00","11","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,40","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H34*I34","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H35*I35","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":77,"d":"€77"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":14.63,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":91.63,"d":"€92"}}]

{"sheet":"09342383GA06","index":149,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA06","LEIPZIGER STRAßE","2,80","2,80","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.8,2,{"$f":"H12*I12","v":{"v":5.6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.8,3,{"$f":"H13*I13","v":{"v":8.399999999999999,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":13.999999999999998,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.6599999999999997,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":16.659999999999997,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA06","LEIPZIGER STRAßE","2,80","2,80","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.8,2,{"$f":"H32*I32","v":{"v":5.6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.8,3,{"$f":"H33*I33","v":{"v":8.399999999999999,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":13.999999999999998,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.6599999999999997,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":16.659999999999997,"d":"€17"}}]

{"sheet":"09342383GA08","index":150,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA08","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H12*I12","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H13*I13","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":5.95,"d":"€6"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA08","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H32*I32","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H33*I33","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":5.95,"d":"€6"}}]

{"sheet":"09342383GA09","index":151,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA09","LEIPZIGER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,10","BAB","B / C","1,00","12 - 12",null,"Rissbildung Riss komplexe Rissbildung"]
["2,20","BBE","B","20,00","4 - 8",null,"Andere Hindernisse Bruchstücke einer Abwasserleitung oder eines Abwasserkanals liegen in der \r\nRohrsohle "]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H14*I14","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H15*I15","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":12.5,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":2.375,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":14.875,"d":"€15"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA09","LEIPZIGER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,10","BAB","B / C","1,00","12 - 12",null,"Rissbildung Riss komplexe Rissbildung"]
["2,20","BBE","B","20,00","4 - 8",null,"Andere Hindernisse Bruchstücke einer Abwasserleitung oder eines Abwasserkanals liegen in der \r\nRohrsohle "]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H36*I36","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H37*I37","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":12.5,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":2.375,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":14.875,"d":"€15"}}]

{"sheet":"09342383GA10","index":152,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA10","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H12*I12","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H13*I13","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":16.065,"d":"€16"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA10","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H32*I32","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H33*I33","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":16.065,"d":"€16"}}]

{"sheet":"09342383GA12","index":153,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA12","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H12*I12","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H13*I13","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":5.355,"d":"€5"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA12","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H32*I32","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H33*I33","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":5.355,"d":"€5"}}]

{"sheet":"09342383GA13","index":154,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA13","LEIPZIGER STRAßE","2,00","2,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,90","BBE","C","70,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["2,00","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2,2,{"$f":"H13*I13","v":{"v":4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2,3,{"$f":"H14*I14","v":{"v":6,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":1.9,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":11.9,"d":"€12"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA13","LEIPZIGER STRAßE","2,00","2,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,90","BBE","C","70,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["2,00","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2,2,{"$f":"H34*I34","v":{"v":4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2,3,{"$f":"H35*I35","v":{"v":6,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":1.9,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":11.9,"d":"€12"}}]

{"sheet":"09342383GA14","index":155,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA14","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H12*I12","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H13*I13","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":17.255,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA14","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H32*I32","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H33*I33","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":17.255,"d":"€17"}}]

{"sheet":"09342383GA16","index":156,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA16","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,30","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","A"]
["1,00","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","B"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H14*I14","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H15*I15","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":5.95,"d":"€6"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA16","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,30","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","A"]
["1,00","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","B"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H36*I36","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H37*I37","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":5.95,"d":"€6"}}]

{"sheet":"09342383GA17","index":157,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA17","LEIPZIGER STRAßE","2,30","2,30","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,10","BBE","C","80,00","12 - 12",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["2,30","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.3,2,{"$f":"H13*I13","v":{"v":4.6,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.3,3,{"$f":"H14*I14","v":{"v":6.8999999999999995,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":11.5,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":2.185,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":13.685,"d":"€14"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA17","LEIPZIGER STRAßE","2,30","2,30","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,10","BBE","C","80,00","12 - 12",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["2,30","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.3,2,{"$f":"H34*I34","v":{"v":4.6,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.3,3,{"$f":"H35*I35","v":{"v":6.8999999999999995,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":11.5,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":2.185,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":13.685,"d":"€14"}}]

{"sheet":"09342383GA18","index":158,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA18","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H13*I13","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H14*I14","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":17.255,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA18","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H34*I34","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H35*I35","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":17.255,"d":"€17"}}]

{"sheet":"09342383GA20","index":159,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA20","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H12*I12","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H13*I13","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":5.355,"d":"€5"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA20","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H32*I32","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H33*I33","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":5.355,"d":"€5"}}]

{"sheet":"09342383GA21","index":160,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA21","LEIPZIGER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,10","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H13*I13","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H14*I14","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":76,"d":"€76"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":14.44,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":90.44,"d":"€90"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA21","LEIPZIGER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,10","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H34*I34","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H35*I35","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":76,"d":"€76"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":14.44,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":90.44,"d":"€90"}}]

{"sheet":"09342383GA22","index":161,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA22","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","A"]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,30","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","B"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H14*I14","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H15*I15","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":17.255,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA22","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","A"]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,30","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","B"]
["2,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H36*I36","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H37*I37","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":17.255,"d":"€17"}}]

{"sheet":"09342383GA24","index":162,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA24","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H12*I12","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H13*I13","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":5.95,"d":"€6"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA24","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H32*I32","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H33*I33","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":5.95,"d":"€6"}}]

{"sheet":"09342383GA25","index":163,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA25","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H12*I12","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H13*I13","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":16.065,"d":"€16"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383GA25","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H32*I32","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H33*I33","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":16.065,"d":"€16"}}]

{"sheet":"09342383NN07","index":164,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383NN07","LEIPZIGER STRAßE","0,80","0,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,80","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.8,2,{"$f":"H12*I12","v":{"v":1.6,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.8,3,{"$f":"H13*I13","v":{"v":2.4000000000000004,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":4,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.76,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":4.76,"d":"€5"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383NN07","LEIPZIGER STRAßE","0,80","0,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,80","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.8,2,{"$f":"H32*I32","v":{"v":1.6,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.8,3,{"$f":"H33*I33","v":{"v":2.4000000000000004,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":4,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.76,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":4.76,"d":"€5"}}]

{"sheet":"09342383NN15","index":165,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383NN15","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383NN15","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09342383NN19","index":166,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383NN19","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383NN19","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09342383NN23","index":167,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383NN23","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383NN23","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09342383RV03","index":168,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383RV03","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H12*I12","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H13*I13","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":5.355,"d":"€5"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383RV03","LEIPZIGER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H32*I32","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H33*I33","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":5.355,"d":"€5"}}]

{"sheet":"09342383RV11","index":169,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383RV11","LEIPZIGER STRAßE","0,70","0,70","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,70","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.7,2,{"$f":"H12*I12","v":{"v":1.4,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.7,3,{"$f":"H13*I13","v":{"v":2.0999999999999996,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":3.4999999999999996,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.6649999999999999,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":4.164999999999999,"d":"€4"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342383RV11","LEIPZIGER STRAßE","0,70","0,70","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,70","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.7,2,{"$f":"H32*I32","v":{"v":1.4,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.7,3,{"$f":"H33*I33","v":{"v":2.0999999999999996,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":3.4999999999999996,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.6649999999999999,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":4.164999999999999,"d":"€4"}}]

{"sheet":"09342384GA01","index":170,"n_rows":48,"n_cols":10,"rows_kept":48}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA01","BERLINER STRAßE","9,00","9,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,40","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,00","BAI","Z","10,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,60","BCC","B / A","45,00","2",null,"Krümmung der Leitung nach rechts nach oben"]
["5,20","BCC","A / B","45,00","8",null,"Krümmung der Leitung nach links nach unten"]
["6,60","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["9,00","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["9,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J13)","v":{"v":150,"d":"€150"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H15/100)*J14","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H16/100)*J14","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H17/100)*J14","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9,2,{"$f":"H18*I18","v":{"v":18,"d":"€18"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9,3,{"$f":"H19*I19","v":{"v":27,"d":"€27"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J14:J19)","v":{"v":235.5,"d":"€236"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H21/100)*J20","v":{"v":44.745,"d":"€45"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J20:J21)","v":{"v":280.245,"d":"€280"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA01","BERLINER STRAßE","9,00","9,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,40","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,00","BAI","Z","10,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart "]
["3,60","BCC","B / A","45,00","2",null,"Krümmung der Leitung nach rechts nach oben"]
["5,20","BCC","A / B","45,00","8",null,"Krümmung der Leitung nach links nach unten"]
["6,60","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["9,00","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["9,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J31:J39)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9,2,{"$f":"H44*I44","v":{"v":18,"d":"€18"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9,3,{"$f":"H45*I45","v":{"v":27,"d":"€27"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":172,"d":"€172"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":32.68,"d":"€33"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":204.68,"d":"€205"}}]

{"sheet":"09342384GA03","index":171,"n_rows":48,"n_cols":10,"rows_kept":48}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA03","BERLINER STRAßE","9,60","9,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,30","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,30","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,70","BCC","A / A","45,00","11",null,"Krümmung der Leitung nach links nach oben"]
["5,70","BAI","Z","10,00","4 - 8","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["7,10","BCC","B / B","45,00","4",null,"Krümmung der Leitung nach rechts nach unten"]
["9,60","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["9,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J13)","v":{"v":150,"d":"€150"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H15/100)*J14","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H16/100)*J14","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H17/100)*J14","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.6,2,{"$f":"H18*I18","v":{"v":19.2,"d":"€19"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.6,3,{"$f":"H19*I19","v":{"v":28.799999999999997,"d":"€29"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J14:J19)","v":{"v":238.5,"d":"€239"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H21/100)*J20","v":{"v":45.315,"d":"€45"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J20:J21)","v":{"v":283.815,"d":"€284"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA03","BERLINER STRAßE","9,60","9,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,30","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,30","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["4,70","BCC","A / A","45,00","11",null,"Krümmung der Leitung nach links nach oben"]
["5,70","BAI","Z","10,00","4 - 8","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["7,10","BCC","B / B","45,00","4",null,"Krümmung der Leitung nach rechts nach unten"]
["9,60","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["9,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J31:J39)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.6,2,{"$f":"H44*I44","v":{"v":19.2,"d":"€19"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.6,3,{"$f":"H45*I45","v":{"v":28.799999999999997,"d":"€29"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":111.5,"d":"€112"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":21.185,"d":"€21"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":132.685,"d":"€133"}}]

{"sheet":"09342384GA05","index":172,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA05","BERLINER STRAßE","9,50","9,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["4,60","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["4,70","BCC","A / A","45,00","11",null,"Krümmung der Leitung nach links nach oben"]
["7,10","BCC","B / B","45,00","4",null,"Krümmung der Leitung nach rechts nach unten"]
["9,50","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["9,50","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["9,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.5,2,{"$f":"H17*I17","v":{"v":19,"d":"€19"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.5,3,{"$f":"H18*I18","v":{"v":28.5,"d":"€29"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":174.5,"d":"€175"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":33.155,"d":"€33"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":207.655,"d":"€208"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA05","BERLINER STRAßE","9,50","9,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["4,60","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["4,70","BCC","A / A","45,00","11",null,"Krümmung der Leitung nach links nach oben"]
["7,10","BCC","B / B","45,00","4",null,"Krümmung der Leitung nach rechts nach unten"]
["9,50","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["9,50","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["9,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.5,2,{"$f":"H42*I42","v":{"v":19,"d":"€19"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.5,3,{"$f":"H43*I43","v":{"v":28.5,"d":"€29"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":174.5,"d":"€175"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":33.155,"d":"€33"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":207.655,"d":"€208"}}]

{"sheet":"09342384GA07","index":173,"n_rows":48,"n_cols":10,"rows_kept":48}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA07","BERLINER STRAßE","9,60","9,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,40","BAI","Z","20,00","2 - 10","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,50","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["4,70","BCC","A / A","45,00","10",null,"Krümmung der Leitung nach links nach oben"]
["8,90","BAC","B","100,00","10 - 2",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["9,10","BAC","A","300,00","12 - 12",null,"Rohrbruch / Einsturz Bruch "]
["9,60","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["9,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J13)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H15/100)*J14","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H16/100)*J14","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H17/100)*J14","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.6,2,{"$f":"H18*I18","v":{"v":19.2,"d":"€19"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.6,3,{"$f":"H19*I19","v":{"v":28.799999999999997,"d":"€29"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J14:J19)","v":{"v":175,"d":"€175"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H21/100)*J20","v":{"v":33.25,"d":"€33"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J20:J21)","v":{"v":208.25,"d":"€208"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA07","BERLINER STRAßE","9,60","9,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,40","BAI","Z","20,00","2 - 10","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["0,50","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["4,70","BCC","A / A","45,00","10",null,"Krümmung der Leitung nach links nach oben"]
["8,90","BAC","B","100,00","10 - 2",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["9,10","BAC","A","300,00","12 - 12",null,"Rohrbruch / Einsturz Bruch "]
["9,60","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["9,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J31:J39)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.6,2,{"$f":"H44*I44","v":{"v":19.2,"d":"€19"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.6,3,{"$f":"H45*I45","v":{"v":28.799999999999997,"d":"€29"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":111.5,"d":"€112"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":21.185,"d":"€21"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":132.685,"d":"€133"}}]

{"sheet":"09342384GA09","index":174,"n_rows":94,"n_cols":10,"rows_kept":94}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA09","LEIPZIGER STRAßE","43,70","44,20","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["3,10","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["3,60","BAI","Z","5,00","11 - 1",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A","Fräsen",{"v":50,"d":"€50"}]
["4,50","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["4,70","BAI","Z","5,00","11 - 1",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B","Fräsen",{"v":50,"d":"€50"}]
["4,90","BBC","C","2,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["5,90","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,80","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["7,00","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen"]
["12,50","BAI","A / A",null,"10 - 2","JA","Einragendes Dichtungsmaterial Dichtring sichtbar verschoben, jedoch nicht in die Rohrleitung hineinragend",null,"Fräsen",{"v":50,"d":"€50"}]
["13,60","BCA","A / A","150,00","2",null,"Anschluss Abzweig offen"]
["16,20","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen"]
["16,70","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen"]
["23,20","BCA","A / A","100,00","1",null,"Anschluss Abzweig offen"]
["23,20","BBC","C","10,00","12 - 3",null,"Ablagerungen hartes oder verdichtetes Material ",null,"Fräsen",{"v":50,"d":"€50"}]
["25,00","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["25,30","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["25,60","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["27,30","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["27,60","BCA","A / A","100,00","10",null,"Anschluss Abzweig offen"]
["29,00","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["33,00","BBC","C","10,00","5 - 9",null,"Ablagerungen hartes oder verdichtetes Material ",null,"Fräsen",{"v":50,"d":"€50"}]
["33,10","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["34,70","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen"]
["36,30","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["37,30","BBB","B","10,00","4 - 8",null,"Anhaftende Stoffe Fett ","A","Fräsen",{"v":50,"d":"€50"}]
["41,10","BBB","B","10,00","4 - 8",null,"Anhaftende Stoffe Fett ","B","Fräsen",{"v":50,"d":"€50"}]
["42,00","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["43,40","BBC","C","20,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["43,70","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["43,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["43,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J36)","v":{"v":550,"d":"€550"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H38/100)*J37","v":{"v":55,"d":"€55"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H39/100)*J37","v":{"v":27.5,"d":"€28"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H40/100)*J37","v":{"v":66,"d":"€66"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",43.7,2,{"$f":"H41*I41","v":{"v":87.4,"d":"€87"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",43.7,3,{"$f":"H42*I42","v":{"v":131.10000000000002,"d":"€131"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J37:J42)","v":{"v":917,"d":"€917"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H44/100)*J43","v":{"v":174.23,"d":"€174"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J43:J44)","v":{"v":1091.23,"d":"€1,091"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA09","LEIPZIGER STRAßE","43,70","44,20","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["3,10","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["3,60","BAI","Z","5,00","11 - 1",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A"]
["4,50","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["4,70","BAI","Z","5,00","11 - 1",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B"]
["4,90","BBC","C","2,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["5,90","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,80","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["7,00","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["12,50","BAI","A / A",null,"10 - 2","JA","Einragendes Dichtungsmaterial Dichtring sichtbar verschoben, jedoch nicht in die Rohrleitung hineinragend"]
["13,60","BCA","A / A","150,00","2",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["16,20","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["16,70","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["23,20","BCA","A / A","100,00","1",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["23,20","BBC","C","10,00","12 - 3",null,"Ablagerungen hartes oder verdichtetes Material ",null,"Fräsen",{"v":50,"d":"€50"}]
["25,00","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["25,30","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["25,60","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["27,30","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["27,60","BCA","A / A","100,00","10",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["29,00","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["33,00","BBC","C","10,00","5 - 9",null,"Ablagerungen hartes oder verdichtetes Material ",null,"Fräsen",{"v":50,"d":"€50"}]
["33,10","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["34,70","BCA","A / A","100,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["36,30","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["37,30","BBB","B","10,00","4 - 8",null,"Anhaftende Stoffe Fett ","A","Fräsen",{"v":50,"d":"€50"}]
["41,10","BBB","B","10,00","4 - 8",null,"Anhaftende Stoffe Fett ","B","Fräsen",{"v":50,"d":"€50"}]
["42,00","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["43,40","BBC","C","20,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["43,70","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["43,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["43,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J54:J85)","v":{"v":5300,"d":"€5,300"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H87/100)*J86","v":{"v":530,"d":"€530"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H88/100)*J86","v":{"v":265,"d":"€265"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H89/100)*J86","v":{"v":636,"d":"€636"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",43.7,2,{"$f":"H90*I90","v":{"v":87.4,"d":"€87"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",43.7,3,{"$f":"H91*I91","v":{"v":131.10000000000002,"d":"€131"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J86:J91)","v":{"v":6949.5,"d":"€6,950"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H93/100)*J92","v":{"v":1320.405,"d":"€1,320"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J92:J93)","v":{"v":8269.905,"d":"€8,270"}}]

{"sheet":"09342384GA10","index":175,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA10","BERLINER STRAßE","10,00","10,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BAB","B / D","2,00","4 - 8","JA","Rissbildung Riss gewundene oder spiralförmige Rissbildung"]
["0,50","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["4,20","BAJ","C","10,00","12","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["7,80","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["10,00","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["10,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",10,2,{"$f":"H16*I16","v":{"v":20,"d":"€20"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",10,3,{"$f":"H17*I17","v":{"v":30,"d":"€30"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":113.5,"d":"€114"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":21.565,"d":"€22"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":135.065,"d":"€135"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA10","BERLINER STRAßE","10,00","10,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BAB","B / D","2,00","4 - 8","JA","Rissbildung Riss gewundene oder spiralförmige Rissbildung"]
["0,50","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["4,20","BAJ","C","10,00","12","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["7,80","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["10,00","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["10,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",10,2,{"$f":"H40*I40","v":{"v":20,"d":"€20"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",10,3,{"$f":"H41*I41","v":{"v":30,"d":"€30"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":113.5,"d":"€114"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":21.565,"d":"€22"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":135.065,"d":"€135"}}]

{"sheet":"09342384GA11","index":176,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA11","LEIPZIGER STRAßE","4,00","4,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,60","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["4,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4,2,{"$f":"H13*I13","v":{"v":8,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4,3,{"$f":"H14*I14","v":{"v":12,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":20,"d":"€20"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":3.8,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":23.8,"d":"€24"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA11","LEIPZIGER STRAßE","4,00","4,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,60","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["4,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4,2,{"$f":"H34*I34","v":{"v":8,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4,3,{"$f":"H35*I35","v":{"v":12,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":20,"d":"€20"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":3.8,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":23.8,"d":"€24"}}]

{"sheet":"09342384GA12","index":177,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA12","LEIPZIGER STRAßE","1,80","1,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBC","C","15,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["0,40","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,80","BBC","C","15,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["1,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.8,2,{"$f":"H14*I14","v":{"v":3.6,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.8,3,{"$f":"H15*I15","v":{"v":5.4,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":136,"d":"€136"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":25.84,"d":"€26"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":161.84,"d":"€162"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA12","LEIPZIGER STRAßE","1,80","1,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBC","C","15,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["0,40","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,80","BBC","C","15,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["1,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.8,2,{"$f":"H36*I36","v":{"v":3.6,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.8,3,{"$f":"H37*I37","v":{"v":5.4,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":136,"d":"€136"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":25.84,"d":"€26"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":161.84,"d":"€162"}}]

{"sheet":"09342384GA13","index":178,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA13","LEIPZIGER STRAßE","2,20","2,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,90","BBE","C","15,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["2,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.2,2,{"$f":"H13*I13","v":{"v":4.4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.2,3,{"$f":"H14*I14","v":{"v":6.6000000000000005,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":11,"d":"€11"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":2.09,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":13.09,"d":"€13"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA13","LEIPZIGER STRAßE","2,20","2,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,90","BBE","C","15,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["2,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.2,2,{"$f":"H34*I34","v":{"v":4.4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.2,3,{"$f":"H35*I35","v":{"v":6.6000000000000005,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":11,"d":"€11"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":2.09,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":13.09,"d":"€13"}}]

{"sheet":"09342384GA15","index":179,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA15","LEIPZIGER STRAßE","1,80","1,80","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBC","C","10,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["0,40","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,80","BBC","C","10,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["1,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.8,2,{"$f":"H14*I14","v":{"v":3.6,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.8,3,{"$f":"H15*I15","v":{"v":5.4,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":136,"d":"€136"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":25.84,"d":"€26"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":161.84,"d":"€162"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA15","LEIPZIGER STRAßE","1,80","1,80","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBC","C","10,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["0,40","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,80","BBC","C","10,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["1,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.8,2,{"$f":"H36*I36","v":{"v":3.6,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.8,3,{"$f":"H37*I37","v":{"v":5.4,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":136,"d":"€136"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":25.84,"d":"€26"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":161.84,"d":"€162"}}]

{"sheet":"09342384GA16","index":180,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA16","LEIPZIGER STRAßE","1,60","1,60","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,20","BBC","C","20,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.6,2,{"$f":"H13*I13","v":{"v":3.2,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.6,3,{"$f":"H14*I14","v":{"v":4.800000000000001,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":71.5,"d":"€72"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":13.585,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":85.08500000000001,"d":"€85"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA16","LEIPZIGER STRAßE","1,60","1,60","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,20","BBC","C","20,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.6,2,{"$f":"H34*I34","v":{"v":3.2,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.6,3,{"$f":"H35*I35","v":{"v":4.800000000000001,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":71.5,"d":"€72"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":13.585,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":85.08500000000001,"d":"€85"}}]

{"sheet":"09342384GA17","index":181,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA17","LEIPZIGER STRAßE","2,80","2,80","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.8,2,{"$f":"H12*I12","v":{"v":5.6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.8,3,{"$f":"H13*I13","v":{"v":8.399999999999999,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":13.999999999999998,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.6599999999999997,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":16.659999999999997,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA17","LEIPZIGER STRAßE","2,80","2,80","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.8,2,{"$f":"H32*I32","v":{"v":5.6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.8,3,{"$f":"H33*I33","v":{"v":8.399999999999999,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":13.999999999999998,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.6599999999999997,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":16.659999999999997,"d":"€17"}}]

{"sheet":"09342384GA18","index":182,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA18","LEIPZIGER STRAßE","2,30","2,30","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,30","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.3,2,{"$f":"H12*I12","v":{"v":4.6,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.3,3,{"$f":"H13*I13","v":{"v":6.8999999999999995,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":11.5,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.185,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":13.685,"d":"€14"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA18","LEIPZIGER STRAßE","2,30","2,30","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,30","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.3,2,{"$f":"H32*I32","v":{"v":4.6,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.3,3,{"$f":"H33*I33","v":{"v":6.8999999999999995,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":11.5,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.185,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":13.685,"d":"€14"}}]

{"sheet":"09342384GA19","index":183,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA19","LEIPZIGER STRAßE","1,40","1,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.4,2,{"$f":"H12*I12","v":{"v":2.8,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.4,3,{"$f":"H13*I13","v":{"v":4.199999999999999,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":6.999999999999999,"d":"€7"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":1.3299999999999998,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":8.329999999999998,"d":"€8"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA19","LEIPZIGER STRAßE","1,40","1,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.4,2,{"$f":"H32*I32","v":{"v":2.8,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.4,3,{"$f":"H33*I33","v":{"v":4.199999999999999,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":6.999999999999999,"d":"€7"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":1.3299999999999998,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":8.329999999999998,"d":"€8"}}]

{"sheet":"09342384GA20","index":184,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA20","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H12*I12","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H13*I13","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":16.065,"d":"€16"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384GA20","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H32*I32","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H33*I33","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":16.065,"d":"€16"}}]

{"sheet":"09342384NN14","index":185,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384NN14","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,00","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H13*I13","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H14*I14","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":5.95,"d":"€6"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384NN14","LEIPZIGER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,00","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H34*I34","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H35*I35","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":5.95,"d":"€6"}}]

{"sheet":"09342384RV02","index":186,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384RV02","BERLINER STRAßE","0,40","0,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,40","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.4,2,{"$f":"H12*I12","v":{"v":0.8,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.4,3,{"$f":"H13*I13","v":{"v":1.2000000000000002,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":2,"d":"€2"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.38,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":2.38,"d":"€2"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384RV02","BERLINER STRAßE","0,40","0,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,40","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.4,2,{"$f":"H32*I32","v":{"v":0.8,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.4,3,{"$f":"H33*I33","v":{"v":1.2000000000000002,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":2,"d":"€2"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.38,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":2.38,"d":"€2"}}]

{"sheet":"09342384RV04","index":187,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384RV04","BERLINER STRAßE","5,50","5,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,30","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["4,40","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,50","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.5,2,{"$f":"H14*I14","v":{"v":11,"d":"€11"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.5,3,{"$f":"H15*I15","v":{"v":16.5,"d":"€17"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":154.5,"d":"€155"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":29.355,"d":"€29"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":183.855,"d":"€184"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384RV04","BERLINER STRAßE","5,50","5,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,30","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["4,40","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,50","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.5,2,{"$f":"H36*I36","v":{"v":11,"d":"€11"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.5,3,{"$f":"H37*I37","v":{"v":16.5,"d":"€17"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":154.5,"d":"€155"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":29.355,"d":"€29"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":183.855,"d":"€184"}}]

{"sheet":"09342384RV06","index":188,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384RV06","BERLINER STRAßE","5,30","5,30","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / B","90,00","8",null,"Krümmung der Leitung nach links nach unten"]
["5,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.3,2,{"$f":"H12*I12","v":{"v":10.6,"d":"€11"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.3,3,{"$f":"H13*I13","v":{"v":15.899999999999999,"d":"€16"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":26.5,"d":"€27"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":5.035,"d":"€5"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":31.535,"d":"€32"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384RV06","BERLINER STRAßE","5,30","5,30","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / B","90,00","8",null,"Krümmung der Leitung nach links nach unten"]
["5,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.3,2,{"$f":"H32*I32","v":{"v":10.6,"d":"€11"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.3,3,{"$f":"H33*I33","v":{"v":15.899999999999999,"d":"€16"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":26.5,"d":"€27"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":5.035,"d":"€5"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":31.535,"d":"€32"}}]

{"sheet":"09342384RV08","index":189,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384RV08","BERLINER STRAßE","5,40","5,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAI","Z","20,00","1 - 5","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,10","BAJ","B","20,00","9","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,20","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,30","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,30","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,40","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":200,"d":"€200"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":20,"d":"€20"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":10,"d":"€10"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":24,"d":"€24"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.4,2,{"$f":"H16*I16","v":{"v":10.8,"d":"€11"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.4,3,{"$f":"H17*I17","v":{"v":16.200000000000003,"d":"€16"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":281,"d":"€281"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":53.39,"d":"€53"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":334.39,"d":"€334"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342384RV08","BERLINER STRAßE","5,40","5,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAI","Z","20,00","1 - 5","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["0,10","BAJ","B","20,00","9","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,20","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,30","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,30","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,40","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":150,"d":"€150"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.4,2,{"$f":"H40*I40","v":{"v":10.8,"d":"€11"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.4,3,{"$f":"H41*I41","v":{"v":16.200000000000003,"d":"€16"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":217.5,"d":"€218"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":41.325,"d":"€41"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":258.825,"d":"€259"}}]

{"sheet":"09342385GA02","index":190,"n_rows":90,"n_cols":10,"rows_kept":90}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385GA02","BERLINER STRAßE","42,80","43,30","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,90","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,90","BAI","A / A",null,"12 - 12","JA","Einragendes Dichtungsmaterial Dichtring sichtbar verschoben, jedoch nicht in die Rohrleitung hineinragend",null,"Fräsen",{"v":50,"d":"€50"}]
["7,10","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen"]
["7,90","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["12,90","BBC","C","10,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["13,60","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["15,00","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["15,00","BAI","A / A",null,"12 - 12","JA","Einragendes Dichtungsmaterial Dichtring sichtbar verschoben, jedoch nicht in die Rohrleitung hineinragend",null,"Fräsen",{"v":50,"d":"€50"}]
["15,90","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["16,10","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["16,50","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["16,60","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["18,00","BBC","C","2,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["22,30","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["24,50","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["25,00","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["25,00","BBC","C","15,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["25,30","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["25,60","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["26,50","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["26,80","BCA","A / A","100,00","1",null,"Anschluss Abzweig offen"]
["32,00","BCA","A / A","100,00","10",null,"Anschluss Abzweig offen"]
["34,70","BCA","A / A","100,00","1",null,"Anschluss Abzweig offen"]
["35,30","BCA","A / A","100,00","11",null,"Anschluss Abzweig offen"]
["40,70","BCA","A / A","100,00","10",null,"Anschluss Abzweig offen"]
["42,40","BBC","C","30,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["42,70","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["42,80","BBC","C","30,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["42,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J34)","v":{"v":550,"d":"€550"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H36/100)*J35","v":{"v":55,"d":"€55"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H37/100)*J35","v":{"v":27.5,"d":"€28"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H38/100)*J35","v":{"v":66,"d":"€66"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",42.8,2,{"$f":"H39*I39","v":{"v":85.6,"d":"€86"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",42.8,3,{"$f":"H40*I40","v":{"v":128.39999999999998,"d":"€128"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J35:J40)","v":{"v":912.5,"d":"€913"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H42/100)*J41","v":{"v":173.375,"d":"€173"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J41:J42)","v":{"v":1085.875,"d":"€1,086"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385GA02","BERLINER STRAßE","42,80","43,30","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,90","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,90","BAI","A / A",null,"12 - 12","JA","Einragendes Dichtungsmaterial Dichtring sichtbar verschoben, jedoch nicht in die Rohrleitung hineinragend"]
["7,10","BCA","A / A","100,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["7,90","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["12,90","BBC","C","10,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["13,60","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["15,00","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["15,00","BAI","A / A",null,"12 - 12","JA","Einragendes Dichtungsmaterial Dichtring sichtbar verschoben, jedoch nicht in die Rohrleitung hineinragend"]
["15,90","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["16,10","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["16,50","BAF","A / E",null,"12 - 12",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar"]
["16,60","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["18,00","BBC","C","2,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["22,30","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["24,50","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["25,00","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["25,00","BBC","C","15,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["25,30","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["25,60","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["26,50","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["26,80","BCA","A / A","100,00","1",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["32,00","BCA","A / A","100,00","10",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["34,70","BCA","A / A","100,00","1",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["35,30","BCA","A / A","100,00","11",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["40,70","BCA","A / A","100,00","10",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["42,40","BBC","C","30,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["42,70","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["42,80","BBC","C","30,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["42,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J52:J81)","v":{"v":5350,"d":"€5,350"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H83/100)*J82","v":{"v":535,"d":"€535"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H84/100)*J82","v":{"v":267.5,"d":"€268"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H85/100)*J82","v":{"v":642,"d":"€642"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",42.8,2,{"$f":"H86*I86","v":{"v":85.6,"d":"€86"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",42.8,3,{"$f":"H87*I87","v":{"v":128.39999999999998,"d":"€128"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J82:J87)","v":{"v":7008.5,"d":"€7,009"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H89/100)*J88","v":{"v":1331.615,"d":"€1,332"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J88:J89)","v":{"v":8340.115,"d":"€8,340"}}]

{"sheet":"09342385GA03","index":191,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385GA03","BERLINER STRAßE","4,10","4,10","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,00","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["3,50","BBB","B","20,00","12 - 12",null,"Anhaftende Stoffe Fett ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.1,2,{"$f":"H14*I14","v":{"v":8.2,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.1,3,{"$f":"H15*I15","v":{"v":12.299999999999999,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":84,"d":"€84"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":15.96,"d":"€16"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":99.96000000000001,"d":"€100"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385GA03","BERLINER STRAßE","4,10","4,10","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,00","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["3,50","BBB","B","20,00","12 - 12",null,"Anhaftende Stoffe Fett ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.1,2,{"$f":"H36*I36","v":{"v":8.2,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.1,3,{"$f":"H37*I37","v":{"v":12.299999999999999,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":84,"d":"€84"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":15.96,"d":"€16"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":99.96000000000001,"d":"€100"}}]

{"sheet":"09342385GA04","index":192,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385GA04","BERLINER STRAßE","1,80","1,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,50","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,60","BAI","Z","20,00","4 - 8","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.8,2,{"$f":"H14*I14","v":{"v":3.6,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.8,3,{"$f":"H15*I15","v":{"v":5.4,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":72.5,"d":"€73"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":13.775,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":86.275,"d":"€86"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385GA04","BERLINER STRAßE","1,80","1,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,50","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,60","BAI","Z","20,00","4 - 8","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["1,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.8,2,{"$f":"H36*I36","v":{"v":3.6,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.8,3,{"$f":"H37*I37","v":{"v":5.4,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":9,"d":"€9"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":1.71,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":10.71,"d":"€11"}}]

{"sheet":"09342385GA06","index":193,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385GA06","BERLINER STRAßE","1,60","1,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,20","BAI","Z","10,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,40","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,40","BBE","C","60,00","12 - 12",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["1,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.6,2,{"$f":"H15*I15","v":{"v":3.2,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.6,3,{"$f":"H16*I16","v":{"v":4.800000000000001,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":71.5,"d":"€72"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":13.585,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":85.08500000000001,"d":"€85"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385GA06","BERLINER STRAßE","1,60","1,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,20","BAI","Z","10,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["0,40","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,40","BBE","C","60,00","12 - 12",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["1,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.6,2,{"$f":"H38*I38","v":{"v":3.2,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.6,3,{"$f":"H39*I39","v":{"v":4.800000000000001,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":8,"d":"€8"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":1.52,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":9.52,"d":"€10"}}]

{"sheet":"09342385GA07","index":194,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385GA07","BERLINER STRAßE","2,20","2,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,80","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["2,20","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["2,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.2,2,{"$f":"H14*I14","v":{"v":4.4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.2,3,{"$f":"H15*I15","v":{"v":6.6000000000000005,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":138,"d":"€138"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":26.22,"d":"€26"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":164.22,"d":"€164"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385GA07","BERLINER STRAßE","2,20","2,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,80","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["2,20","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["2,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.2,2,{"$f":"H36*I36","v":{"v":4.4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.2,3,{"$f":"H37*I37","v":{"v":6.6000000000000005,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":138,"d":"€138"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":26.22,"d":"€26"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":164.22,"d":"€164"}}]

{"sheet":"09342385GA09","index":195,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385GA09","BERLINER STRAßE","1,50","1,50","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / B","45,00","8",null,"Krümmung der Leitung nach links nach unten"]
["1,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.5,2,{"$f":"H12*I12","v":{"v":3,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.5,3,{"$f":"H13*I13","v":{"v":4.5,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":7.5,"d":"€8"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":1.425,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":8.925,"d":"€9"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385GA09","BERLINER STRAßE","1,50","1,50","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / B","45,00","8",null,"Krümmung der Leitung nach links nach unten"]
["1,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.5,2,{"$f":"H32*I32","v":{"v":3,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.5,3,{"$f":"H33*I33","v":{"v":4.5,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":7.5,"d":"€8"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":1.425,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":8.925,"d":"€9"}}]

{"sheet":"09342385NN05","index":196,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385NN05","BERLINER STRAßE","1,90","1,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,50","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,90","BBE","C","50,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["1,90","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.9,2,{"$f":"H14*I14","v":{"v":3.8,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.9,3,{"$f":"H15*I15","v":{"v":5.699999999999999,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":9.5,"d":"€10"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":1.805,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":11.305,"d":"€11"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385NN05","BERLINER STRAßE","1,90","1,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["0,50","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,90","BBE","C","50,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["1,90","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.9,2,{"$f":"H36*I36","v":{"v":3.8,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.9,3,{"$f":"H37*I37","v":{"v":5.699999999999999,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":9.5,"d":"€10"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":1.805,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":11.305,"d":"€11"}}]

{"sheet":"09342385NN08","index":197,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385NN08","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385NN08","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09342385NN10","index":198,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385NN10","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385NN10","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09342385NN11","index":199,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385NN11","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385NN11","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09342385NN12","index":200,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385NN12","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385NN12","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"100","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09342385RV01","index":201,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385RV01","BERLINER STRAßE","3,50","3,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["3,50","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H12*I12","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H13*I13","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":17.5,"d":"€18"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":3.325,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":20.825,"d":"€21"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342385RV01","BERLINER STRAßE","3,50","3,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["3,50","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H32*I32","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H33*I33","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":17.5,"d":"€18"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":3.325,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":20.825,"d":"€21"}}]

{"sheet":"09342386GA01","index":202,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342386GA01","LEIPZIGER STRAßE","6,60","6,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,30","BAJ","B","25,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.6,2,{"$f":"H13*I13","v":{"v":13.2,"d":"€13"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.6,3,{"$f":"H14*I14","v":{"v":19.799999999999997,"d":"€20"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":96.5,"d":"€97"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":18.335,"d":"€18"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":114.83500000000001,"d":"€115"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342386GA01","LEIPZIGER STRAßE","6,60","6,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,30","BAJ","B","25,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.6,2,{"$f":"H34*I34","v":{"v":13.2,"d":"€13"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.6,3,{"$f":"H35*I35","v":{"v":19.799999999999997,"d":"€20"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":96.5,"d":"€97"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":18.335,"d":"€18"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":114.83500000000001,"d":"€115"}}]

{"sheet":"09342386GA04","index":203,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342386GA04","LEIPZIGER STRAßE","7,90","7,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["6,20","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["7,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",7.9,2,{"$f":"H13*I13","v":{"v":15.8,"d":"€16"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",7.9,3,{"$f":"H14*I14","v":{"v":23.700000000000003,"d":"€24"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":103,"d":"€103"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":19.57,"d":"€20"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":122.57,"d":"€123"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342386GA04","LEIPZIGER STRAßE","7,90","7,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["6,20","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["7,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",7.9,2,{"$f":"H34*I34","v":{"v":15.8,"d":"€16"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",7.9,3,{"$f":"H35*I35","v":{"v":23.700000000000003,"d":"€24"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":103,"d":"€103"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":19.57,"d":"€20"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":122.57,"d":"€123"}}]

{"sheet":"09342386RV02","index":204,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342386RV02","LEIPZIGER STRAßE","6,30","6,30","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAI","Z","5,00","8 - 10","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,30","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["2,00","BBC","C","5,00","4 - 8","JA","Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["2,70","BBC","C","5,00","4 - 8","JA","Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["6,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":150,"d":"€150"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.3,2,{"$f":"H15*I15","v":{"v":12.6,"d":"€13"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.3,3,{"$f":"H16*I16","v":{"v":18.9,"d":"€19"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":222,"d":"€222"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":42.18,"d":"€42"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":264.18,"d":"€264"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342386RV02","LEIPZIGER STRAßE","6,30","6,30","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAI","Z","5,00","8 - 10","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["1,30","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["2,00","BBC","C","5,00","4 - 8","JA","Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["2,70","BBC","C","5,00","4 - 8","JA","Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["6,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.3,2,{"$f":"H38*I38","v":{"v":12.6,"d":"€13"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.3,3,{"$f":"H39*I39","v":{"v":18.9,"d":"€19"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":158.5,"d":"€159"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":30.115000000000002,"d":"€30"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":188.615,"d":"€189"}}]

{"sheet":"09342386RV03","index":205,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342386RV03","LEIPZIGER STRAßE","6,40","6,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,30","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,40","BAB","B / C","1,00","12 - 12",null,"Rissbildung Riss komplexe Rissbildung","A"]
["1,60","BAB","B / C","1,00","12 - 12",null,"Rissbildung Riss komplexe Rissbildung","B"]
["6,40","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.4,2,{"$f":"H14*I14","v":{"v":12.8,"d":"€13"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.4,3,{"$f":"H15*I15","v":{"v":19.200000000000003,"d":"€19"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":32,"d":"€32"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":6.08,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":38.08,"d":"€38"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342386RV03","LEIPZIGER STRAßE","6,40","6,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,30","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,40","BAB","B / C","1,00","12 - 12",null,"Rissbildung Riss komplexe Rissbildung","A"]
["1,60","BAB","B / C","1,00","12 - 12",null,"Rissbildung Riss komplexe Rissbildung","B"]
["6,40","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.4,2,{"$f":"H36*I36","v":{"v":12.8,"d":"€13"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.4,3,{"$f":"H37*I37","v":{"v":19.200000000000003,"d":"€19"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":32,"d":"€32"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":6.08,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":38.08,"d":"€38"}}]

{"sheet":"09342387GA02","index":206,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342387GA02","LEIPZIGER STRAßE","9,10","9,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,10","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["6,00","BAC","A","200,00","2 - 10",null,"Rohrbruch / Einsturz Bruch "]
["6,40","BCC","B / A","45,00","2",null,"Krümmung der Leitung nach rechts nach oben"]
["9,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.1,2,{"$f":"H14*I14","v":{"v":18.2,"d":"€18"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.1,3,{"$f":"H15*I15","v":{"v":27.299999999999997,"d":"€27"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":45.5,"d":"€46"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":8.645,"d":"€9"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":54.144999999999996,"d":"€54"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342387GA02","LEIPZIGER STRAßE","9,10","9,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,10","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["6,00","BAC","A","200,00","2 - 10",null,"Rohrbruch / Einsturz Bruch "]
["6,40","BCC","B / A","45,00","2",null,"Krümmung der Leitung nach rechts nach oben"]
["9,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.1,2,{"$f":"H36*I36","v":{"v":18.2,"d":"€18"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.1,3,{"$f":"H37*I37","v":{"v":27.299999999999997,"d":"€27"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":45.5,"d":"€46"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":8.645,"d":"€9"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":54.144999999999996,"d":"€54"}}]

{"sheet":"09342387GA04","index":207,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342387GA04","LEIPZIGER STRAßE","7,70","7,70","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["6,00","BAC","A","200,00","2 - 10",null,"Rohrbruch / Einsturz Bruch "]
["7,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",7.7,2,{"$f":"H13*I13","v":{"v":15.4,"d":"€15"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",7.7,3,{"$f":"H14*I14","v":{"v":23.1,"d":"€23"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":38.5,"d":"€39"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":7.315,"d":"€7"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":45.815,"d":"€46"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342387GA04","LEIPZIGER STRAßE","7,70","7,70","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["6,00","BAC","A","200,00","2 - 10",null,"Rohrbruch / Einsturz Bruch "]
["7,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",7.7,2,{"$f":"H34*I34","v":{"v":15.4,"d":"€15"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",7.7,3,{"$f":"H35*I35","v":{"v":23.1,"d":"€23"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":38.5,"d":"€39"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":7.315,"d":"€7"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":45.815,"d":"€46"}}]

{"sheet":"09342387NN06","index":208,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342387NN06","LEIPZIGER STRAßE","7,00","7,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["7,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",7,2,{"$f":"H12*I12","v":{"v":14,"d":"€14"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",7,3,{"$f":"H13*I13","v":{"v":21,"d":"€21"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":35,"d":"€35"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":6.65,"d":"€7"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":41.65,"d":"€42"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342387NN06","LEIPZIGER STRAßE","7,00","7,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["7,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",7,2,{"$f":"H32*I32","v":{"v":14,"d":"€14"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",7,3,{"$f":"H33*I33","v":{"v":21,"d":"€21"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":35,"d":"€35"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":6.65,"d":"€7"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":41.65,"d":"€42"}}]

{"sheet":"09342387RS08","index":209,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342387RS08","LEIPZIGER STRAßE","16,20","17,20","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,50","BCA","A / A","200,00","6",null,"Anschluss Abzweig offen"]
["1,20","BDD","C","50,00",null,null,"Wasserspiegel trüb ","A"]
["10,40","BDD","C","20,00",null,null,"Wasserspiegel trüb ","C"]
["12,80","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["16,20","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["16,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",16.2,2,{"$f":"H16*I16","v":{"v":32.4,"d":"€32"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",16.2,3,{"$f":"H17*I17","v":{"v":48.599999999999994,"d":"€49"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":144.5,"d":"€145"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":27.455000000000002,"d":"€27"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":171.955,"d":"€172"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342387RS08","LEIPZIGER STRAßE","16,20","17,20","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,50","BCA","A / A","200,00","6",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["1,20","BDD","C","50,00",null,null,"Wasserspiegel trüb ","A"]
["10,40","BDD","C","20,00",null,null,"Wasserspiegel trüb ","C"]
["12,80","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["16,20","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["16,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":2236,"d":"€2,236"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":2776,"d":"€2,776"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":277.6,"d":"€278"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":138.8,"d":"€139"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":333.12,"d":"€333"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",16.2,2,{"$f":"H40*I40","v":{"v":32.4,"d":"€32"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",16.2,3,{"$f":"H41*I41","v":{"v":48.599999999999994,"d":"€49"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":3606.52,"d":"€3,607"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":685.2388,"d":"€685"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":4291.7588,"d":"€4,292"}}]

{"sheet":"09342387RV03","index":210,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342387RV03","LEIPZIGER STRAßE","6,30","6,30","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["6,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.3,2,{"$f":"H12*I12","v":{"v":12.6,"d":"€13"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.3,3,{"$f":"H13*I13","v":{"v":18.9,"d":"€19"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":31.5,"d":"€32"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":5.985,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":37.485,"d":"€37"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342387RV03","LEIPZIGER STRAßE","6,30","6,30","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["6,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.3,2,{"$f":"H32*I32","v":{"v":12.6,"d":"€13"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.3,3,{"$f":"H33*I33","v":{"v":18.9,"d":"€19"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":31.5,"d":"€32"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":5.985,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":37.485,"d":"€37"}}]

{"sheet":"09342387RV05","index":211,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342387RV05","LEIPZIGER STRAßE","6,30","6,30","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["6,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.3,2,{"$f":"H12*I12","v":{"v":12.6,"d":"€13"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.3,3,{"$f":"H13*I13","v":{"v":18.9,"d":"€19"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":31.5,"d":"€32"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":5.985,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":37.485,"d":"€37"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342387RV05","LEIPZIGER STRAßE","6,30","6,30","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["6,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.3,2,{"$f":"H32*I32","v":{"v":12.6,"d":"€13"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.3,3,{"$f":"H33*I33","v":{"v":18.9,"d":"€19"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":31.5,"d":"€32"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":5.985,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":37.485,"d":"€37"}}]

{"sheet":"09342387RV07","index":212,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342387RV07","LEIPZIGER STRAßE","6,40","6,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,40","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,50","BAJ","B","25,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,30","BAI","Z","10,00","12 - 3","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,40","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.4,2,{"$f":"H14*I14","v":{"v":12.8,"d":"€13"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.4,3,{"$f":"H15*I15","v":{"v":19.200000000000003,"d":"€19"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":159,"d":"€159"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":30.21,"d":"€30"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":189.21,"d":"€189"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342387RV07","LEIPZIGER STRAßE","6,40","6,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,40","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,50","BAJ","B","25,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,30","BAI","Z","10,00","12 - 3","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["6,40","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.4,2,{"$f":"H36*I36","v":{"v":12.8,"d":"€13"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.4,3,{"$f":"H37*I37","v":{"v":19.200000000000003,"d":"€19"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":95.5,"d":"€96"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":18.145,"d":"€18"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":113.645,"d":"€114"}}]

{"sheet":"09342668GA02","index":213,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668GA02","LEIPZIGER STRAßE","4,20","4,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.2,2,{"$f":"H11*I11","v":{"v":8.4,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.2,3,{"$f":"H12*I12","v":{"v":12.600000000000001,"d":"€13"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":21,"d":"€21"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":3.99,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":24.990000000000002,"d":"€25"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668GA02","LEIPZIGER STRAßE","4,20","4,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.2,2,{"$f":"H30*I30","v":{"v":8.4,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.2,3,{"$f":"H31*I31","v":{"v":12.600000000000001,"d":"€13"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":21,"d":"€21"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":3.99,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":24.990000000000002,"d":"€25"}}]

{"sheet":"09342668GA03","index":214,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668GA03","LEIPZIGER STRAßE","6,10","6,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["6,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.1,2,{"$f":"H11*I11","v":{"v":12.2,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.1,3,{"$f":"H12*I12","v":{"v":18.299999999999997,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":30.499999999999996,"d":"€31"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":5.794999999999999,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":36.294999999999995,"d":"€36"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668GA03","LEIPZIGER STRAßE","6,10","6,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["6,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.1,2,{"$f":"H30*I30","v":{"v":12.2,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.1,3,{"$f":"H31*I31","v":{"v":18.299999999999997,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":30.499999999999996,"d":"€31"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":5.794999999999999,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":36.294999999999995,"d":"€36"}}]

{"sheet":"09342668GA04","index":215,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668GA04","LEIPZIGER STRAßE","9,70","9,70","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,90","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["6,30","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["7,80","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["9,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.7,2,{"$f":"H14*I14","v":{"v":19.4,"d":"€19"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.7,3,{"$f":"H15*I15","v":{"v":29.099999999999998,"d":"€29"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":112,"d":"€112"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":21.28,"d":"€21"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":133.28,"d":"€133"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668GA04","LEIPZIGER STRAßE","9,70","9,70","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,90","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["6,30","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["7,80","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["9,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.7,2,{"$f":"H36*I36","v":{"v":19.4,"d":"€19"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.7,3,{"$f":"H37*I37","v":{"v":29.099999999999998,"d":"€29"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":48.5,"d":"€49"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":9.215,"d":"€9"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":57.715,"d":"€58"}}]

{"sheet":"09342668GA05","index":216,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668GA05","LEIPZIGER STRAßE","4,00","4,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["3,10","BBC","C","3,00","5 - 7",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["4,00","BBC","C","3,00","5 - 7",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["4,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4,2,{"$f":"H13*I13","v":{"v":8,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4,3,{"$f":"H14*I14","v":{"v":12,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":147,"d":"€147"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":27.93,"d":"€28"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":174.93,"d":"€175"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668GA05","LEIPZIGER STRAßE","4,00","4,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["3,10","BBC","C","3,00","5 - 7",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["4,00","BBC","C","3,00","5 - 7",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["4,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4,2,{"$f":"H34*I34","v":{"v":8,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4,3,{"$f":"H35*I35","v":{"v":12,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":147,"d":"€147"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":27.93,"d":"€28"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":174.93,"d":"€175"}}]

{"sheet":"09342668RS07","index":217,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668RS07","LEIPZIGER STRAßE","5,80","6,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,70","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,70","AED","PP",{"$nulls":3},"Grundlagen änderung  "]
["4,10","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["4,10","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["5,80","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.8,2,{"$f":"H16*I16","v":{"v":11.6,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.8,3,{"$f":"H17*I17","v":{"v":17.4,"d":"€17"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":29,"d":"€29"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":5.51,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":34.51,"d":"€35"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668RS07","LEIPZIGER STRAßE","5,80","6,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,70","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,70","AED","PP",{"$nulls":3},"Grundlagen änderung  "]
["4,10","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["4,10","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["5,80","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.8,2,{"$f":"H40*I40","v":{"v":11.6,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.8,3,{"$f":"H41*I41","v":{"v":17.4,"d":"€17"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":29,"d":"€29"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":5.51,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":34.51,"d":"€35"}}]

{"sheet":"09342668RV06","index":218,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668RV06","LEIPZIGER STRAßE","9,30","9,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["9,30","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["9,30","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["9,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.3,2,{"$f":"H14*I14","v":{"v":18.6,"d":"€19"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.3,3,{"$f":"H15*I15","v":{"v":27.900000000000002,"d":"€28"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":46.5,"d":"€47"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":8.835,"d":"€9"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":55.335,"d":"€55"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668RV06","LEIPZIGER STRAßE","9,30","9,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["9,30","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["9,30","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["9,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.3,2,{"$f":"H36*I36","v":{"v":18.6,"d":"€19"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.3,3,{"$f":"H37*I37","v":{"v":27.900000000000002,"d":"€28"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":46.5,"d":"€47"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":8.835,"d":"€9"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":55.335,"d":"€55"}}]

{"sheet":"09342668SE01","index":219,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668SE01","LEIPZIGER STRAßE","3,50","3,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,30","BAB","B / B","10,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["2,20","BAB","B / C","8,00","2 - 10",null,"Rissbildung Riss komplexe Rissbildung","A"]
["2,70","BAB","B / C","8,00","12 - 12",null,"Rissbildung Riss komplexe Rissbildung","B"]
["3,50","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H15*I15","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H16*I16","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":17.5,"d":"€18"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":3.325,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":20.825,"d":"€21"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668SE01","LEIPZIGER STRAßE","3,50","3,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,30","BAB","B / B","10,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["2,20","BAB","B / C","8,00","2 - 10",null,"Rissbildung Riss komplexe Rissbildung","A"]
["2,70","BAB","B / C","8,00","12 - 12",null,"Rissbildung Riss komplexe Rissbildung","B"]
["3,50","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H38*I38","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H39*I39","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":17.5,"d":"€18"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":3.325,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":20.825,"d":"€21"}}]

{"sheet":"09342668_1SE01","index":220,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668_1SE01","LEIPZIGER STRAßE","2,70","2,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,20","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["1,50","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["2,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,40","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["2,70","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H16*I16","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H17*I17","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":16.065,"d":"€16"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342668_1SE01","LEIPZIGER STRAßE","2,70","2,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,20","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["1,50","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["2,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,40","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["2,70","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H40*I40","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H41*I41","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":16.065,"d":"€16"}}]

{"sheet":"09342669GA02","index":221,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342669GA02","LEIPZIGER STRAßE","10,60","10,60","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,30","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,40","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["3,70","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,70","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,70","BAI","Z","10,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["10,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":150,"d":"€150"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",10.6,2,{"$f":"H16*I16","v":{"v":21.2,"d":"€21"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",10.6,3,{"$f":"H17*I17","v":{"v":31.799999999999997,"d":"€32"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":243.5,"d":"€244"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":46.265,"d":"€46"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":289.765,"d":"€290"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342669GA02","LEIPZIGER STRAßE","10,60","10,60","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,30","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,40","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["3,70","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["4,70","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["6,70","BAI","Z","10,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["10,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",10.6,2,{"$f":"H40*I40","v":{"v":21.2,"d":"€21"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",10.6,3,{"$f":"H41*I41","v":{"v":31.799999999999997,"d":"€32"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":53,"d":"€53"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":10.07,"d":"€10"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":63.07,"d":"€63"}}]

{"sheet":"09342669GA03","index":222,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342669GA03","LEIPZIGER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,40","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,40","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["2,40","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,80","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["2,80","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["3,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H16*I16","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H17*I17","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":16,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":3.04,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":19.04,"d":"€19"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342669GA03","LEIPZIGER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,40","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,40","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["2,40","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,80","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["2,80","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["3,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H40*I40","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H41*I41","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":16,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":3.04,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":19.04,"d":"€19"}}]

{"sheet":"09342669GA04","index":223,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342669GA04","LEIPZIGER STRAßE","6,00","6,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["5,10","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["5,10","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["5,10","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["5,80","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["6,00","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["6,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6,2,{"$f":"H16*I16","v":{"v":12,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6,3,{"$f":"H17*I17","v":{"v":18,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":30,"d":"€30"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":5.7,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":35.7,"d":"€36"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342669GA04","LEIPZIGER STRAßE","6,00","6,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["5,10","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["5,10","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["5,10","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["5,80","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["6,00","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["6,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6,2,{"$f":"H40*I40","v":{"v":12,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6,3,{"$f":"H41*I41","v":{"v":18,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":30,"d":"€30"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":5.7,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":35.7,"d":"€36"}}]

{"sheet":"09342669GA05","index":224,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342669GA05","LEIPZIGER STRAßE","3,70","3,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["3,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.7,2,{"$f":"H11*I11","v":{"v":7.4,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.7,3,{"$f":"H12*I12","v":{"v":11.100000000000001,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":18.5,"d":"€19"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":3.515,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":22.015,"d":"€22"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342669GA05","LEIPZIGER STRAßE","3,70","3,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["3,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.7,2,{"$f":"H30*I30","v":{"v":7.4,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.7,3,{"$f":"H31*I31","v":{"v":11.100000000000001,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":18.5,"d":"€19"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":3.515,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":22.015,"d":"€22"}}]

{"sheet":"09342669GA06","index":225,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342669GA06","LEIPZIGER STRAßE","5,80","5,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["5,60","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["5,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.8,2,{"$f":"H12*I12","v":{"v":11.6,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.8,3,{"$f":"H13*I13","v":{"v":17.4,"d":"€17"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":29,"d":"€29"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":5.51,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":34.51,"d":"€35"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342669GA06","LEIPZIGER STRAßE","5,80","5,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["5,60","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["5,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.8,2,{"$f":"H32*I32","v":{"v":11.6,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.8,3,{"$f":"H33*I33","v":{"v":17.4,"d":"€17"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":29,"d":"€29"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":5.51,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":34.51,"d":"€35"}}]

{"sheet":"09342669RV01","index":226,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342669RV01","LEIPZIGER STRAßE","4,00","4,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,00","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["4,00","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4,2,{"$f":"H12*I12","v":{"v":8,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4,3,{"$f":"H13*I13","v":{"v":12,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":20,"d":"€20"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":3.8,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":23.8,"d":"€24"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342669RV01","LEIPZIGER STRAßE","4,00","4,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,00","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["4,00","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4,2,{"$f":"H32*I32","v":{"v":8,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4,3,{"$f":"H33*I33","v":{"v":12,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":20,"d":"€20"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":3.8,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":23.8,"d":"€24"}}]

{"sheet":"09342670RS03","index":227,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342670RS03","LEIPZIGER STRAßE","16,30","17,30","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["16,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",16.3,2,{"$f":"H11*I11","v":{"v":32.6,"d":"€33"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",16.3,3,{"$f":"H12*I12","v":{"v":48.900000000000006,"d":"€49"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":81.5,"d":"€82"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":15.485,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":96.985,"d":"€97"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342670RS03","LEIPZIGER STRAßE","16,30","17,30","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["16,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":2249,"d":"€2,249"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":2249,"d":"€2,249"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":224.9,"d":"€225"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":112.45,"d":"€112"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":269.88,"d":"€270"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",16.3,2,{"$f":"H30*I30","v":{"v":32.6,"d":"€33"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",16.3,3,{"$f":"H31*I31","v":{"v":48.900000000000006,"d":"€49"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":2937.73,"d":"€2,938"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":558.1687000000001,"d":"€558"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":3495.8987,"d":"€3,496"}}]

{"sheet":"09342670RV01","index":228,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342670RV01","LEIPZIGER STRAßE","5,70","5,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["5,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["5,70","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.7,2,{"$f":"H12*I12","v":{"v":11.4,"d":"€11"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.7,3,{"$f":"H13*I13","v":{"v":17.1,"d":"€17"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":28.5,"d":"€29"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":5.415,"d":"€5"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":33.915,"d":"€34"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342670RV01","LEIPZIGER STRAßE","5,70","5,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["5,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["5,70","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.7,2,{"$f":"H32*I32","v":{"v":11.4,"d":"€11"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.7,3,{"$f":"H33*I33","v":{"v":17.1,"d":"€17"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":28.5,"d":"€29"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":5.415,"d":"€5"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":33.915,"d":"€34"}}]

{"sheet":"09342670SE02","index":229,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342670SE02","LEIPZIGER STRAßE","3,50","3,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,00","BAJ","B","30,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,90","BAJ","B","30,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,50","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H14*I14","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H15*I15","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":144.5,"d":"€145"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":27.455000000000002,"d":"€27"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":171.955,"d":"€172"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342670SE02","LEIPZIGER STRAßE","3,50","3,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,00","BAJ","B","30,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,90","BAJ","B","30,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,50","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H36*I36","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H37*I37","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":144.5,"d":"€145"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":27.455000000000002,"d":"€27"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":171.955,"d":"€172"}}]

{"sheet":"09342671GA01","index":230,"n_rows":50,"n_cols":10,"rows_kept":50}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671GA01","LEIPZIGER STRAßE","8,80","8,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["1,90","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","C"]
["7,60","BAJ","B","10,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["7,60","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","C"]
["8,70","BAB","B / B","3,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["8,80","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["8,80","BAC","C",null,"12 - 12",null,"Rohrbruch / Einsturz Einsturz "]
["8,80","BAO",null,null,"12 - 12",null,"Boden sichtbar  "]
["8,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J14)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H16/100)*J15","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H17/100)*J15","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H18/100)*J15","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",8.8,2,{"$f":"H19*I19","v":{"v":17.6,"d":"€18"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",8.8,3,{"$f":"H20*I20","v":{"v":26.400000000000002,"d":"€26"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J15:J20)","v":{"v":107.5,"d":"€108"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H22/100)*J21","v":{"v":20.425,"d":"€20"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J21:J22)","v":{"v":127.925,"d":"€128"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671GA01","LEIPZIGER STRAßE","8,80","8,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["1,90","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","C"]
["7,60","BAJ","B","10,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["7,60","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","C"]
["8,70","BAB","B / B","3,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["8,80","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["8,80","BAC","C",null,"12 - 12",null,"Rohrbruch / Einsturz Einsturz "]
["8,80","BAO",null,null,"12 - 12",null,"Boden sichtbar  "]
["8,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J32:J41)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H43/100)*J42","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H44/100)*J42","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H45/100)*J42","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",8.8,2,{"$f":"H46*I46","v":{"v":17.6,"d":"€18"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",8.8,3,{"$f":"H47*I47","v":{"v":26.400000000000002,"d":"€26"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J42:J47)","v":{"v":107.5,"d":"€108"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H49/100)*J48","v":{"v":20.425,"d":"€20"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J48:J49)","v":{"v":127.925,"d":"€128"}}]

{"sheet":"09342671GA02","index":231,"n_rows":56,"n_cols":10,"rows_kept":56}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671GA02","LEIPZIGER STRAßE","8,50","8,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,40","BDD","C","10,00",null,null,"Wasserspiegel trüb ","A"]
["0,40","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["0,40","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,40","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["3,30","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["5,50","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["7,30","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["7,90","BAB","B / A","3,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","A"]
["8,40","BAB","B / A","3,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","B"]
["8,50","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["8,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J17)","v":{"v":150,"d":"€150"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H19/100)*J18","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H20/100)*J18","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H21/100)*J18","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",8.5,2,{"$f":"H22*I22","v":{"v":17,"d":"€17"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",8.5,3,{"$f":"H23*I23","v":{"v":25.5,"d":"€26"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J18:J23)","v":{"v":233,"d":"€233"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H25/100)*J24","v":{"v":44.27,"d":"€44"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J24:J25)","v":{"v":277.27,"d":"€277"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671GA02","LEIPZIGER STRAßE","8,50","8,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,40","BDD","C","10,00",null,null,"Wasserspiegel trüb ","A"]
["0,40","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["0,40","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,40","BDD","C",{"$nulls":3},"Wasserspiegel trüb ","B"]
["3,30","BBC","C","3,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["5,50","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["7,30","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["7,90","BAB","B / A","3,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","A"]
["8,40","BAB","B / A","3,00","5 - 7",null,"Rissbildung Riss in Längsrichtung","B"]
["8,50","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["8,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J35:J47)","v":{"v":150,"d":"€150"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H49/100)*J48","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H50/100)*J48","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H51/100)*J48","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",8.5,2,{"$f":"H52*I52","v":{"v":17,"d":"€17"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",8.5,3,{"$f":"H53*I53","v":{"v":25.5,"d":"€26"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J48:J53)","v":{"v":233,"d":"€233"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H55/100)*J54","v":{"v":44.27,"d":"€44"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J54:J55)","v":{"v":277.27,"d":"€277"}}]

{"sheet":"09342671GA04","index":232,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671GA04","LEIPZIGER STRAßE","5,90","5,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,70","BAJ","C","10,00","10","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.9,2,{"$f":"H12*I12","v":{"v":11.8,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.9,3,{"$f":"H13*I13","v":{"v":17.700000000000003,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":93,"d":"€93"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":17.67,"d":"€18"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":110.67,"d":"€111"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671GA04","LEIPZIGER STRAßE","5,90","5,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,70","BAJ","C","10,00","10","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.9,2,{"$f":"H32*I32","v":{"v":11.8,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.9,3,{"$f":"H33*I33","v":{"v":17.700000000000003,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":93,"d":"€93"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":17.67,"d":"€18"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":110.67,"d":"€111"}}]

{"sheet":"09342671GA05","index":233,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671GA05","LEIPZIGER STRAßE","4,60","4,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,40","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,50","BAJ","B","15,00","5","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,60","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["3,60","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["3,60","BAJ","A","40,00","12 - 12","JA","Verschobene Verbindung in längsrichtung ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,60","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["4,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.6,2,{"$f":"H17*I17","v":{"v":9.2,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.6,3,{"$f":"H18*I18","v":{"v":13.799999999999999,"d":"€14"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":150,"d":"€150"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":28.5,"d":"€29"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":178.5,"d":"€179"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671GA05","LEIPZIGER STRAßE","4,60","4,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,40","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,50","BAJ","B","15,00","5","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,60","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["3,60","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["3,60","BAJ","A","40,00","12 - 12","JA","Verschobene Verbindung in längsrichtung ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,60","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["4,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.6,2,{"$f":"H42*I42","v":{"v":9.2,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.6,3,{"$f":"H43*I43","v":{"v":13.799999999999999,"d":"€14"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":150,"d":"€150"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":28.5,"d":"€29"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":178.5,"d":"€179"}}]

{"sheet":"09342671GA06","index":234,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671GA06","LEIPZIGER STRAßE","5,90","5,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["4,20","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["5,90","BBD","A","60,00","2 - 10",null,"Eindringen von Bodenmaterial Sand "]
["5,90","BAJ","B","80,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,90","BAP",null,null,"8 - 4","JA","Hohlraum sichtbar  "]
["5,90","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.9,2,{"$f":"H16*I16","v":{"v":11.8,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.9,3,{"$f":"H17*I17","v":{"v":17.700000000000003,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":93,"d":"€93"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":17.67,"d":"€18"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":110.67,"d":"€111"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671GA06","LEIPZIGER STRAßE","5,90","5,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["4,20","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["5,90","BBD","A","60,00","2 - 10",null,"Eindringen von Bodenmaterial Sand "]
["5,90","BAJ","B","80,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,90","BAP",null,null,"8 - 4","JA","Hohlraum sichtbar  "]
["5,90","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.9,2,{"$f":"H40*I40","v":{"v":11.8,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.9,3,{"$f":"H41*I41","v":{"v":17.700000000000003,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":93,"d":"€93"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":17.67,"d":"€18"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":110.67,"d":"€111"}}]

{"sheet":"09342671GA07","index":235,"n_rows":48,"n_cols":10,"rows_kept":48}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671GA07","LEIPZIGER STRAßE","5,50","5,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,40","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["0,40","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,40","BBE","C","5,00","4 - 8","JA","Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["0,40","BAJ","A","50,00","12 - 12","JA","Verschobene Verbindung in längsrichtung ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,50","BAF","C / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["4,30","BAJ","C","5,00","9","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,50","BAF","C / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["5,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J13)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H15/100)*J14","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H16/100)*J14","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H17/100)*J14","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.5,2,{"$f":"H18*I18","v":{"v":11,"d":"€11"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.5,3,{"$f":"H19*I19","v":{"v":16.5,"d":"€17"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J14:J19)","v":{"v":154.5,"d":"€155"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H21/100)*J20","v":{"v":29.355,"d":"€29"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J20:J21)","v":{"v":183.855,"d":"€184"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671GA07","LEIPZIGER STRAßE","5,50","5,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,40","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["0,40","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,40","BBE","C","5,00","4 - 8","JA","Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["0,40","BAJ","A","50,00","12 - 12","JA","Verschobene Verbindung in längsrichtung ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,50","BAF","C / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["4,30","BAJ","C","5,00","9","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,50","BAF","C / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["5,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J31:J39)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.5,2,{"$f":"H44*I44","v":{"v":11,"d":"€11"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.5,3,{"$f":"H45*I45","v":{"v":16.5,"d":"€17"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":154.5,"d":"€155"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":29.355,"d":"€29"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":183.855,"d":"€184"}}]

{"sheet":"09342671GA08","index":236,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671GA08","LEIPZIGER STRAßE","6,00","6,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["5,90","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["5,90","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["6,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6,2,{"$f":"H14*I14","v":{"v":12,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6,3,{"$f":"H15*I15","v":{"v":18,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":30,"d":"€30"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":5.7,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":35.7,"d":"€36"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671GA08","LEIPZIGER STRAßE","6,00","6,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["5,90","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["5,90","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["6,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6,2,{"$f":"H36*I36","v":{"v":12,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6,3,{"$f":"H37*I37","v":{"v":18,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":30,"d":"€30"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":5.7,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":35.7,"d":"€36"}}]

{"sheet":"09342671SE03","index":237,"n_rows":50,"n_cols":10,"rows_kept":50}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671SE03","LEIPZIGER STRAßE","4,80","5,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAC","B","15,00","8 - 4",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["0,20","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,20","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,40","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,40","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["3,40","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["3,40","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["4,60","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["4,80","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J14)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H16/100)*J15","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H17/100)*J15","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H18/100)*J15","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.8,2,{"$f":"H19*I19","v":{"v":9.6,"d":"€10"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.8,3,{"$f":"H20*I20","v":{"v":14.399999999999999,"d":"€14"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J15:J20)","v":{"v":24,"d":"€24"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H22/100)*J21","v":{"v":4.5600000000000005,"d":"€5"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J21:J22)","v":{"v":28.560000000000002,"d":"€29"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342671SE03","LEIPZIGER STRAßE","4,80","5,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAC","B","15,00","8 - 4",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["0,20","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,20","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,40","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,40","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["3,40","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["3,40","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["4,60","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["4,80","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J32:J41)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H43/100)*J42","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H44/100)*J42","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H45/100)*J42","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.8,2,{"$f":"H46*I46","v":{"v":9.6,"d":"€10"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.8,3,{"$f":"H47*I47","v":{"v":14.399999999999999,"d":"€14"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J42:J47)","v":{"v":24,"d":"€24"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H49/100)*J48","v":{"v":4.5600000000000005,"d":"€5"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J48:J49)","v":{"v":28.560000000000002,"d":"€29"}}]

{"sheet":"09342829GA01","index":238,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829GA01","BERLINER STRAßE","1,70","1,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["0,70","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["0,70","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["0,70","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["1,50","BCC","Y / A","15,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,60","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.7,2,{"$f":"H17*I17","v":{"v":3.4,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.7,3,{"$f":"H18*I18","v":{"v":5.1,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":8.5,"d":"€9"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":1.615,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":10.115,"d":"€10"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829GA01","BERLINER STRAßE","1,70","1,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["0,70","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["0,70","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["0,70","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["1,50","BCC","Y / A","15,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,60","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.7,2,{"$f":"H42*I42","v":{"v":3.4,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.7,3,{"$f":"H43*I43","v":{"v":5.1,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":8.5,"d":"€9"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":1.615,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":10.115,"d":"€10"}}]

{"sheet":"09342829GA03","index":239,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829GA03","BERLINER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["0,60","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["0,60","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["0,90","BAI","A / C",null,"12 - 12","JA","Einragendes Dichtungsmaterial Dichtring einragend, aber nicht gebrochen - tiefster Punkt liegt unterhalb der horizontale Mittellinie",null,"Fräsen",{"v":50,"d":"€50"}]
["0,90","BAJ","A","60,00","12 - 12","JA","Verschobene Verbindung in längsrichtung ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H16*I16","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H17*I17","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":132.5,"d":"€133"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":25.175,"d":"€25"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":157.675,"d":"€158"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829GA03","BERLINER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["0,60","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["0,60","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["0,90","BAI","A / C",null,"12 - 12","JA","Einragendes Dichtungsmaterial Dichtring einragend, aber nicht gebrochen - tiefster Punkt liegt unterhalb der horizontale Mittellinie"]
["0,90","BAJ","A","60,00","12 - 12","JA","Verschobene Verbindung in längsrichtung ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H40*I40","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H41*I41","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":69,"d":"€69"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":13.11,"d":"€13"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":82.11,"d":"€82"}}]

{"sheet":"09342829GA05","index":240,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829GA05","BERLINER STRAßE","1,20","1,20","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.2,2,{"$f":"H12*I12","v":{"v":2.4,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.2,3,{"$f":"H13*I13","v":{"v":3.5999999999999996,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":6,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":1.1400000000000001,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":7.140000000000001,"d":"€7"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829GA05","BERLINER STRAßE","1,20","1,20","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.2,2,{"$f":"H32*I32","v":{"v":2.4,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.2,3,{"$f":"H33*I33","v":{"v":3.5999999999999996,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":6,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":1.1400000000000001,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":7.140000000000001,"d":"€7"}}]

{"sheet":"09342829GA09","index":241,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829GA09","BERLINER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"125","PVC"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H11*I11","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H12*I12","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":6.545,"d":"€7"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829GA09","BERLINER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"125","PVC"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H30*I30","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H31*I31","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":6.545,"d":"€7"}}]

{"sheet":"09342829GA10","index":242,"n_rows":56,"n_cols":10,"rows_kept":56}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829GA10","BERLINER STRAßE","3,60","3,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,40","BAI","Z","15,00","5 - 7",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A","Fräsen",{"v":50,"d":"€50"}]
["0,80","BAI","Z","15,00","5 - 7",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B","Fräsen",{"v":50,"d":"€50"}]
["0,80","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,50","BAI","Z","15,00","5 - 7","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,70","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["2,50","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,70","BBC","C","3,00","3 - 9",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["3,40","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["3,40","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["3,40","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,60","BBC","C","3,00","3 - 9",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["3,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J17)","v":{"v":350,"d":"€350"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H19/100)*J18","v":{"v":35,"d":"€35"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H20/100)*J18","v":{"v":17.5,"d":"€18"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H21/100)*J18","v":{"v":42,"d":"€42"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.6,2,{"$f":"H22*I22","v":{"v":7.2,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.6,3,{"$f":"H23*I23","v":{"v":10.8,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J18:J23)","v":{"v":462.5,"d":"€463"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H25/100)*J24","v":{"v":87.875,"d":"€88"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J24:J25)","v":{"v":550.375,"d":"€550"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829GA10","BERLINER STRAßE","3,60","3,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,40","BAI","Z","15,00","5 - 7",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A"]
["0,80","BAI","Z","15,00","5 - 7",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B"]
["0,80","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,50","BAI","Z","15,00","5 - 7","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["1,70","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["2,50","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,70","BBC","C","3,00","3 - 9",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["3,40","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["3,40","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["3,40","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,60","BBC","C","3,00","3 - 9",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["3,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J35:J47)","v":{"v":200,"d":"€200"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H49/100)*J48","v":{"v":20,"d":"€20"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H50/100)*J48","v":{"v":10,"d":"€10"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H51/100)*J48","v":{"v":24,"d":"€24"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.6,2,{"$f":"H52*I52","v":{"v":7.2,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.6,3,{"$f":"H53*I53","v":{"v":10.8,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J48:J53)","v":{"v":272,"d":"€272"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H55/100)*J54","v":{"v":51.68,"d":"€52"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J54:J55)","v":{"v":323.68,"d":"€324"}}]

{"sheet":"09342829GA11","index":243,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829GA11","BERLINER STRAßE","3,50","3,50","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,40","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["2,40","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["3,10","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H14*I14","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H15*I15","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":17.5,"d":"€18"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":3.325,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":20.825,"d":"€21"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829GA11","BERLINER STRAßE","3,50","3,50","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,40","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["2,40","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["3,10","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H36*I36","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H37*I37","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":17.5,"d":"€18"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":3.325,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":20.825,"d":"€21"}}]

{"sheet":"09342829NN07","index":244,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829NN07","BERLINER STRAßE","0,10","0,10","Not Implemented yet",{"$nulls":3},"100","PVC"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.1,2,{"$f":"H11*I11","v":{"v":0.2,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.1,3,{"$f":"H12*I12","v":{"v":0.30000000000000004,"d":"€0"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":0.5,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.095,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":0.595,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829NN07","BERLINER STRAßE","0,10","0,10","Not Implemented yet",{"$nulls":3},"100","PVC"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.1,2,{"$f":"H30*I30","v":{"v":0.2,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.1,3,{"$f":"H31*I31","v":{"v":0.30000000000000004,"d":"€0"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":0.5,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.095,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":0.595,"d":"€1"}}]

{"sheet":"09342829RS02","index":245,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829RS02","BERLINER STRAßE","3,60","3,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,60","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["2,30","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,40","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["3,60","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.6,2,{"$f":"H14*I14","v":{"v":7.2,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.6,3,{"$f":"H15*I15","v":{"v":10.8,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":81.5,"d":"€82"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":15.485,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":96.985,"d":"€97"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829RS02","BERLINER STRAßE","3,60","3,90","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,60","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["2,30","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,40","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["3,60","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.6,2,{"$f":"H36*I36","v":{"v":7.2,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.6,3,{"$f":"H37*I37","v":{"v":10.8,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":81.5,"d":"€82"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":15.485,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":96.985,"d":"€97"}}]

{"sheet":"09342829RS04","index":246,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829RS04","BERLINER STRAßE","3,70","4,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,80","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,30","BAI","Z","10,00","5 - 7",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A","Fräsen",{"v":50,"d":"€50"}]
["1,50","BAJ","B","10,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,60","BAI","Z","10,00","5 - 7",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B","Fräsen",{"v":50,"d":"€50"}]
["3,40","BBE","B","20,00","4 - 8",null,"Andere Hindernisse Bruchstücke einer Abwasserleitung oder eines Abwasserkanals liegen in der \r\nRohrsohle "]
["3,60","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["3,70","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":200,"d":"€200"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":20,"d":"€20"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":10,"d":"€10"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":24,"d":"€24"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.7,2,{"$f":"H17*I17","v":{"v":7.4,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.7,3,{"$f":"H18*I18","v":{"v":11.100000000000001,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":272.5,"d":"€273"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":51.775,"d":"€52"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":324.275,"d":"€324"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829RS04","BERLINER STRAßE","3,70","4,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,80","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,30","BAI","Z","10,00","5 - 7",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A"]
["1,50","BAJ","B","10,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,60","BAI","Z","10,00","5 - 7",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B"]
["3,40","BBE","B","20,00","4 - 8",null,"Andere Hindernisse Bruchstücke einer Abwasserleitung oder eines Abwasserkanals liegen in der \r\nRohrsohle "]
["3,60","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["3,70","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.7,2,{"$f":"H42*I42","v":{"v":7.4,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.7,3,{"$f":"H43*I43","v":{"v":11.100000000000001,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":145.5,"d":"€146"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":27.645,"d":"€28"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":173.145,"d":"€173"}}]

{"sheet":"09342829RS06","index":247,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829RS06","BERLINER STRAßE","3,50","3,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,80","BAI","Z","15,00","5 - 7",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A","Fräsen",{"v":50,"d":"€50"}]
["1,50","BAI","Z","15,00","5 - 7",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B","Fräsen",{"v":50,"d":"€50"}]
["1,50","BAJ","C","10,00","6","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,50","BAJ","B","20,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,40","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["3,50","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":200,"d":"€200"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":20,"d":"€20"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":10,"d":"€10"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":24,"d":"€24"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H16*I16","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H17*I17","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":271.5,"d":"€272"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":51.585,"d":"€52"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":323.085,"d":"€323"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829RS06","BERLINER STRAßE","3,50","3,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,80","BAI","Z","15,00","5 - 7",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A"]
["1,50","BAI","Z","15,00","5 - 7",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B"]
["1,50","BAJ","C","10,00","6","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,50","BAJ","B","20,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,40","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["3,50","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H40*I40","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H41*I41","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":144.5,"d":"€145"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":27.455000000000002,"d":"€27"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":171.955,"d":"€172"}}]

{"sheet":"09342829RS08","index":248,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829RS08","BERLINER STRAßE","3,10","3,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,70","BAJ","B","10,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,40","BAJ","C","15,00","6","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,40","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,10","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["3,10","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":150,"d":"€150"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H15*I15","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H16*I16","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":206,"d":"€206"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":39.14,"d":"€39"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":245.14,"d":"€245"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342829RS08","BERLINER STRAßE","3,10","3,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,70","BAJ","B","10,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,40","BAJ","C","15,00","6","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,40","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,10","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["3,10","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":150,"d":"€150"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H38*I38","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H39*I39","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":206,"d":"€206"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":39.14,"d":"€39"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":245.14,"d":"€245"}}]

{"sheet":"09342831GA02","index":249,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831GA02","LEIPZIGER STRAßE","2,80","2,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBC","C","2,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["2,80","BBC","C","2,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["2,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.8,2,{"$f":"H13*I13","v":{"v":5.6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.8,3,{"$f":"H14*I14","v":{"v":8.399999999999999,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":141,"d":"€141"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":26.79,"d":"€27"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":167.79,"d":"€168"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831GA02","LEIPZIGER STRAßE","2,80","2,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBC","C","2,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["2,80","BBC","C","2,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["2,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.8,2,{"$f":"H34*I34","v":{"v":5.6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.8,3,{"$f":"H35*I35","v":{"v":8.399999999999999,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":141,"d":"€141"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":26.79,"d":"€27"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":167.79,"d":"€168"}}]

{"sheet":"09342831GA04","index":250,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831GA04","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H11*I11","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H12*I12","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":16.065,"d":"€16"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831GA04","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H30*I30","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H31*I31","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":16.065,"d":"€16"}}]

{"sheet":"09342831GA06","index":251,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831GA06","LEIPZIGER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,00","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,20","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["3,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H13*I13","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H14*I14","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":18.445,"d":"€18"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831GA06","LEIPZIGER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,00","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,20","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["3,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H34*I34","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H35*I35","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":18.445,"d":"€18"}}]

{"sheet":"09342831GA08","index":252,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831GA08","LEIPZIGER STRAßE","2,60","2,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.6,2,{"$f":"H11*I11","v":{"v":5.2,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.6,3,{"$f":"H12*I12","v":{"v":7.800000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":13,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":2.47,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":15.47,"d":"€15"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831GA08","LEIPZIGER STRAßE","2,60","2,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.6,2,{"$f":"H30*I30","v":{"v":5.2,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.6,3,{"$f":"H31*I31","v":{"v":7.800000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":13,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":2.47,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":15.47,"d":"€15"}}]

{"sheet":"09342831GA10","index":253,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831GA10","LEIPZIGER STRAßE","2,40","2,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,80","BCC","A / Y","30,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.4,2,{"$f":"H12*I12","v":{"v":4.8,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.4,3,{"$f":"H13*I13","v":{"v":7.199999999999999,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":12,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.2800000000000002,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":14.280000000000001,"d":"€14"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831GA10","LEIPZIGER STRAßE","2,40","2,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,80","BCC","A / Y","30,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.4,2,{"$f":"H32*I32","v":{"v":4.8,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.4,3,{"$f":"H33*I33","v":{"v":7.199999999999999,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":12,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.2800000000000002,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":14.280000000000001,"d":"€14"}}]

{"sheet":"09342831NN03","index":254,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831NN03","LEIPZIGER STRAßE","3,80","3,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,50","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,50","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,50","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,80","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,00","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,80","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.8,2,{"$f":"H17*I17","v":{"v":7.6,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.8,3,{"$f":"H18*I18","v":{"v":11.399999999999999,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":19,"d":"€19"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":3.61,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":22.61,"d":"€23"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831NN03","LEIPZIGER STRAßE","3,80","3,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,50","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,50","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,50","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,80","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,00","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,80","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.8,2,{"$f":"H42*I42","v":{"v":7.6,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.8,3,{"$f":"H43*I43","v":{"v":11.399999999999999,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":19,"d":"€19"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":3.61,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":22.61,"d":"€23"}}]

{"sheet":"09342831RR01","index":255,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831RR01","LEIPZIGER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["1,70","BBA","B","3,00","2 - 10","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,70","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,70","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["3,10","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H17*I17","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H18*I18","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":79.5,"d":"€80"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":15.105,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":94.605,"d":"€95"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831RR01","LEIPZIGER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["1,70","BBA","B","3,00","2 - 10","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,70","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,70","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["3,10","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H42*I42","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H43*I43","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":79.5,"d":"€80"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":15.105,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":94.605,"d":"€95"}}]

{"sheet":"09342831RR05","index":256,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831RR05","LEIPZIGER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,70","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,90","BAI","A / B",null,"9 - 11","JA","Einragendes Dichtungsmaterial Dichtring einragend, aber nicht gebrochen - tiefster Punkt liegt oberhalb der horizontale Mittellinie",null,"Fräsen",{"v":50,"d":"€50"}]
["2,90","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H15*I15","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H16*I16","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":79,"d":"€79"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":15.01,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":94.01,"d":"€94"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831RR05","LEIPZIGER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,70","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,90","BAI","A / B",null,"9 - 11","JA","Einragendes Dichtungsmaterial Dichtring einragend, aber nicht gebrochen - tiefster Punkt liegt oberhalb der horizontale Mittellinie"]
["2,90","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H38*I38","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H39*I39","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":18.445,"d":"€18"}}]

{"sheet":"09342831RR07","index":257,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831RR07","LEIPZIGER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["0,70","AED","PVCU",{"$nulls":3},"Grundlagen änderung  "]
["2,90","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,00","BCC","Y / A","15,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCC","Y / A","15,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H16*I16","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H17*I17","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":18.445,"d":"€18"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831RR07","LEIPZIGER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["0,70","AED","PVCU",{"$nulls":3},"Grundlagen änderung  "]
["2,90","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,00","BCC","Y / A","15,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCC","Y / A","15,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H40*I40","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H41*I41","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":18.445,"d":"€18"}}]

{"sheet":"09342831RR09","index":258,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831RR09","LEIPZIGER STRAßE","3,40","3,40","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,60","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,60","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["2,60","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,90","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCC","Y / A","15,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,40","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.4,2,{"$f":"H16*I16","v":{"v":6.8,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.4,3,{"$f":"H17*I17","v":{"v":10.2,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":17,"d":"€17"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":3.23,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":20.23,"d":"€20"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342831RR09","LEIPZIGER STRAßE","3,40","3,40","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,60","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,60","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["2,60","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,90","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCC","Y / A","15,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,40","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.4,2,{"$f":"H40*I40","v":{"v":6.8,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.4,3,{"$f":"H41*I41","v":{"v":10.2,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":17,"d":"€17"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":3.23,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":20.23,"d":"€20"}}]

{"sheet":"09342832GA02","index":259,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832GA02","LEIPZIGER STRAßE","3,40","3,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,50","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,60","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["3,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.4,2,{"$f":"H13*I13","v":{"v":6.8,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.4,3,{"$f":"H14*I14","v":{"v":10.2,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":17,"d":"€17"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":3.23,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":20.23,"d":"€20"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832GA02","LEIPZIGER STRAßE","3,40","3,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,50","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,60","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["3,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.4,2,{"$f":"H34*I34","v":{"v":6.8,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.4,3,{"$f":"H35*I35","v":{"v":10.2,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":17,"d":"€17"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":3.23,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":20.23,"d":"€20"}}]

{"sheet":"09342832GA04","index":260,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832GA04","LEIPZIGER STRAßE","2,40","2,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.4,2,{"$f":"H11*I11","v":{"v":4.8,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.4,3,{"$f":"H12*I12","v":{"v":7.199999999999999,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":12,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":2.2800000000000002,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":14.280000000000001,"d":"€14"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832GA04","LEIPZIGER STRAßE","2,40","2,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.4,2,{"$f":"H30*I30","v":{"v":4.8,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.4,3,{"$f":"H31*I31","v":{"v":7.199999999999999,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":12,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":2.2800000000000002,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":14.280000000000001,"d":"€14"}}]

{"sheet":"09342832GA06","index":261,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832GA06","LEIPZIGER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,00","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,00","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H13*I13","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H14*I14","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":12.5,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":2.375,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":14.875,"d":"€15"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832GA06","LEIPZIGER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,00","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,00","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H34*I34","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H35*I35","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":12.5,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":2.375,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":14.875,"d":"€15"}}]

{"sheet":"09342832GA08","index":262,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832GA08","LEIPZIGER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H11*I11","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H12*I12","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":12.5,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":2.375,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":14.875,"d":"€15"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832GA08","LEIPZIGER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H30*I30","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H31*I31","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":12.5,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":2.375,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":14.875,"d":"€15"}}]

{"sheet":"09342832GA10","index":263,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832GA10","LEIPZIGER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H11*I11","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H12*I12","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":12.5,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":2.375,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":14.875,"d":"€15"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832GA10","LEIPZIGER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H30*I30","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H31*I31","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":12.5,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":2.375,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":14.875,"d":"€15"}}]

{"sheet":"09342832RR01","index":264,"n_rows":48,"n_cols":10,"rows_kept":48}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832RR01","LEIPZIGER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["0,90","BBA","B","2,00","4 - 8","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,40","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,40","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["2,40","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,40","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["3,00","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J13)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H15/100)*J14","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H16/100)*J14","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H17/100)*J14","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H18*I18","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H19*I19","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J14:J19)","v":{"v":79.5,"d":"€80"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H21/100)*J20","v":{"v":15.105,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J20:J21)","v":{"v":94.605,"d":"€95"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832RR01","LEIPZIGER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["0,90","BBA","B","2,00","4 - 8","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,40","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,40","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["2,40","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,40","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["3,00","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J31:J39)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H44*I44","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H45*I45","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":79.5,"d":"€80"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":15.105,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":94.605,"d":"€95"}}]

{"sheet":"09342832RR03","index":265,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832RR03","LEIPZIGER STRAßE","3,30","3,30","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,80","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["3,20","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.3,2,{"$f":"H14*I14","v":{"v":6.6,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.3,3,{"$f":"H15*I15","v":{"v":9.899999999999999,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":16.5,"d":"€17"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":3.1350000000000002,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":19.635,"d":"€20"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832RR03","LEIPZIGER STRAßE","3,30","3,30","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,80","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["3,20","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.3,2,{"$f":"H36*I36","v":{"v":6.6,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.3,3,{"$f":"H37*I37","v":{"v":9.899999999999999,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":16.5,"d":"€17"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":3.1350000000000002,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":19.635,"d":"€20"}}]

{"sheet":"09342832RR05","index":266,"n_rows":48,"n_cols":10,"rows_kept":48}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832RR05","LEIPZIGER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["1,40","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,40","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,40","AED","PVCU",{"$nulls":3},"Grundlagen änderung  "]
["1,40","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["2,10","BCC","Y / B","15,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["3,00","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J13)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H15/100)*J14","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H16/100)*J14","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H17/100)*J14","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H18*I18","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H19*I19","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J14:J19)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H21/100)*J20","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J20:J21)","v":{"v":18.445,"d":"€18"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832RR05","LEIPZIGER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["1,40","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,40","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,40","AED","PVCU",{"$nulls":3},"Grundlagen änderung  "]
["1,40","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["2,10","BCC","Y / B","15,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["3,00","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J31:J39)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H44*I44","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H45*I45","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":18.445,"d":"€18"}}]

{"sheet":"09342832RR07","index":267,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832RR07","LEIPZIGER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["2,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,70","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,70","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["3,10","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H16*I16","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H17*I17","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":16,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":3.04,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":19.04,"d":"€19"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832RR07","LEIPZIGER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["2,70","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,70","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,70","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["3,10","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H40*I40","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H41*I41","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":16,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":3.04,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":19.04,"d":"€19"}}]

{"sheet":"09342832RR09","index":268,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832RR09","LEIPZIGER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,80","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["3,10","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H14*I14","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H15*I15","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":16,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":3.04,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":19.04,"d":"€19"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342832RR09","LEIPZIGER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,80","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["3,10","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H36*I36","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H37*I37","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":16,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":3.04,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":19.04,"d":"€19"}}]

{"sheet":"09342833GA02","index":269,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342833GA02","LEIPZIGER STRAßE","1,20","1,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.2,2,{"$f":"H11*I11","v":{"v":2.4,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.2,3,{"$f":"H12*I12","v":{"v":3.5999999999999996,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":6,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":1.1400000000000001,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":7.140000000000001,"d":"€7"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342833GA02","LEIPZIGER STRAßE","1,20","1,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.2,2,{"$f":"H30*I30","v":{"v":2.4,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.2,3,{"$f":"H31*I31","v":{"v":3.5999999999999996,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":6,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":1.1400000000000001,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":7.140000000000001,"d":"€7"}}]

{"sheet":"09342833GA03","index":270,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342833GA03","LEIPZIGER STRAßE","1,30","1,30","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,30","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.3,2,{"$f":"H11*I11","v":{"v":2.6,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.3,3,{"$f":"H12*I12","v":{"v":3.9000000000000004,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":6.5,"d":"€7"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":1.235,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":7.735,"d":"€8"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342833GA03","LEIPZIGER STRAßE","1,30","1,30","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,30","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.3,2,{"$f":"H30*I30","v":{"v":2.6,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.3,3,{"$f":"H31*I31","v":{"v":3.9000000000000004,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":6.5,"d":"€7"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":1.235,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":7.735,"d":"€8"}}]

{"sheet":"09342833GA04","index":271,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342833GA04","LEIPZIGER STRAßE","1,20","1,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.2,2,{"$f":"H11*I11","v":{"v":2.4,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.2,3,{"$f":"H12*I12","v":{"v":3.5999999999999996,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":6,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":1.1400000000000001,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":7.140000000000001,"d":"€7"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342833GA04","LEIPZIGER STRAßE","1,20","1,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.2,2,{"$f":"H30*I30","v":{"v":2.4,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.2,3,{"$f":"H31*I31","v":{"v":3.5999999999999996,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":6,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":1.1400000000000001,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":7.140000000000001,"d":"€7"}}]

{"sheet":"09342833GA05","index":272,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342833GA05","LEIPZIGER STRAßE","2,80","2,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen"]
["2,80","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.8,2,{"$f":"H13*I13","v":{"v":5.6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.8,3,{"$f":"H14*I14","v":{"v":8.399999999999999,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":13.999999999999998,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":2.6599999999999997,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":16.659999999999997,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342833GA05","LEIPZIGER STRAßE","2,80","2,80","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCA","A / A","150,00","9",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["2,80","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,80","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":490,"d":"€490"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":49,"d":"€49"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":24.5,"d":"€25"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":58.8,"d":"€59"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.8,2,{"$f":"H34*I34","v":{"v":5.6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.8,3,{"$f":"H35*I35","v":{"v":8.399999999999999,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":636.3,"d":"€636"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":120.89699999999999,"d":"€121"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":757.1969999999999,"d":"€757"}}]

{"sheet":"09342833GA06","index":273,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342833GA06","LEIPZIGER STRAßE","2,40","2,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,40","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,40","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,40","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["2,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.4,2,{"$f":"H14*I14","v":{"v":4.8,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.4,3,{"$f":"H15*I15","v":{"v":7.199999999999999,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":12,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":2.2800000000000002,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":14.280000000000001,"d":"€14"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342833GA06","LEIPZIGER STRAßE","2,40","2,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,40","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,40","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,40","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["2,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.4,2,{"$f":"H36*I36","v":{"v":4.8,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.4,3,{"$f":"H37*I37","v":{"v":7.199999999999999,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":12,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":2.2800000000000002,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":14.280000000000001,"d":"€14"}}]

{"sheet":"09342833GA07","index":274,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342833GA07","LEIPZIGER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H12*I12","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H13*I13","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":6.545,"d":"€7"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342833GA07","LEIPZIGER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H32*I32","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H33*I33","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":6.545,"d":"€7"}}]

{"sheet":"09342833NN01","index":275,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342833NN01","LEIPZIGER STRAßE","2,80","2,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["0,80","BAC","B","50,00","4 - 8","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["0,80","BAP",null,null,"4 - 8","JA","Hohlraum sichtbar  "]
["2,70","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["2,70","BAC","B","300,00","12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["2,80","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.8,2,{"$f":"H16*I16","v":{"v":5.6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.8,3,{"$f":"H17*I17","v":{"v":8.399999999999999,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":13.999999999999998,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":2.6599999999999997,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":16.659999999999997,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342833NN01","LEIPZIGER STRAßE","2,80","2,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["0,80","BAC","B","50,00","4 - 8","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["0,80","BAP",null,null,"4 - 8","JA","Hohlraum sichtbar  "]
["2,70","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["2,70","BAC","B","300,00","12 - 12",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["2,80","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.8,2,{"$f":"H40*I40","v":{"v":5.6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.8,3,{"$f":"H41*I41","v":{"v":8.399999999999999,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":13.999999999999998,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":2.6599999999999997,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":16.659999999999997,"d":"€17"}}]

{"sheet":"09342834GA01","index":276,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834GA01","LEIPZIGER STRAßE","4,70","4,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.7,2,{"$f":"H11*I11","v":{"v":9.4,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.7,3,{"$f":"H12*I12","v":{"v":14.100000000000001,"d":"€14"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":23.5,"d":"€24"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":4.465,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":27.965,"d":"€28"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834GA01","LEIPZIGER STRAßE","4,70","4,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.7,2,{"$f":"H30*I30","v":{"v":9.4,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.7,3,{"$f":"H31*I31","v":{"v":14.100000000000001,"d":"€14"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":23.5,"d":"€24"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":4.465,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":27.965,"d":"€28"}}]

{"sheet":"09342834RS04","index":277,"n_rows":48,"n_cols":10,"rows_kept":48}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834RS04","LEIPZIGER STRAßE","3,70","3,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,70","BAB","B / A","3,00","6",null,"Rissbildung Riss in Längsrichtung","A"]
["1,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,80","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,80","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["1,80","BAB","B / A","3,00","6",null,"Rissbildung Riss in Längsrichtung","B"]
["1,80","BBA","C","5,00","12 - 12","JA","Wurzeln komplexes Wurzelwerk ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,90","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["3,70","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J13)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H15/100)*J14","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H16/100)*J14","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H17/100)*J14","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.7,2,{"$f":"H18*I18","v":{"v":7.4,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.7,3,{"$f":"H19*I19","v":{"v":11.100000000000001,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J14:J19)","v":{"v":82,"d":"€82"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H21/100)*J20","v":{"v":15.58,"d":"€16"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J20:J21)","v":{"v":97.58,"d":"€98"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834RS04","LEIPZIGER STRAßE","3,70","3,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,70","BAB","B / A","3,00","6",null,"Rissbildung Riss in Längsrichtung","A"]
["1,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,80","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,80","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["1,80","BAB","B / A","3,00","6",null,"Rissbildung Riss in Längsrichtung","B"]
["1,80","BBA","C","5,00","12 - 12","JA","Wurzeln komplexes Wurzelwerk ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,90","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["3,70","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J31:J39)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.7,2,{"$f":"H44*I44","v":{"v":7.4,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.7,3,{"$f":"H45*I45","v":{"v":11.100000000000001,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":82,"d":"€82"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":15.58,"d":"€16"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":97.58,"d":"€98"}}]

{"sheet":"09342834RS07","index":278,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834RS07","LEIPZIGER STRAßE","3,50","3,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,90","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,20","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["2,20","AED","PP",{"$nulls":3},"Grundlagen änderung  "]
["3,50","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H15*I15","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H16*I16","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":81,"d":"€81"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":15.39,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":96.39,"d":"€96"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834RS07","LEIPZIGER STRAßE","3,50","3,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,90","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,20","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["2,20","AED","PP",{"$nulls":3},"Grundlagen änderung  "]
["3,50","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H38*I38","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H39*I39","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":81,"d":"€81"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":15.39,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":96.39,"d":"€96"}}]

{"sheet":"09342834RS09","index":279,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834RS09","LEIPZIGER STRAßE","3,10","3,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,10","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,10","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,10","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,10","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["3,10","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H15*I15","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H16*I16","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":18.445,"d":"€18"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834RS09","LEIPZIGER STRAßE","3,10","3,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,10","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,10","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,10","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,10","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["3,10","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H38*I38","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H39*I39","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":18.445,"d":"€18"}}]

{"sheet":"09342834RV03","index":280,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834RV03","LEIPZIGER STRAßE","5,10","5,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["0,80","BBA","C","20,00","4 - 8",null,"Wurzeln komplexes Wurzelwerk ","A","Fräsen",{"v":50,"d":"€50"}]
["2,60","BBA","C","20,00","4 - 8",null,"Wurzeln komplexes Wurzelwerk ","C","Fräsen",{"v":50,"d":"€50"}]
["3,00","BBE","C",null,"4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["3,00","BBA","C",null,"4 - 8",null,"Wurzeln komplexes Wurzelwerk ","B","Fräsen",{"v":50,"d":"€50"}]
["5,10","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["5,10","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":150,"d":"€150"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.1,2,{"$f":"H17*I17","v":{"v":10.2,"d":"€10"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.1,3,{"$f":"H18*I18","v":{"v":15.299999999999999,"d":"€15"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":216,"d":"€216"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":41.04,"d":"€41"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":257.04,"d":"€257"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834RV03","LEIPZIGER STRAßE","5,10","5,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["0,80","BBA","C","20,00","4 - 8",null,"Wurzeln komplexes Wurzelwerk ","A","Fräsen",{"v":50,"d":"€50"}]
["2,60","BBA","C","20,00","4 - 8",null,"Wurzeln komplexes Wurzelwerk ","C","Fräsen",{"v":50,"d":"€50"}]
["3,00","BBE","C",null,"4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["3,00","BBA","C",null,"4 - 8",null,"Wurzeln komplexes Wurzelwerk ","B","Fräsen",{"v":50,"d":"€50"}]
["5,10","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["5,10","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":150,"d":"€150"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.1,2,{"$f":"H42*I42","v":{"v":10.2,"d":"€10"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.1,3,{"$f":"H43*I43","v":{"v":15.299999999999999,"d":"€15"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":216,"d":"€216"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":41.04,"d":"€41"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":257.04,"d":"€257"}}]

{"sheet":"09342834RV05","index":281,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834RV05","LEIPZIGER STRAßE","4,90","4,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["3,40","BBA","C","15,00","4 - 8","JA","Wurzeln komplexes Wurzelwerk ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,90","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["4,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.9,2,{"$f":"H13*I13","v":{"v":9.8,"d":"€10"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.9,3,{"$f":"H14*I14","v":{"v":14.700000000000001,"d":"€15"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":88,"d":"€88"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":16.72,"d":"€17"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":104.72,"d":"€105"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834RV05","LEIPZIGER STRAßE","4,90","4,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["3,40","BBA","C","15,00","4 - 8","JA","Wurzeln komplexes Wurzelwerk ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,90","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["4,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.9,2,{"$f":"H34*I34","v":{"v":9.8,"d":"€10"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.9,3,{"$f":"H35*I35","v":{"v":14.700000000000001,"d":"€15"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":88,"d":"€88"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":16.72,"d":"€17"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":104.72,"d":"€105"}}]

{"sheet":"09342834RV08","index":282,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834RV08","LEIPZIGER STRAßE","3,60","3,60","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["3,60","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["3,60","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.6,2,{"$f":"H12*I12","v":{"v":7.2,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.6,3,{"$f":"H13*I13","v":{"v":10.8,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":18,"d":"€18"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":3.42,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":21.42,"d":"€21"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834RV08","LEIPZIGER STRAßE","3,60","3,60","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["3,60","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["3,60","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.6,2,{"$f":"H32*I32","v":{"v":7.2,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.6,3,{"$f":"H33*I33","v":{"v":10.8,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":18,"d":"€18"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":3.42,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":21.42,"d":"€21"}}]

{"sheet":"09342834SE02","index":283,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834SE02","LEIPZIGER STRAßE","3,50","3,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["3,50","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H12*I12","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H13*I13","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":17.5,"d":"€18"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":3.325,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":20.825,"d":"€21"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342834SE02","LEIPZIGER STRAßE","3,50","3,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["3,50","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H32*I32","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H33*I33","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":17.5,"d":"€18"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":3.325,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":20.825,"d":"€21"}}]

{"sheet":"09342838GA01","index":284,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838GA01","BERLINER STRAßE","1,60","1,60","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["1,60","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["1,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.6,2,{"$f":"H13*I13","v":{"v":3.2,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.6,3,{"$f":"H14*I14","v":{"v":4.800000000000001,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":8,"d":"€8"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":1.52,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":9.52,"d":"€10"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838GA01","BERLINER STRAßE","1,60","1,60","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["1,60","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["1,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.6,2,{"$f":"H34*I34","v":{"v":3.2,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.6,3,{"$f":"H35*I35","v":{"v":4.800000000000001,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":8,"d":"€8"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":1.52,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":9.52,"d":"€10"}}]

{"sheet":"09342838GA03","index":285,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838GA03","BERLINER STRAßE","1,20","1,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,10","BAC","B","100,00","3 - 6","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["1,10","BAP",null,null,"3 - 6","JA","Hohlraum sichtbar  "]
["1,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.2,2,{"$f":"H13*I13","v":{"v":2.4,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.2,3,{"$f":"H14*I14","v":{"v":3.5999999999999996,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":6,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":1.1400000000000001,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":7.140000000000001,"d":"€7"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838GA03","BERLINER STRAßE","1,20","1,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,10","BAC","B","100,00","3 - 6","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["1,10","BAP",null,null,"3 - 6","JA","Hohlraum sichtbar  "]
["1,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.2,2,{"$f":"H34*I34","v":{"v":2.4,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.2,3,{"$f":"H35*I35","v":{"v":3.5999999999999996,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":6,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":1.1400000000000001,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":7.140000000000001,"d":"€7"}}]

{"sheet":"09342838GA05","index":286,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838GA05","BERLINER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","BAC","B","50,00","4 - 6","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["1,00","BAP",null,null,"4 - 6","JA","Hohlraum sichtbar  "]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H13*I13","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H14*I14","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":6.545,"d":"€7"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838GA05","BERLINER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","BAC","B","50,00","4 - 6","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["1,00","BAP",null,null,"4 - 6","JA","Hohlraum sichtbar  "]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H34*I34","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H35*I35","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":6.545,"d":"€7"}}]

{"sheet":"09342838GA07","index":287,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838GA07","BERLINER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["1,00","BAC","B","100,00","3 - 6","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["1,00","BAP",null,null,"3 - 9","JA","Hohlraum sichtbar  "]
["1,00","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H15*I15","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H16*I16","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":5.95,"d":"€6"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838GA07","BERLINER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["1,00","BAC","B","100,00","3 - 6","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["1,00","BAP",null,null,"3 - 9","JA","Hohlraum sichtbar  "]
["1,00","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H38*I38","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H39*I39","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":5.95,"d":"€6"}}]

{"sheet":"09342838GA09","index":288,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838GA09","BERLINER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H11*I11","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H12*I12","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":5.95,"d":"€6"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838GA09","BERLINER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H30*I30","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H31*I31","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":5.95,"d":"€6"}}]

{"sheet":"09342838GA10","index":289,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838GA10","BERLINER STRAßE","3,40","3,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / A","30,00","1",null,"Krümmung der Leitung nach rechts nach oben"]
["1,80","BAI","Z","5,00","5 - 7","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,00","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["3,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.4,2,{"$f":"H14*I14","v":{"v":6.8,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.4,3,{"$f":"H15*I15","v":{"v":10.2,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":80.5,"d":"€81"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":15.295,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":95.795,"d":"€96"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838GA10","BERLINER STRAßE","3,40","3,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / A","30,00","1",null,"Krümmung der Leitung nach rechts nach oben"]
["1,80","BAI","Z","5,00","5 - 7","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["2,00","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["3,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.4,2,{"$f":"H36*I36","v":{"v":6.8,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.4,3,{"$f":"H37*I37","v":{"v":10.2,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":17,"d":"€17"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":3.23,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":20.23,"d":"€20"}}]

{"sheet":"09342838NN11","index":290,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838NN11","BERLINER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,50","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["0,90","BAF","I / E",null,"4 - 8","JA","Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["0,90","BAP",null,null,"4 - 8","JA","Hohlraum sichtbar  "]
["3,00","BBE","C","50,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["3,10","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["3,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H16*I16","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H17*I17","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":18.445,"d":"€18"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838NN11","BERLINER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,50","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["0,90","BAF","I / E",null,"4 - 8","JA","Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["0,90","BAP",null,null,"4 - 8","JA","Hohlraum sichtbar  "]
["3,00","BBE","C","50,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["3,10","BAF","C / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["3,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H40*I40","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H41*I41","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":18.445,"d":"€18"}}]

{"sheet":"09342838RS02","index":291,"n_rows":48,"n_cols":10,"rows_kept":48}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838RS02","BERLINER STRAßE","4,30","4,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","BAI","Z","5,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A","Fräsen",{"v":50,"d":"€50"}]
["1,70","BAI","Z","5,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B","Fräsen",{"v":50,"d":"€50"}]
["1,90","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["2,00","BAJ","B","40,00","3","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,00","BAP",null,null,"6 - 12","JA","Hohlraum sichtbar  "]
["4,00","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,10","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["4,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J13)","v":{"v":200,"d":"€200"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H15/100)*J14","v":{"v":20,"d":"€20"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H16/100)*J14","v":{"v":10,"d":"€10"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H17/100)*J14","v":{"v":24,"d":"€24"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.3,2,{"$f":"H18*I18","v":{"v":8.6,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.3,3,{"$f":"H19*I19","v":{"v":12.899999999999999,"d":"€13"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J14:J19)","v":{"v":275.5,"d":"€276"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H21/100)*J20","v":{"v":52.345,"d":"€52"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J20:J21)","v":{"v":327.845,"d":"€328"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838RS02","BERLINER STRAßE","4,30","4,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","BAI","Z","5,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A"]
["1,70","BAI","Z","5,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B"]
["1,90","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["2,00","BAJ","B","40,00","3","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,00","BAP",null,null,"6 - 12","JA","Hohlraum sichtbar  "]
["4,00","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,10","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["4,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J31:J39)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.3,2,{"$f":"H44*I44","v":{"v":8.6,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.3,3,{"$f":"H45*I45","v":{"v":12.899999999999999,"d":"€13"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":148.5,"d":"€149"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":28.215,"d":"€28"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":176.715,"d":"€177"}}]

{"sheet":"09342838RS04","index":292,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838RS04","BERLINER STRAßE","4,30","4,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,90","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,10","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["4,00","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["4,10","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["4,30","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["4,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.3,2,{"$f":"H16*I16","v":{"v":8.6,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.3,3,{"$f":"H17*I17","v":{"v":12.899999999999999,"d":"€13"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":85,"d":"€85"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":16.15,"d":"€16"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":101.15,"d":"€101"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838RS04","BERLINER STRAßE","4,30","4,60","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,90","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,10","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["4,00","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["4,10","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["4,30","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["4,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.3,2,{"$f":"H40*I40","v":{"v":8.6,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.3,3,{"$f":"H41*I41","v":{"v":12.899999999999999,"d":"€13"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":85,"d":"€85"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":16.15,"d":"€16"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":101.15,"d":"€101"}}]

{"sheet":"09342838RS06","index":293,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838RS06","BERLINER STRAßE","4,20","4,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,60","BAI","Z","15,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A","Fräsen",{"v":50,"d":"€50"}]
["2,10","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["3,80","BAI","Z","15,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B","Fräsen",{"v":50,"d":"€50"}]
["4,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.2,2,{"$f":"H15*I15","v":{"v":8.4,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.2,3,{"$f":"H16*I16","v":{"v":12.600000000000001,"d":"€13"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":148,"d":"€148"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":28.12,"d":"€28"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":176.12,"d":"€176"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838RS06","BERLINER STRAßE","4,20","4,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,60","BAI","Z","15,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A"]
["2,10","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["3,80","BAI","Z","15,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B"]
["4,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.2,2,{"$f":"H38*I38","v":{"v":8.4,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.2,3,{"$f":"H39*I39","v":{"v":12.600000000000001,"d":"€13"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":21,"d":"€21"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":3.99,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":24.990000000000002,"d":"€25"}}]

{"sheet":"09342838RS08","index":294,"n_rows":56,"n_cols":10,"rows_kept":56}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838RS08","BERLINER STRAßE","3,90","4,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAI","Z","3,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A","Fräsen",{"v":50,"d":"€50"}]
["0,80","BAI","Z","10,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","C","Fräsen",{"v":50,"d":"€50"}]
["0,80","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,80","BAJ","C","15,00","12","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,70","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,70","BAC","B","200,00","10 - 2",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["1,70","BAP",null,null,"10 - 2",null,"Hohlraum sichtbar  "]
["1,70","BAC","A","200,00","12 - 12",null,"Rohrbruch / Einsturz Bruch "]
["2,20","BAI","Z","3,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","C","Fräsen",{"v":50,"d":"€50"}]
["3,70","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["3,70","BAI","Z","20,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B","Fräsen",{"v":50,"d":"€50"}]
["3,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J17)","v":{"v":300,"d":"€300"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H19/100)*J18","v":{"v":30,"d":"€30"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H20/100)*J18","v":{"v":15,"d":"€15"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H21/100)*J18","v":{"v":36,"d":"€36"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.9,2,{"$f":"H22*I22","v":{"v":7.8,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.9,3,{"$f":"H23*I23","v":{"v":11.7,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J18:J23)","v":{"v":400.5,"d":"€401"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H25/100)*J24","v":{"v":76.095,"d":"€76"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J24:J25)","v":{"v":476.595,"d":"€477"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342838RS08","BERLINER STRAßE","3,90","4,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAI","Z","3,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A"]
["0,80","BAI","Z","10,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","C"]
["0,80","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,80","BAJ","C","15,00","12","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,70","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,70","BAC","B","200,00","10 - 2",null,"Rohrbruch / Einsturz Fehlen von Teilen "]
["1,70","BAP",null,null,"10 - 2",null,"Hohlraum sichtbar  "]
["1,70","BAC","A","200,00","12 - 12",null,"Rohrbruch / Einsturz Bruch "]
["2,20","BAI","Z","3,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","C"]
["3,70","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["3,70","BAI","Z","20,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B"]
["3,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J35:J47)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H49/100)*J48","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H50/100)*J48","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H51/100)*J48","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.9,2,{"$f":"H52*I52","v":{"v":7.8,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.9,3,{"$f":"H53*I53","v":{"v":11.7,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J48:J53)","v":{"v":146.5,"d":"€147"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H55/100)*J54","v":{"v":27.835,"d":"€28"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J54:J55)","v":{"v":174.335,"d":"€174"}}]

{"sheet":"09342839GA01","index":295,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839GA01","BERLINER STRAßE","1,50","1,50","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["0,70","BAC","B","50,00","4 - 8","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["1,30","BAC","C",null,"4 - 8",null,"Rohrbruch / Einsturz Einsturz "]
["1,30","BAP",null,null,"4 - 8",null,"Hohlraum sichtbar  "]
["1,50","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["1,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.5,2,{"$f":"H16*I16","v":{"v":3,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.5,3,{"$f":"H17*I17","v":{"v":4.5,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":7.5,"d":"€8"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":1.425,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":8.925,"d":"€9"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839GA01","BERLINER STRAßE","1,50","1,50","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","A"]
["0,70","BAC","B","50,00","4 - 8","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["1,30","BAC","C",null,"4 - 8",null,"Rohrbruch / Einsturz Einsturz "]
["1,30","BAP",null,null,"4 - 8",null,"Hohlraum sichtbar  "]
["1,50","BAF","C / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe sichtbar Ursache nicht eindeutig festellbar","B"]
["1,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.5,2,{"$f":"H40*I40","v":{"v":3,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.5,3,{"$f":"H41*I41","v":{"v":4.5,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":7.5,"d":"€8"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":1.425,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":8.925,"d":"€9"}}]

{"sheet":"09342839GA03","index":296,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839GA03","BERLINER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,50","BAF","A / E",null,"4 - 8",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","A"]
["0,90","BAF","E / E",null,"4 - 8","JA","Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["1,10","BAF","A / E",null,"4 - 8",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","B"]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H14*I14","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H15*I15","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":6.545,"d":"€7"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839GA03","BERLINER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,50","BAF","A / E",null,"4 - 8",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","A"]
["0,90","BAF","E / E",null,"4 - 8","JA","Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["1,10","BAF","A / E",null,"4 - 8",null,"Oberflächenschaden erhöhte Rauheit Ursache nicht eindeutig festellbar","B"]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H36*I36","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H37*I37","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":6.545,"d":"€7"}}]

{"sheet":"09342839GA05","index":297,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839GA05","BERLINER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,90","BAC","B","100,00","4 - 8","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["0,90","BAP",null,null,"4 - 8","JA","Hohlraum sichtbar  "]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H13*I13","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H14*I14","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":5.95,"d":"€6"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839GA05","BERLINER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,90","BAC","B","100,00","4 - 8","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["0,90","BAP",null,null,"4 - 8","JA","Hohlraum sichtbar  "]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H34*I34","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H35*I35","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":5.95,"d":"€6"}}]

{"sheet":"09342839GA07","index":298,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839GA07","BERLINER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H11*I11","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H12*I12","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":5.95,"d":"€6"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839GA07","BERLINER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H30*I30","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H31*I31","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":5.95,"d":"€6"}}]

{"sheet":"09342839GA11","index":299,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839GA11","BERLINER STRAßE","2,30","2,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,90","BAN",null,null,"4 - 8","JA","Poröses Rohr  "]
["0,90","BAF","E / E",null,"4 - 8","JA","Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["2,30","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.3,2,{"$f":"H13*I13","v":{"v":4.6,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.3,3,{"$f":"H14*I14","v":{"v":6.8999999999999995,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":11.5,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":2.185,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":13.685,"d":"€14"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839GA11","BERLINER STRAßE","2,30","2,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,90","BAN",null,null,"4 - 8","JA","Poröses Rohr  "]
["0,90","BAF","E / E",null,"4 - 8","JA","Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["2,30","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.3,2,{"$f":"H34*I34","v":{"v":4.6,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.3,3,{"$f":"H35*I35","v":{"v":6.8999999999999995,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":11.5,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":2.185,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":13.685,"d":"€14"}}]

{"sheet":"09342839NN09","index":300,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839NN09","BERLINER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,80","BAC","B","60,00","4 - 8","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["0,90","BAG",null,"70,00","1 - 5",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,90","BCA","C / A","125,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["1,00","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H14*I14","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H15*I15","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":68.5,"d":"€69"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":13.015,"d":"€13"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":81.515,"d":"€82"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839NN09","BERLINER STRAßE","1,00","1,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,80","BAC","B","60,00","4 - 8","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["0,90","BAG",null,"70,00","1 - 5",null,"Einragender Anschluss  "]
["0,90","BCA","C / A","125,00","3",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["1,00","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":490,"d":"€490"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":49,"d":"€49"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":24.5,"d":"€25"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":58.8,"d":"€59"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H36*I36","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H37*I37","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":627.3,"d":"€627"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":119.187,"d":"€119"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":746.487,"d":"€746"}}]

{"sheet":"09342839RS02","index":301,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839RS02","BERLINER STRAßE","4,10","4,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAI","Z","10,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A","Fräsen",{"v":50,"d":"€50"}]
["0,60","BAI","Z","10,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B","Fräsen",{"v":50,"d":"€50"}]
["1,40","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,70","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["2,90","BBC","C","3,00","8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["4,10","BBC","C","3,00","8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["4,10","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":250,"d":"€250"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":25,"d":"€25"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":12.5,"d":"€13"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":30,"d":"€30"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.1,2,{"$f":"H17*I17","v":{"v":8.2,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.1,3,{"$f":"H18*I18","v":{"v":12.299999999999999,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":338,"d":"€338"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":64.22,"d":"€64"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":402.22,"d":"€402"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839RS02","BERLINER STRAßE","4,10","4,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAI","Z","10,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A"]
["0,60","BAI","Z","10,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B"]
["1,40","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,70","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["2,90","BBC","C","3,00","8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["4,10","BBC","C","3,00","8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["4,10","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":150,"d":"€150"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.1,2,{"$f":"H42*I42","v":{"v":8.2,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.1,3,{"$f":"H43*I43","v":{"v":12.299999999999999,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":211,"d":"€211"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":40.09,"d":"€40"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":251.09,"d":"€251"}}]

{"sheet":"09342839RS04","index":302,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839RS04","BERLINER STRAßE","4,00","4,30","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAI","Z","10,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A","Fräsen",{"v":50,"d":"€50"}]
["1,40","BAI","Z","10,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B","Fräsen",{"v":50,"d":"€50"}]
["1,70","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,70","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,70","BCA","C / A","80,00","11",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["4,00","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":150,"d":"€150"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4,2,{"$f":"H16*I16","v":{"v":8,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4,3,{"$f":"H17*I17","v":{"v":12,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":210.5,"d":"€211"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":39.995,"d":"€40"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":250.495,"d":"€250"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839RS04","BERLINER STRAßE","4,00","4,30","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAI","Z","10,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A"]
["1,40","BAI","Z","10,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B"]
["1,70","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,70","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,70","BCA","C / A","80,00","11",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["4,00","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":540,"d":"€540"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":54,"d":"€54"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":27,"d":"€27"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":64.8,"d":"€65"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4,2,{"$f":"H40*I40","v":{"v":8,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4,3,{"$f":"H41*I41","v":{"v":12,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":705.8,"d":"€706"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":134.102,"d":"€134"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":839.9019999999999,"d":"€840"}}]

{"sheet":"09342839RS06","index":303,"n_rows":48,"n_cols":10,"rows_kept":48}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839RS06","BERLINER STRAßE","4,20","4,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["0,80","BBC","C","15,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["1,80","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,90","BBC","C","15,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["3,90","BAB","B / A","1,00","12",null,"Rissbildung Riss in Längsrichtung"]
["4,00","BAG",null,"50,00","9 - 3",null,"Einragender Anschluss  ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,00","BCA","C / A","50,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["4,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J13)","v":{"v":200,"d":"€200"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H15/100)*J14","v":{"v":20,"d":"€20"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H16/100)*J14","v":{"v":10,"d":"€10"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H17/100)*J14","v":{"v":24,"d":"€24"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.2,2,{"$f":"H18*I18","v":{"v":8.4,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.2,3,{"$f":"H19*I19","v":{"v":12.600000000000001,"d":"€13"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J14:J19)","v":{"v":275,"d":"€275"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H21/100)*J20","v":{"v":52.25,"d":"€52"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J20:J21)","v":{"v":327.25,"d":"€327"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839RS06","BERLINER STRAßE","4,20","4,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBC","C","5,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","A","Fräsen",{"v":50,"d":"€50"}]
["0,80","BBC","C","15,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","C","Fräsen",{"v":50,"d":"€50"}]
["1,80","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,90","BBC","C","15,00","4 - 8",null,"Ablagerungen hartes oder verdichtetes Material ","B","Fräsen",{"v":50,"d":"€50"}]
["3,90","BAB","B / A","1,00","12",null,"Rissbildung Riss in Längsrichtung"]
["4,00","BAG",null,"50,00","9 - 3",null,"Einragender Anschluss  "]
["4,00","BCA","C / A","50,00","12",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["4,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J31:J39)","v":{"v":640,"d":"€640"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":64,"d":"€64"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":32,"d":"€32"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":76.8,"d":"€77"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.2,2,{"$f":"H44*I44","v":{"v":8.4,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.2,3,{"$f":"H45*I45","v":{"v":12.600000000000001,"d":"€13"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":833.8,"d":"€834"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":158.422,"d":"€158"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":992.222,"d":"€992"}}]

{"sheet":"09342839RS08","index":304,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839RS08","BERLINER STRAßE","3,90","4,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAI","Z","5,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A","Fräsen",{"v":50,"d":"€50"}]
["1,60","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,70","BAI","Z","5,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B","Fräsen",{"v":50,"d":"€50"}]
["3,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.9,2,{"$f":"H14*I14","v":{"v":7.8,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.9,3,{"$f":"H15*I15","v":{"v":11.7,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":146.5,"d":"€147"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":27.835,"d":"€28"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":174.335,"d":"€174"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839RS08","BERLINER STRAßE","3,90","4,20","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAI","Z","5,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","A"]
["1,60","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,70","BAI","Z","5,00","4 - 8",null,"Einragendes Dichtungsmaterial andere Dichtungsart ","B"]
["3,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.9,2,{"$f":"H36*I36","v":{"v":7.8,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.9,3,{"$f":"H37*I37","v":{"v":11.7,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":19.5,"d":"€20"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":3.705,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":23.205,"d":"€23"}}]

{"sheet":"09342839RS10","index":305,"n_rows":48,"n_cols":10,"rows_kept":48}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839RS10","BERLINER STRAßE","4,70","5,00","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["0,30","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["0,80","BCC","A / B","45,00","8",null,"Krümmung der Leitung nach links nach unten"]
["1,00","BCC","A / A","30,00","10",null,"Krümmung der Leitung nach links nach oben"]
["1,20","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["2,10","BAI","Z","5,00","3 - 7","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,40","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["4,70","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J13)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H15/100)*J14","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H16/100)*J14","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H17/100)*J14","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.7,2,{"$f":"H18*I18","v":{"v":9.4,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.7,3,{"$f":"H19*I19","v":{"v":14.100000000000001,"d":"€14"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J14:J19)","v":{"v":87,"d":"€87"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H21/100)*J20","v":{"v":16.53,"d":"€17"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J20:J21)","v":{"v":103.53,"d":"€104"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342839RS10","BERLINER STRAßE","4,70","5,00","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["0,30","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["0,80","BCC","A / B","45,00","8",null,"Krümmung der Leitung nach links nach unten"]
["1,00","BCC","A / A","30,00","10",null,"Krümmung der Leitung nach links nach oben"]
["1,20","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["2,10","BAI","Z","5,00","3 - 7","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["2,40","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["4,70","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J31:J39)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.7,2,{"$f":"H44*I44","v":{"v":9.4,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.7,3,{"$f":"H45*I45","v":{"v":14.100000000000001,"d":"€14"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":23.5,"d":"€24"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":4.465,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":27.965,"d":"€28"}}]

{"sheet":"09342840GA03","index":306,"n_rows":50,"n_cols":10,"rows_kept":50}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342840GA03","BERLINER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCB","Z",null,"12 - 12",null,"Punktuelle Reparatur anderes grabenloses Reparaturverfahren ","A"]
["0,30","BCC","B / Y","15,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,40","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,70","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["0,70","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen"]
["0,80","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["0,80","BCB","Z",null,"12 - 12",null,"Punktuelle Reparatur anderes grabenloses Reparaturverfahren ","B"]
["1,00","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J14)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H16/100)*J15","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H17/100)*J15","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H18/100)*J15","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H19*I19","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H20*I20","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J15:J20)","v":{"v":5.5,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H22/100)*J21","v":{"v":1.045,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J21:J22)","v":{"v":6.545,"d":"€7"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342840GA03","BERLINER STRAßE","1,10","1,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCB","Z",null,"12 - 12",null,"Punktuelle Reparatur anderes grabenloses Reparaturverfahren ","A"]
["0,30","BCC","B / Y","15,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,40","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,70","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["0,70","BCA","A / A","150,00","12",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["0,80","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["0,80","BCB","Z",null,"12 - 12",null,"Punktuelle Reparatur anderes grabenloses Reparaturverfahren ","B"]
["1,00","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J32:J41)","v":{"v":490,"d":"€490"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H43/100)*J42","v":{"v":49,"d":"€49"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H44/100)*J42","v":{"v":24.5,"d":"€25"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H45/100)*J42","v":{"v":58.8,"d":"€59"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.1,2,{"$f":"H46*I46","v":{"v":2.2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.1,3,{"$f":"H47*I47","v":{"v":3.3000000000000003,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J42:J47)","v":{"v":627.8,"d":"€628"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H49/100)*J48","v":{"v":119.282,"d":"€119"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J48:J49)","v":{"v":747.082,"d":"€747"}}]

{"sheet":"09342840GA04","index":307,"n_rows":48,"n_cols":10,"rows_kept":48}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342840GA04","BERLINER STRAßE","2,10","2,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,40","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,50","BAJ","B","30,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,90","BCA","A / A","100,00","3",null,"Anschluss Abzweig offen"]
["1,10","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,10","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["1,10","BAJ","B","20,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,90","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["2,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J13)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H15/100)*J14","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H16/100)*J14","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H17/100)*J14","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.1,2,{"$f":"H18*I18","v":{"v":4.2,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.1,3,{"$f":"H19*I19","v":{"v":6.300000000000001,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J14:J19)","v":{"v":137.5,"d":"€138"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H21/100)*J20","v":{"v":26.125,"d":"€26"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J20:J21)","v":{"v":163.625,"d":"€164"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342840GA04","BERLINER STRAßE","2,10","2,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,40","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,50","BAJ","B","30,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,90","BCA","A / A","100,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["1,10","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,10","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["1,10","BAJ","B","20,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,90","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["2,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J31:J39)","v":{"v":590,"d":"€590"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":59,"d":"€59"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":29.5,"d":"€30"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":70.8,"d":"€71"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.1,2,{"$f":"H44*I44","v":{"v":4.2,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.1,3,{"$f":"H45*I45","v":{"v":6.300000000000001,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":759.8,"d":"€760"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":144.362,"d":"€144"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":904.1619999999999,"d":"€904"}}]

{"sheet":"09342840NN05","index":308,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342840NN05","BERLINER STRAßE","0,70","0,70","Not Implemented yet",{"$nulls":3},"100","PVC"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BAA","A","50,00","1 - 11",null,"Verformung vertikal "]
["0,70","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.7,2,{"$f":"H12*I12","v":{"v":1.4,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.7,3,{"$f":"H13*I13","v":{"v":2.0999999999999996,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":3.4999999999999996,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.6649999999999999,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":4.164999999999999,"d":"€4"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342840NN05","BERLINER STRAßE","0,70","0,70","Not Implemented yet",{"$nulls":3},"100","PVC"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BAA","A","50,00","1 - 11",null,"Verformung vertikal "]
["0,70","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.7,2,{"$f":"H32*I32","v":{"v":1.4,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.7,3,{"$f":"H33*I33","v":{"v":2.0999999999999996,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":3.4999999999999996,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.6649999999999999,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":4.164999999999999,"d":"€4"}}]

{"sheet":"09342840RS01","index":309,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342840RS01","BERLINER STRAßE","0,90","1,30","Not Implemented yet",{"$nulls":3},"150","PVC"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H11*I11","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H12*I12","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":5.355,"d":"€5"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342840RS01","BERLINER STRAßE","0,90","1,30","Not Implemented yet",{"$nulls":3},"150","PVC"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H30*I30","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H31*I31","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":5.355,"d":"€5"}}]

{"sheet":"09342840RV02","index":310,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342840RV02","BERLINER STRAßE","0,50","0,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["0,30","BCA","A / A","100,00","6",null,"Anschluss Abzweig offen"]
["0,50","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.5,2,{"$f":"H13*I13","v":{"v":1,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.5,3,{"$f":"H14*I14","v":{"v":1.5,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":2.5,"d":"€3"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":0.475,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":2.975,"d":"€3"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342840RV02","BERLINER STRAßE","0,50","0,50","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["0,30","BCA","A / A","100,00","6",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["0,50","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":490,"d":"€490"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":49,"d":"€49"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":24.5,"d":"€25"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":58.8,"d":"€59"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.5,2,{"$f":"H34*I34","v":{"v":1,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.5,3,{"$f":"H35*I35","v":{"v":1.5,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":624.8,"d":"€625"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":118.71199999999999,"d":"€119"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":743.512,"d":"€744"}}]

{"sheet":"09342841","index":311,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342841","BERLINER STRAßE","26,80","26,80","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["13,40","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen"]
["17,20","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen"]
["21,90","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen"]
["26,80","BDC","Y / Z",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar andere"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",26.8,2,{"$f":"H14*I14","v":{"v":53.6,"d":"€54"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",26.8,3,{"$f":"H15*I15","v":{"v":80.4,"d":"€80"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":134,"d":"€134"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":25.46,"d":"€25"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":159.46,"d":"€159"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09342841","BERLINER STRAßE","26,80","26,80","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["13,40","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["17,20","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["21,90","BCA","A / A","150,00","3",null,"Anschluss Abzweig offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["26,80","BDC","Y / Z",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar andere"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":1470,"d":"€1,470"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":147,"d":"€147"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":73.5,"d":"€74"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":176.4,"d":"€176"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",26.8,2,{"$f":"H36*I36","v":{"v":53.6,"d":"€54"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",26.8,3,{"$f":"H37*I37","v":{"v":80.4,"d":"€80"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":2000.9,"d":"€2,001"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":380.17100000000005,"d":"€380"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":2381.071,"d":"€2,381"}}]

{"sheet":"09343174","index":312,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09343174","BERLINER STRAßE","22,40","58,41","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["8,30","BAJ","B","10,00","11","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["9,70","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["17,90","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["20,80","BDD","C","20,00",null,null,"Wasserspiegel trüb ","A"]
["22,40","BDD","C","20,00",null,null,"Wasserspiegel trüb ","B"]
["22,40","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",22.4,2,{"$f":"H16*I16","v":{"v":44.8,"d":"€45"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",22.4,3,{"$f":"H17*I17","v":{"v":67.19999999999999,"d":"€67"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":175.5,"d":"€176"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":33.345,"d":"€33"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":208.845,"d":"€209"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09343174","BERLINER STRAßE","22,40","58,41","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["8,30","BAJ","B","10,00","11","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["9,70","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["17,90","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["20,80","BDD","C","20,00",null,null,"Wasserspiegel trüb ","A"]
["22,40","BDD","C","20,00",null,null,"Wasserspiegel trüb ","B"]
["22,40","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":1030,"d":"€1,030"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":103,"d":"€103"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":51.5,"d":"€52"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":123.6,"d":"€124"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",22.4,2,{"$f":"H40*I40","v":{"v":44.8,"d":"€45"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",22.4,3,{"$f":"H41*I41","v":{"v":67.19999999999999,"d":"€67"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":1420.1,"d":"€1,420"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":269.81899999999996,"d":"€270"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":1689.9189999999999,"d":"€1,690"}}]

{"sheet":"09343175GA01","index":313,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09343175GA01","BERLINER STRAßE","3,40","3,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / A","15,00","2",null,"Krümmung der Leitung nach rechts nach oben"]
["1,90","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,90","BAJ","C","10,00","12","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,40","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["3,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.4,2,{"$f":"H15*I15","v":{"v":6.8,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.4,3,{"$f":"H16*I16","v":{"v":10.2,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":144,"d":"€144"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":27.36,"d":"€27"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":171.36,"d":"€171"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09343175GA01","BERLINER STRAßE","3,40","3,40","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / A","15,00","2",null,"Krümmung der Leitung nach rechts nach oben"]
["1,90","BAJ","B","15,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,90","BAJ","C","10,00","12","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,40","AED","GGG",{"$nulls":3},"Grundlagen änderung  "]
["3,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.4,2,{"$f":"H38*I38","v":{"v":6.8,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.4,3,{"$f":"H39*I39","v":{"v":10.2,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":144,"d":"€144"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":27.36,"d":"€27"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":171.36,"d":"€171"}}]

{"sheet":"09343175GA03","index":314,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09343175GA03","BERLINER STRAßE","3,50","3,50","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / Y","30,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,30","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["1,10","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H14*I14","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H15*I15","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":81,"d":"€81"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":15.39,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":96.39,"d":"€96"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09343175GA03","BERLINER STRAßE","3,50","3,50","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","B / Y","30,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,30","AED","STZ",{"$nulls":3},"Grundlagen änderung  "]
["1,10","BAJ","B","10,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H36*I36","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H37*I37","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":81,"d":"€81"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":15.39,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":96.39,"d":"€96"}}]

{"sheet":"09343175RR02","index":315,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09343175RR02","BERLINER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,70","BAJ","B","15,00","3","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,50","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,50","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,50","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,70","BCC","A / A","90,00","10",null,"Krümmung der Leitung nach links nach oben"]
["2,80","BCC","B / A","45,00","1",null,"Krümmung der Leitung nach rechts nach oben"]
["2,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H17*I17","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H18*I18","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":78,"d":"€78"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":14.82,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":92.82,"d":"€93"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09343175RR02","BERLINER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,70","BAJ","B","15,00","3","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,50","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,50","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,50","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,70","BCC","A / A","90,00","10",null,"Krümmung der Leitung nach links nach oben"]
["2,80","BCC","B / A","45,00","1",null,"Krümmung der Leitung nach rechts nach oben"]
["2,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H42*I42","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H43*I43","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":78,"d":"€78"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":14.82,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":92.82,"d":"€93"}}]

{"sheet":"09345300GA02","index":316,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345300GA02","BERLINER STRAßE","2,10","2,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,90","BAI","Z","15,00","4 - 8","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,90","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.1,2,{"$f":"H13*I13","v":{"v":4.2,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.1,3,{"$f":"H14*I14","v":{"v":6.300000000000001,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":137.5,"d":"€138"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":26.125,"d":"€26"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":163.625,"d":"€164"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345300GA02","BERLINER STRAßE","2,10","2,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,90","BAI","Z","15,00","4 - 8","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["1,90","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.1,2,{"$f":"H34*I34","v":{"v":4.2,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.1,3,{"$f":"H35*I35","v":{"v":6.300000000000001,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":74,"d":"€74"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":14.06,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":88.06,"d":"€88"}}]

{"sheet":"09345300GA03","index":317,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345300GA03","BERLINER STRAßE","2,10","2,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,80","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,00","BAC","A","500,00","12 - 12","JA","Rohrbruch / Einsturz Bruch ","A"]
["1,20","BAC","A","500,00","12 - 12","JA","Rohrbruch / Einsturz Bruch ","B"]
["2,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.1,2,{"$f":"H14*I14","v":{"v":4.2,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.1,3,{"$f":"H15*I15","v":{"v":6.300000000000001,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":74,"d":"€74"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":14.06,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":88.06,"d":"€88"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345300GA03","BERLINER STRAßE","2,10","2,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,80","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,00","BAC","A","500,00","12 - 12","JA","Rohrbruch / Einsturz Bruch ","A"]
["1,20","BAC","A","500,00","12 - 12","JA","Rohrbruch / Einsturz Bruch ","B"]
["2,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.1,2,{"$f":"H36*I36","v":{"v":4.2,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.1,3,{"$f":"H37*I37","v":{"v":6.300000000000001,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":74,"d":"€74"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":14.06,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":88.06,"d":"€88"}}]

{"sheet":"09345300GA04","index":318,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345300GA04","BERLINER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,90","BAI","Z","10,00","4 - 8","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H12*I12","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H13*I13","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":79,"d":"€79"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":15.01,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":94.01,"d":"€94"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345300GA04","BERLINER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,90","BAI","Z","10,00","4 - 8","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["3,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H32*I32","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H33*I33","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":18.445,"d":"€18"}}]

{"sheet":"09345300NN01","index":319,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345300NN01","BERLINER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,60","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,60","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["2,60","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["3,00","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H16*I16","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H17*I17","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":16,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":3.04,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":19.04,"d":"€19"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345300NN01","BERLINER STRAßE","3,20","3,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,60","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,60","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["2,60","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["3,00","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H40*I40","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H41*I41","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":16,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":3.04,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":19.04,"d":"€19"}}]

{"sheet":"09345300RR05","index":320,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345300RR05","BERLINER STRAßE","7,50","7,50","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,00","BBE","B","20,00","4 - 8",null,"Andere Hindernisse Bruchstücke einer Abwasserleitung oder eines Abwasserkanals liegen in der \r\nRohrsohle "]
["6,30","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["6,30","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["6,30","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["7,50","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["7,50","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",7.5,2,{"$f":"H16*I16","v":{"v":15,"d":"€15"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",7.5,3,{"$f":"H17*I17","v":{"v":22.5,"d":"€23"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":37.5,"d":"€38"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":7.125,"d":"€7"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":44.625,"d":"€45"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345300RR05","BERLINER STRAßE","7,50","7,50","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,00","BBE","B","20,00","4 - 8",null,"Andere Hindernisse Bruchstücke einer Abwasserleitung oder eines Abwasserkanals liegen in der \r\nRohrsohle "]
["6,30","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["6,30","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["6,30","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["7,50","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["7,50","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",7.5,2,{"$f":"H40*I40","v":{"v":15,"d":"€15"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",7.5,3,{"$f":"H41*I41","v":{"v":22.5,"d":"€23"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":37.5,"d":"€38"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":7.125,"d":"€7"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":44.625,"d":"€45"}}]

{"sheet":"09345333GA04","index":321,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333GA04","BERLINER STRAßE","6,00","6,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["4,60","BBE","C",null,"3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["4,70","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6,2,{"$f":"H14*I14","v":{"v":12,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6,3,{"$f":"H15*I15","v":{"v":18,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":93.5,"d":"€94"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":17.765,"d":"€18"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":111.265,"d":"€111"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333GA04","BERLINER STRAßE","6,00","6,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["4,60","BBE","C",null,"3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["4,70","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,00","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6,2,{"$f":"H36*I36","v":{"v":12,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6,3,{"$f":"H37*I37","v":{"v":18,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":93.5,"d":"€94"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":17.765,"d":"€18"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":111.265,"d":"€111"}}]

{"sheet":"09345333NN01","index":322,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333NN01","BERLINER STRAßE","4,50","4,50","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,50","BBE","C","70,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["4,50","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.5,2,{"$f":"H12*I12","v":{"v":9,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.5,3,{"$f":"H13*I13","v":{"v":13.5,"d":"€14"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":22.5,"d":"€23"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":4.275,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":26.775,"d":"€27"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333NN01","BERLINER STRAßE","4,50","4,50","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,50","BBE","C","70,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["4,50","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.5,2,{"$f":"H32*I32","v":{"v":9,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.5,3,{"$f":"H33*I33","v":{"v":13.5,"d":"€14"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":22.5,"d":"€23"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":4.275,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":26.775,"d":"€27"}}]

{"sheet":"09345333NN02","index":323,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333NN02","BERLINER STRAßE","1,30","1,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBE","C","40,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["1,30","BBE","C","70,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["1,30","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.3,2,{"$f":"H13*I13","v":{"v":2.6,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.3,3,{"$f":"H14*I14","v":{"v":3.9000000000000004,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":6.5,"d":"€7"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":1.235,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":7.735,"d":"€8"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333NN02","BERLINER STRAßE","1,30","1,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBE","C","40,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["1,30","BBE","C","70,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["1,30","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.3,2,{"$f":"H34*I34","v":{"v":2.6,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.3,3,{"$f":"H35*I35","v":{"v":3.9000000000000004,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":6.5,"d":"€7"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":1.235,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":7.735,"d":"€8"}}]

{"sheet":"09345333NN05","index":324,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333NN05","BERLINER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,60","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["0,90","BAJ","B","30,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,50","BBE","C","60,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["2,50","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H14*I14","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H15*I15","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":76,"d":"€76"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":14.44,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":90.44,"d":"€90"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333NN05","BERLINER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,60","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["0,90","BAJ","B","30,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,50","BBE","C","60,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["2,50","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H36*I36","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H37*I37","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":76,"d":"€76"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":14.44,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":90.44,"d":"€90"}}]

{"sheet":"09345333SE03","index":325,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333SE03","BERLINER STRAßE","1,00","1,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H11*I11","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H12*I12","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":5.95,"d":"€6"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333SE03","BERLINER STRAßE","1,00","1,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1,2,{"$f":"H30*I30","v":{"v":2,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1,3,{"$f":"H31*I31","v":{"v":3,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.95,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":5.95,"d":"€6"}}]

{"sheet":"09345333_1GA02","index":326,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333_1GA02","BERLINER STRAßE","2,40","2,40","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,40","BAB","B / B","8,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["1,50","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,50","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["1,50","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,10","BCC","B / A","45,00","2",null,"Krümmung der Leitung nach rechts nach oben"]
["2,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.4,2,{"$f":"H16*I16","v":{"v":4.8,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.4,3,{"$f":"H17*I17","v":{"v":7.199999999999999,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":12,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":2.2800000000000002,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":14.280000000000001,"d":"€14"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333_1GA02","BERLINER STRAßE","2,40","2,40","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,40","BAB","B / B","8,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["1,50","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,50","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["1,50","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,10","BCC","B / A","45,00","2",null,"Krümmung der Leitung nach rechts nach oben"]
["2,40","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.4,2,{"$f":"H40*I40","v":{"v":4.8,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.4,3,{"$f":"H41*I41","v":{"v":7.199999999999999,"d":"€7"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":12,"d":"€12"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":2.2800000000000002,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":14.280000000000001,"d":"€14"}}]

{"sheet":"09345333_1GA03","index":327,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333_1GA03","BERLINER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,70","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,20","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,20","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H15*I15","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H16*I16","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":76,"d":"€76"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":14.44,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":90.44,"d":"€90"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333_1GA03","BERLINER STRAßE","2,50","2,50","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,70","BAJ","B","15,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,20","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["1,20","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,50","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H38*I38","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H39*I39","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":76,"d":"€76"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":14.44,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":90.44,"d":"€90"}}]

{"sheet":"09345333_1GA05","index":328,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333_1GA05","BERLINER STRAßE","3,30","3,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,80","BBE","C","5,00","6 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["3,30","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.3,2,{"$f":"H12*I12","v":{"v":6.6,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.3,3,{"$f":"H13*I13","v":{"v":9.899999999999999,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":16.5,"d":"€17"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":3.1350000000000002,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":19.635,"d":"€20"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333_1GA05","BERLINER STRAßE","3,30","3,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,80","BBE","C","5,00","6 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["3,30","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.3,2,{"$f":"H32*I32","v":{"v":6.6,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.3,3,{"$f":"H33*I33","v":{"v":9.899999999999999,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":16.5,"d":"€17"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":3.1350000000000002,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":19.635,"d":"€20"}}]

{"sheet":"09345333_1GA06","index":329,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333_1GA06","BERLINER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["0,20","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["0,20","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["0,90","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["0,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H15*I15","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H16*I16","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":5.355,"d":"€5"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333_1GA06","BERLINER STRAßE","0,90","0,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["0,20","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["0,20","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["0,90","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["0,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.9,2,{"$f":"H38*I38","v":{"v":1.8,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.9,3,{"$f":"H39*I39","v":{"v":2.7,"d":"€3"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":4.5,"d":"€5"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":0.855,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":5.355,"d":"€5"}}]

{"sheet":"09345333_1NN04","index":330,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333_1NN04","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"125","PVC"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333_1NN04","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"125","PVC"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09345333_1RR01","index":331,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333_1RR01","BERLINER STRAßE","3,30","3,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,40","BAB","B / B","8,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["2,80","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["2,80","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["3,30","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.3,2,{"$f":"H16*I16","v":{"v":6.6,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.3,3,{"$f":"H17*I17","v":{"v":9.899999999999999,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":16.5,"d":"€17"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":3.1350000000000002,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":19.635,"d":"€20"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345333_1RR01","BERLINER STRAßE","3,30","3,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,40","BAB","B / B","8,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["2,80","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["2,80","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["3,30","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.3,2,{"$f":"H40*I40","v":{"v":6.6,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.3,3,{"$f":"H41*I41","v":{"v":9.899999999999999,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":16.5,"d":"€17"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":3.1350000000000002,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":19.635,"d":"€20"}}]

{"sheet":"09345334GA02","index":332,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345334GA02","LEIPZIGER STRAßE","6,10","6,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["4,80","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["4,80","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["6,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.1,2,{"$f":"H14*I14","v":{"v":12.2,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.1,3,{"$f":"H15*I15","v":{"v":18.299999999999997,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":30.499999999999996,"d":"€31"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":5.794999999999999,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":36.294999999999995,"d":"€36"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345334GA02","LEIPZIGER STRAßE","6,10","6,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["4,80","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["4,80","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["4,80","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["6,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.1,2,{"$f":"H36*I36","v":{"v":12.2,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.1,3,{"$f":"H37*I37","v":{"v":18.299999999999997,"d":"€18"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":30.499999999999996,"d":"€31"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":5.794999999999999,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":36.294999999999995,"d":"€36"}}]

{"sheet":"09345334GA04","index":333,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345334GA04","LEIPZIGER STRAßE","4,30","4,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["4,30","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.3,2,{"$f":"H12*I12","v":{"v":8.6,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.3,3,{"$f":"H13*I13","v":{"v":12.899999999999999,"d":"€13"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":21.5,"d":"€22"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":4.085,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":25.585,"d":"€26"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345334GA04","LEIPZIGER STRAßE","4,30","4,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["4,30","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.3,2,{"$f":"H32*I32","v":{"v":8.6,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.3,3,{"$f":"H33*I33","v":{"v":12.899999999999999,"d":"€13"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":21.5,"d":"€22"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":4.085,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":25.585,"d":"€26"}}]

{"sheet":"09345334NN03","index":334,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345334NN03","LEIPZIGER STRAßE","4,10","4,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BBE","C","60,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["2,00","BBE","C",null,"2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["4,10","BBE","C","99,00","12 - 12",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["4,10","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.1,2,{"$f":"H14*I14","v":{"v":8.2,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.1,3,{"$f":"H15*I15","v":{"v":12.299999999999999,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":20.5,"d":"€21"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":3.895,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":24.395,"d":"€24"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345334NN03","LEIPZIGER STRAßE","4,10","4,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BBE","C","60,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["2,00","BBE","C",null,"2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["4,10","BBE","C","99,00","12 - 12",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["4,10","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.1,2,{"$f":"H36*I36","v":{"v":8.2,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.1,3,{"$f":"H37*I37","v":{"v":12.299999999999999,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":20.5,"d":"€21"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":3.895,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":24.395,"d":"€24"}}]

{"sheet":"09345334NN06","index":335,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345334NN06","LEIPZIGER STRAßE","8,40","8,40","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["7,90","BBE","C","40,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["8,40","BBE","C","40,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["8,40","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",8.4,2,{"$f":"H13*I13","v":{"v":16.8,"d":"€17"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",8.4,3,{"$f":"H14*I14","v":{"v":25.200000000000003,"d":"€25"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":42,"d":"€42"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":7.98,"d":"€8"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":49.980000000000004,"d":"€50"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345334NN06","LEIPZIGER STRAßE","8,40","8,40","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["7,90","BBE","C","40,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["8,40","BBE","C","40,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["8,40","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",8.4,2,{"$f":"H34*I34","v":{"v":16.8,"d":"€17"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",8.4,3,{"$f":"H35*I35","v":{"v":25.200000000000003,"d":"€25"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":42,"d":"€42"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":7.98,"d":"€8"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":49.980000000000004,"d":"€50"}}]

{"sheet":"09345334RV01","index":336,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345334RV01","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBE","C","15,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["1,90","BBE","C",null,"4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["2,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H13*I13","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H14*I14","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":17.255,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345334RV01","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBE","C","15,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["1,90","BBE","C",null,"4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["2,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H34*I34","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H35*I35","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":17.255,"d":"€17"}}]

{"sheet":"09345334RV05","index":337,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345334RV05","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,50","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["2,90","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,90","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["2,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H14*I14","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H15*I15","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":17.255,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345334RV05","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,50","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["2,90","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["2,90","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["2,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H36*I36","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H37*I37","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":17.255,"d":"€17"}}]

{"sheet":"09345335NN01","index":338,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345335NN01","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H12*I12","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H13*I13","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345335NN01","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H32*I32","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H33*I33","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09345335NN02","index":339,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345335NN02","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345335NN02","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09345335NN03","index":340,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345335NN03","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBE","C","35,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H12*I12","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H13*I13","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345335NN03","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBE","C","35,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H32*I32","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H33*I33","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09345335NN04","index":341,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345335NN04","LEIPZIGER STRAßE","0,60","0,60","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBE","C","35,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["0,60","BBE","C","35,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["0,60","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.6,2,{"$f":"H13*I13","v":{"v":1.2,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.6,3,{"$f":"H14*I14","v":{"v":1.7999999999999998,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":3,"d":"€3"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":0.5700000000000001,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":3.5700000000000003,"d":"€4"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345335NN04","LEIPZIGER STRAßE","0,60","0,60","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBE","C","35,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["0,60","BBE","C","35,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["0,60","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.6,2,{"$f":"H34*I34","v":{"v":1.2,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.6,3,{"$f":"H35*I35","v":{"v":1.7999999999999998,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":3,"d":"€3"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":0.5700000000000001,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":3.5700000000000003,"d":"€4"}}]

{"sheet":"09345335NN05","index":342,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345335NN05","LEIPZIGER STRAßE","7,30","7,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBE","C","15,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["1,60","BBE","C","15,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["4,70","BAI","Z","15,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,00","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["7,20","BAP",null,null,"3 - 9",null,"Hohlraum sichtbar  "]
["7,20","BAC","C",null,"12 - 12",null,"Rohrbruch / Einsturz Einsturz "]
["7,30","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",7.3,2,{"$f":"H17*I17","v":{"v":14.6,"d":"€15"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",7.3,3,{"$f":"H18*I18","v":{"v":21.9,"d":"€22"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":100,"d":"€100"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":19,"d":"€19"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":119,"d":"€119"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345335NN05","LEIPZIGER STRAßE","7,30","7,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBE","C","15,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["1,60","BBE","C","15,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["4,70","BAI","Z","15,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["5,00","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["7,20","BAP",null,null,"3 - 9",null,"Hohlraum sichtbar  "]
["7,20","BAC","C",null,"12 - 12",null,"Rohrbruch / Einsturz Einsturz "]
["7,30","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",7.3,2,{"$f":"H42*I42","v":{"v":14.6,"d":"€15"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",7.3,3,{"$f":"H43*I43","v":{"v":21.9,"d":"€22"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":36.5,"d":"€37"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":6.9350000000000005,"d":"€7"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":43.435,"d":"€43"}}]

{"sheet":"09345335NN06","index":343,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345335NN06","LEIPZIGER STRAßE","5,00","5,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["0,90","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,40","BBE","C",null,"4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["5,00","BCC","B / A","45,00","2",null,"Krümmung der Leitung nach rechts nach oben"]
["5,00","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["5,00","BAO",null,null,"4 - 8",null,"Boden sichtbar  "]
["5,00","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5,2,{"$f":"H17*I17","v":{"v":10,"d":"€10"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5,3,{"$f":"H18*I18","v":{"v":15,"d":"€15"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":88.5,"d":"€89"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":16.815,"d":"€17"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":105.315,"d":"€105"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345335NN06","LEIPZIGER STRAßE","5,00","5,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["0,90","BAJ","B","20,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,40","BBE","C",null,"4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["5,00","BCC","B / A","45,00","2",null,"Krümmung der Leitung nach rechts nach oben"]
["5,00","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["5,00","BAO",null,null,"4 - 8",null,"Boden sichtbar  "]
["5,00","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5,2,{"$f":"H42*I42","v":{"v":10,"d":"€10"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5,3,{"$f":"H43*I43","v":{"v":15,"d":"€15"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":88.5,"d":"€89"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":16.815,"d":"€17"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":105.315,"d":"€105"}}]

{"sheet":"09345335RV07","index":344,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345335RV07","LEIPZIGER STRAßE","6,80","6,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBE","C","25,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["3,60","BBE","C","3,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","C"]
["5,90","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["6,80","BBE","C","3,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["6,80","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.8,2,{"$f":"H15*I15","v":{"v":13.6,"d":"€14"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.8,3,{"$f":"H16*I16","v":{"v":20.4,"d":"€20"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":34,"d":"€34"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":6.46,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":40.46,"d":"€40"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345335RV07","LEIPZIGER STRAßE","6,80","6,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBE","C","25,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["3,60","BBE","C","3,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","C"]
["5,90","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["6,80","BBE","C","3,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["6,80","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.8,2,{"$f":"H38*I38","v":{"v":13.6,"d":"€14"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.8,3,{"$f":"H39*I39","v":{"v":20.4,"d":"€20"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":34,"d":"€34"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":6.46,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":40.46,"d":"€40"}}]

{"sheet":"09345336GA01","index":345,"n_rows":42,"n_cols":10,"rows_kept":42}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345336GA01","LEIPZIGER STRAßE","9,90","9,90","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["2,50","BBE","C",null,"4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["8,70","BBE","C","15,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["9,90","BBE","C","15,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["9,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J10)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H12/100)*J11","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H13/100)*J11","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H14/100)*J11","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.9,2,{"$f":"H15*I15","v":{"v":19.8,"d":"€20"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.9,3,{"$f":"H16*I16","v":{"v":29.700000000000003,"d":"€30"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J11:J16)","v":{"v":49.5,"d":"€50"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H18/100)*J17","v":{"v":9.405,"d":"€9"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J17:J18)","v":{"v":58.905,"d":"€59"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345336GA01","LEIPZIGER STRAßE","9,90","9,90","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["2,50","BBE","C",null,"4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["8,70","BBE","C","15,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["9,90","BBE","C","15,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["9,90","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J28:J33)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H35/100)*J34","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H36/100)*J34","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H37/100)*J34","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.9,2,{"$f":"H38*I38","v":{"v":19.8,"d":"€20"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.9,3,{"$f":"H39*I39","v":{"v":29.700000000000003,"d":"€30"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J34:J39)","v":{"v":49.5,"d":"€50"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H41/100)*J40","v":{"v":9.405,"d":"€9"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J40:J41)","v":{"v":58.905,"d":"€59"}}]

{"sheet":"09345336GA06","index":346,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345336GA06","LEIPZIGER STRAßE","6,70","6,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["6,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.7,2,{"$f":"H11*I11","v":{"v":13.4,"d":"€13"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.7,3,{"$f":"H12*I12","v":{"v":20.1,"d":"€20"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":33.5,"d":"€34"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":6.365,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":39.865,"d":"€40"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345336GA06","LEIPZIGER STRAßE","6,70","6,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["6,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",6.7,2,{"$f":"H30*I30","v":{"v":13.4,"d":"€13"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",6.7,3,{"$f":"H31*I31","v":{"v":20.1,"d":"€20"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":33.5,"d":"€34"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":6.365,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":39.865,"d":"€40"}}]

{"sheet":"09345336NN04","index":347,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345336NN04","LEIPZIGER STRAßE","2,00","2,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BAJ","B","30,00","2","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,50","BAC","B","100,00","4 - 10","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["0,50","BAP",null,null,"4 - 10",null,"Hohlraum sichtbar  "]
["0,60","BCC","B / B","45,00","4",null,"Krümmung der Leitung nach rechts nach unten"]
["0,70","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["2,00","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2,2,{"$f":"H16*I16","v":{"v":4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2,3,{"$f":"H17*I17","v":{"v":6,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":73.5,"d":"€74"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":13.965,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":87.465,"d":"€87"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345336NN04","LEIPZIGER STRAßE","2,00","2,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BAJ","B","30,00","2","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,50","BAC","B","100,00","4 - 10","JA","Rohrbruch / Einsturz Fehlen von Teilen "]
["0,50","BAP",null,null,"4 - 10",null,"Hohlraum sichtbar  "]
["0,60","BCC","B / B","45,00","4",null,"Krümmung der Leitung nach rechts nach unten"]
["0,70","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["2,00","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2,2,{"$f":"H40*I40","v":{"v":4,"d":"€4"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2,3,{"$f":"H41*I41","v":{"v":6,"d":"€6"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":73.5,"d":"€74"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":13.965,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":87.465,"d":"€87"}}]

{"sheet":"09345336NN05","index":348,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345336NN05","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBE","C","70,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H12*I12","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H13*I13","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345336NN05","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBE","C","70,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H32*I32","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H33*I33","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09345336RS02","index":349,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345336RS02","LEIPZIGER STRAßE","4,70","5,20","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,50","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["4,70","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.7,2,{"$f":"H13*I13","v":{"v":9.4,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.7,3,{"$f":"H14*I14","v":{"v":14.100000000000001,"d":"€14"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":23.5,"d":"€24"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":4.465,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":27.965,"d":"€28"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345336RS02","LEIPZIGER STRAßE","4,70","5,20","Not Implemented yet",{"$nulls":3},"200","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BCC","B / Y","90,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["0,50","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["4,70","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":780,"d":"€780"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":780,"d":"€780"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":78,"d":"€78"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":39,"d":"€39"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":93.6,"d":"€94"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.7,2,{"$f":"H34*I34","v":{"v":9.4,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.7,3,{"$f":"H35*I35","v":{"v":14.100000000000001,"d":"€14"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":1014.1,"d":"€1,014"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":192.679,"d":"€193"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":1206.779,"d":"€1,207"}}]

{"sheet":"09345336RV03","index":350,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345336RV03","LEIPZIGER STRAßE","5,80","5,80","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["5,80","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.8,2,{"$f":"H11*I11","v":{"v":11.6,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.8,3,{"$f":"H12*I12","v":{"v":17.4,"d":"€17"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":29,"d":"€29"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":5.51,"d":"€6"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":34.51,"d":"€35"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345336RV03","LEIPZIGER STRAßE","5,80","5,80","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["5,80","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":870,"d":"€870"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":870,"d":"€870"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":87,"d":"€87"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":43.5,"d":"€44"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":104.39999999999999,"d":"€104"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.8,2,{"$f":"H30*I30","v":{"v":11.6,"d":"€12"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.8,3,{"$f":"H31*I31","v":{"v":17.4,"d":"€17"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1133.9,"d":"€1,134"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":215.44100000000003,"d":"€215"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1349.3410000000001,"d":"€1,349"}}]

{"sheet":"09345338GA01","index":351,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345338GA01","LEIPZIGER STRAßE","8,60","8,60","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["8,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",8.6,2,{"$f":"H11*I11","v":{"v":17.2,"d":"€17"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",8.6,3,{"$f":"H12*I12","v":{"v":25.799999999999997,"d":"€26"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":43,"d":"€43"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":8.17,"d":"€8"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":51.17,"d":"€51"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345338GA01","LEIPZIGER STRAßE","8,60","8,60","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["8,60","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",8.6,2,{"$f":"H30*I30","v":{"v":17.2,"d":"€17"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",8.6,3,{"$f":"H31*I31","v":{"v":25.799999999999997,"d":"€26"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":43,"d":"€43"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":8.17,"d":"€8"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":51.17,"d":"€51"}}]

{"sheet":"09345338RS02","index":352,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345338RS02","LEIPZIGER STRAßE","4,30","4,70","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,70","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["4,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.3,2,{"$f":"H12*I12","v":{"v":8.6,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.3,3,{"$f":"H13*I13","v":{"v":12.899999999999999,"d":"€13"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":21.5,"d":"€22"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":4.085,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":25.585,"d":"€26"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345338RS02","LEIPZIGER STRAßE","4,30","4,70","Not Implemented yet",{"$nulls":3},"150","PP"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,70","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["4,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.3,2,{"$f":"H32*I32","v":{"v":8.6,"d":"€9"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.3,3,{"$f":"H33*I33","v":{"v":12.899999999999999,"d":"€13"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":21.5,"d":"€22"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":4.085,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":25.585,"d":"€26"}}]

{"sheet":"09345338SE03","index":353,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345338SE03","LEIPZIGER STRAßE","1,20","1,40","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.2,2,{"$f":"H11*I11","v":{"v":2.4,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.2,3,{"$f":"H12*I12","v":{"v":3.5999999999999996,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":6,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":1.1400000000000001,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":7.140000000000001,"d":"€7"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345338SE03","LEIPZIGER STRAßE","1,20","1,40","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.2,2,{"$f":"H30*I30","v":{"v":2.4,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.2,3,{"$f":"H31*I31","v":{"v":3.5999999999999996,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":6,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":1.1400000000000001,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":7.140000000000001,"d":"€7"}}]

{"sheet":"09345339NN02","index":354,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345339NN02","LEIPZIGER STRAßE","8,80","8,80","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,10","BBE","C","15,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["4,20","BBE","C","25,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","C"]
["8,80","BBE","C","40,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["8,80","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",8.8,2,{"$f":"H14*I14","v":{"v":17.6,"d":"€18"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",8.8,3,{"$f":"H15*I15","v":{"v":26.400000000000002,"d":"€26"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":44,"d":"€44"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":8.36,"d":"€8"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":52.36,"d":"€52"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345339NN02","LEIPZIGER STRAßE","8,80","8,80","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,10","BBE","C","15,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["4,20","BBE","C","25,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","C"]
["8,80","BBE","C","40,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["8,80","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",8.8,2,{"$f":"H36*I36","v":{"v":17.6,"d":"€18"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",8.8,3,{"$f":"H37*I37","v":{"v":26.400000000000002,"d":"€26"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":44,"d":"€44"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":8.36,"d":"€8"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":52.36,"d":"€52"}}]

{"sheet":"09345339SE01","index":355,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345339SE01","LEIPZIGER STRAßE","1,20","1,40","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.2,2,{"$f":"H11*I11","v":{"v":2.4,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.2,3,{"$f":"H12*I12","v":{"v":3.5999999999999996,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":6,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":1.1400000000000001,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":7.140000000000001,"d":"€7"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345339SE01","LEIPZIGER STRAßE","1,20","1,40","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.2,2,{"$f":"H30*I30","v":{"v":2.4,"d":"€2"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.2,3,{"$f":"H31*I31","v":{"v":3.5999999999999996,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":6,"d":"€6"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":1.1400000000000001,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":7.140000000000001,"d":"€7"}}]

{"sheet":"09345339SE03","index":356,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345339SE03","LEIPZIGER STRAßE","1,70","1,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAC","A","200,00","12 - 12",null,"Rohrbruch / Einsturz Bruch "]
["0,80","BAB","B / B","3,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["1,70","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.7,2,{"$f":"H13*I13","v":{"v":3.4,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.7,3,{"$f":"H14*I14","v":{"v":5.1,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":8.5,"d":"€9"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":1.615,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":10.115,"d":"€10"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345339SE03","LEIPZIGER STRAßE","1,70","1,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAC","A","200,00","12 - 12",null,"Rohrbruch / Einsturz Bruch "]
["0,80","BAB","B / B","3,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["1,70","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.7,2,{"$f":"H34*I34","v":{"v":3.4,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.7,3,{"$f":"H35*I35","v":{"v":5.1,"d":"€5"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":8.5,"d":"€9"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":1.615,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":10.115,"d":"€10"}}]

{"sheet":"09345340GA01","index":357,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345340GA01","LEIPZIGER STRAßE","4,10","4,10","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BBE","C","10,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["4,10","BBE","C","10,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["4,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.1,2,{"$f":"H13*I13","v":{"v":8.2,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.1,3,{"$f":"H14*I14","v":{"v":12.299999999999999,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":20.5,"d":"€21"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":3.895,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":24.395,"d":"€24"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345340GA01","LEIPZIGER STRAßE","4,10","4,10","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BBE","C","10,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["4,10","BBE","C","10,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["4,10","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.1,2,{"$f":"H34*I34","v":{"v":8.2,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.1,3,{"$f":"H35*I35","v":{"v":12.299999999999999,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":20.5,"d":"€21"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":3.895,"d":"€4"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":24.395,"d":"€24"}}]

{"sheet":"09345342_1NN01","index":358,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345342_1NN01","LEIPZIGER STRAßE","0,30","0,80","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["0,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["0,30","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["0,30","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.3,2,{"$f":"H14*I14","v":{"v":0.6,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.3,3,{"$f":"H15*I15","v":{"v":0.8999999999999999,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":1.5,"d":"€2"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":0.28500000000000003,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":1.7850000000000001,"d":"€2"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345342_1NN01","LEIPZIGER STRAßE","0,30","0,80","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["0,20","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["0,30","BBE","C","20,00","4 - 8",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["0,30","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.3,2,{"$f":"H36*I36","v":{"v":0.6,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.3,3,{"$f":"H37*I37","v":{"v":0.8999999999999999,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":1.5,"d":"€2"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":0.28500000000000003,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":1.7850000000000001,"d":"€2"}}]

{"sheet":"09345455NN01","index":359,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345455NN01","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"80","PVCU"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345455NN01","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"80","PVCU"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09345455NN02","index":360,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345455NN02","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"80","PVCU"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345455NN02","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"80","PVCU"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09345455NN03","index":361,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345455NN03","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"80","PVCU"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345455NN03","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"80","PVCU"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09345455NN04","index":362,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345455NN04","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"80","PVCU"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345455NN04","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"80","PVCU"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09345455NN05","index":363,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345455NN05","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"80","PVCU"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345455NN05","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"80","PVCU"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09345455NN06","index":364,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345455NN06","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"80","PVCU"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345455NN06","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"80","PVCU"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09345455NN07","index":365,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345455NN07","BERLINER STRAßE","0,40","0,90","Not Implemented yet",{"$nulls":3},"100","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["0,30","AEC","A","80,00",null,null,"Grundlagen änderung  "]
["0,30","AED","PVCU",{"$nulls":3},"Grundlagen änderung  "]
["0,40","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.4,2,{"$f":"H14*I14","v":{"v":0.8,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.4,3,{"$f":"H15*I15","v":{"v":1.2000000000000002,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":2,"d":"€2"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":0.38,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":2.38,"d":"€2"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345455NN07","BERLINER STRAßE","0,40","0,90","Not Implemented yet",{"$nulls":3},"100","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,30","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["0,30","AEC","A","80,00",null,null,"Grundlagen änderung  "]
["0,30","AED","PVCU",{"$nulls":3},"Grundlagen änderung  "]
["0,40","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.4,2,{"$f":"H36*I36","v":{"v":0.8,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.4,3,{"$f":"H37*I37","v":{"v":1.2000000000000002,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":2,"d":"€2"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":0.38,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":2.38,"d":"€2"}}]

{"sheet":"09345487GA02","index":366,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345487GA02","LEIPZIGER STRAßE","9,20","9,20","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,00","BBA","C","10,00","4 - 8",null,"Wurzeln komplexes Wurzelwerk ","A","Fräsen",{"v":50,"d":"€50"}]
["5,00","BBA","C","10,00","4 - 8",null,"Wurzeln komplexes Wurzelwerk ","B","Fräsen",{"v":50,"d":"€50"}]
["9,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":150,"d":"€150"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.2,2,{"$f":"H14*I14","v":{"v":18.4,"d":"€18"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.2,3,{"$f":"H15*I15","v":{"v":27.599999999999998,"d":"€28"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":236.5,"d":"€237"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":44.935,"d":"€45"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":281.435,"d":"€281"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345487GA02","LEIPZIGER STRAßE","9,20","9,20","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BBA","B","3,00","12 - 12","JA","Wurzeln einzelne feine Wurzeln ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,00","BBA","C","10,00","4 - 8",null,"Wurzeln komplexes Wurzelwerk ","A","Fräsen",{"v":50,"d":"€50"}]
["5,00","BBA","C","10,00","4 - 8",null,"Wurzeln komplexes Wurzelwerk ","B","Fräsen",{"v":50,"d":"€50"}]
["9,20","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":150,"d":"€150"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",9.2,2,{"$f":"H36*I36","v":{"v":18.4,"d":"€18"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",9.2,3,{"$f":"H37*I37","v":{"v":27.599999999999998,"d":"€28"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":236.5,"d":"€237"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":44.935,"d":"€45"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":281.435,"d":"€281"}}]

{"sheet":"09345487RS02","index":367,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345487RS02","LEIPZIGER STRAßE","14,00","15,00","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["14,00","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",14,2,{"$f":"H11*I11","v":{"v":28,"d":"€28"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",14,3,{"$f":"H12*I12","v":{"v":42,"d":"€42"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":70,"d":"€70"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":13.3,"d":"€13"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":83.3,"d":"€83"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345487RS02","LEIPZIGER STRAßE","14,00","15,00","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["14,00","BCE","XP",{"$nulls":3},"Endknoten  ",null,"Schlauchliner",{"v":1950,"d":"€1,950"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":1950,"d":"€1,950"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":195,"d":"€195"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":97.5,"d":"€98"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":234,"d":"€234"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",14,2,{"$f":"H30*I30","v":{"v":28,"d":"€28"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",14,3,{"$f":"H31*I31","v":{"v":42,"d":"€42"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":2546.5,"d":"€2,547"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":483.835,"d":"€484"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":3030.335,"d":"€3,030"}}]

{"sheet":"09345488NN01","index":368,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345488NN01","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345488NN01","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09345488NN03","index":369,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345488NN03","LEIPZIGER STRAßE","4,90","4,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,70","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["3,50","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["4,90","BBE","C","80,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["4,90","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.9,2,{"$f":"H14*I14","v":{"v":9.8,"d":"€10"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.9,3,{"$f":"H15*I15","v":{"v":14.700000000000001,"d":"€15"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":24.5,"d":"€25"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":4.655,"d":"€5"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":29.155,"d":"€29"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345488NN03","LEIPZIGER STRAßE","4,90","4,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,70","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["3,50","BCC","B / Y","45,00","3",null,"Krümmung der Leitung nach rechts nicht erkennbar"]
["4,90","BBE","C","80,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["4,90","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",4.9,2,{"$f":"H36*I36","v":{"v":9.8,"d":"€10"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",4.9,3,{"$f":"H37*I37","v":{"v":14.700000000000001,"d":"€15"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":24.5,"d":"€25"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":4.655,"d":"€5"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":29.155,"d":"€29"}}]

{"sheet":"09345488SE02","index":370,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345488SE02","LEIPZIGER STRAßE","1,40","1,60","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,60","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["0,60","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["0,60","AED","PP",{"$nulls":3},"Grundlagen änderung  "]
["1,40","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.4,2,{"$f":"H14*I14","v":{"v":2.8,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.4,3,{"$f":"H15*I15","v":{"v":4.199999999999999,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":6.999999999999999,"d":"€7"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":1.3299999999999998,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":8.329999999999998,"d":"€8"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345488SE02","LEIPZIGER STRAßE","1,40","1,60","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,60","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["0,60","AEC","A","125,00",null,null,"Grundlagen änderung  "]
["0,60","AED","PP",{"$nulls":3},"Grundlagen änderung  "]
["1,40","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",1.4,2,{"$f":"H36*I36","v":{"v":2.8,"d":"€3"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",1.4,3,{"$f":"H37*I37","v":{"v":4.199999999999999,"d":"€4"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":6.999999999999999,"d":"€7"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":1.3299999999999998,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":8.329999999999998,"d":"€8"}}]

{"sheet":"09345540","index":371,"n_rows":50,"n_cols":10,"rows_kept":50}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345540","BERLINER STRAßE","14,10","60,07","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,80","BAF","E / E",null,"4 - 8","JA","Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["2,70","BAI","Z","5,00","2 - 10","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,70","BAJ","B","20,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["8,40","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["10,40","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["13,20","BCA","C / A","150,00","1",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["13,20","BAH","A",null,"12 - 3",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch ",null,null,{"v":0,"d":"€0"}]
["14,10","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["14,10","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J14)","v":{"v":150,"d":"€150"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H16/100)*J15","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H17/100)*J15","v":{"v":7.5,"d":"€8"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H18/100)*J15","v":{"v":18,"d":"€18"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",14.1,2,{"$f":"H19*I19","v":{"v":28.2,"d":"€28"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",14.1,3,{"$f":"H20*I20","v":{"v":42.3,"d":"€42"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J15:J20)","v":{"v":261,"d":"€261"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H22/100)*J21","v":{"v":49.59,"d":"€50"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J21:J22)","v":{"v":310.59000000000003,"d":"€311"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345540","BERLINER STRAßE","14,10","60,07","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,80","BAF","E / E",null,"4 - 8","JA","Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["2,70","BAI","Z","5,00","2 - 10","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["3,70","BAJ","B","20,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["8,40","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["10,40","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["13,20","BCA","C / A","150,00","1",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["13,20","BAH","A",null,"12 - 3",null,"Schadhafter Anschluss Lage des Anschlusses um das Rohr ist falsch "]
["14,10","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["14,10","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J32:J41)","v":{"v":540,"d":"€540"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H43/100)*J42","v":{"v":54,"d":"€54"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H44/100)*J42","v":{"v":27,"d":"€27"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H45/100)*J42","v":{"v":64.8,"d":"€65"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",14.1,2,{"$f":"H46*I46","v":{"v":28.2,"d":"€28"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",14.1,3,{"$f":"H47*I47","v":{"v":42.3,"d":"€42"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J42:J47)","v":{"v":756.3,"d":"€756"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H49/100)*J48","v":{"v":143.697,"d":"€144"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J48:J49)","v":{"v":899.997,"d":"€900"}}]

{"sheet":"09345577NN01","index":372,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345577NN01","BERLINER STRAßE","0,70","0,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBE","C","40,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["0,70","BBE","C","40,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["0,70","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.7,2,{"$f":"H13*I13","v":{"v":1.4,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.7,3,{"$f":"H14*I14","v":{"v":2.0999999999999996,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":3.4999999999999996,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":0.6649999999999999,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":4.164999999999999,"d":"€4"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345577NN01","BERLINER STRAßE","0,70","0,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BBE","C","40,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["0,70","BBE","C","40,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["0,70","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.7,2,{"$f":"H34*I34","v":{"v":1.4,"d":"€1"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.7,3,{"$f":"H35*I35","v":{"v":2.0999999999999996,"d":"€2"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":3.4999999999999996,"d":"€4"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":0.6649999999999999,"d":"€1"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":4.164999999999999,"d":"€4"}}]

{"sheet":"09345577NN02","index":373,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345577NN02","BERLINER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAB","B / C","2,00","12 - 12",null,"Rissbildung Riss komplexe Rissbildung"]
["0,60","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["1,10","BAB","B / B","3,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["2,00","BAI","Z","25,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,90","BBE","C","60,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","C"]
["3,10","BBE","C","60,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["3,10","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H17*I17","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H18*I18","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":79,"d":"€79"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":15.01,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":94.01,"d":"€94"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345577NN02","BERLINER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","STZ"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAB","B / C","2,00","12 - 12",null,"Rissbildung Riss komplexe Rissbildung"]
["0,60","BBE","C","30,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","A"]
["1,10","BAB","B / B","3,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["2,00","BAI","Z","25,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["2,90","BBE","C","60,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","C"]
["3,10","BBE","C","60,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle ","B"]
["3,10","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H42*I42","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H43*I43","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":18.445,"d":"€18"}}]

{"sheet":"09345819NN01","index":374,"n_rows":52,"n_cols":10,"rows_kept":52}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345819NN01","LEIPZIGER STRAßE","3,00","3,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["0,10","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,30","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["0,30","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["2,40","BAJ","B","20,00","3","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,90","BAF","I / E",null,"2 - 10",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["3,00","BAF","I / E",null,"2 - 10",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["3,00","BAC","C",null,"12 - 12",null,"Rohrbruch / Einsturz Einsturz "]
["3,00","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  "]
["3,00","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J15)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H17/100)*J16","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H18/100)*J16","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H19/100)*J16","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3,2,{"$f":"H20*I20","v":{"v":6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3,3,{"$f":"H21*I21","v":{"v":9,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J16:J21)","v":{"v":78.5,"d":"€79"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H23/100)*J22","v":{"v":14.915000000000001,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J22:J23)","v":{"v":93.415,"d":"€93"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345819NN01","LEIPZIGER STRAßE","3,00","3,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["0,10","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,30","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["0,30","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["2,40","BAJ","B","20,00","3","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,90","BAF","I / E",null,"2 - 10",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["3,00","BAF","I / E",null,"2 - 10",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["3,00","BAC","C",null,"12 - 12",null,"Rohrbruch / Einsturz Einsturz "]
["3,00","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  "]
["3,00","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J33:J43)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H45/100)*J44","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H46/100)*J44","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H47/100)*J44","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3,2,{"$f":"H48*I48","v":{"v":6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3,3,{"$f":"H49*I49","v":{"v":9,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J44:J49)","v":{"v":78.5,"d":"€79"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H51/100)*J50","v":{"v":14.915000000000001,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J50:J51)","v":{"v":93.415,"d":"€93"}}]

{"sheet":"09345819NN03","index":375,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345819NN03","LEIPZIGER STRAßE","2,80","2,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["0,20","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,60","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["0,70","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,80","BBE","C","50,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["2,80","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.8,2,{"$f":"H17*I17","v":{"v":5.6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.8,3,{"$f":"H18*I18","v":{"v":8.399999999999999,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":13.999999999999998,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":2.6599999999999997,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":16.659999999999997,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345819NN03","LEIPZIGER STRAßE","2,80","2,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["0,20","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,60","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["0,70","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,80","BBE","C","50,00","3 - 9",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["2,80","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.8,2,{"$f":"H42*I42","v":{"v":5.6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.8,3,{"$f":"H43*I43","v":{"v":8.399999999999999,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":13.999999999999998,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":2.6599999999999997,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":16.659999999999997,"d":"€17"}}]

{"sheet":"09345819RR02","index":376,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345819RR02","LEIPZIGER STRAßE","3,50","3,50","Not Implemented yet",{"$nulls":3},"150","PVC"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","A / B","45,00","7",null,"Krümmung der Leitung nach links nach unten"]
["0,40","BCC","A / Y","30,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,60","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,80","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["3,20","BAP",null,null,"3 - 9",null,"Hohlraum sichtbar  "]
["3,20","BAC","C",null,"12 - 12",null,"Rohrbruch / Einsturz Einsturz "]
["3,50","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H17*I17","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H18*I18","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":17.5,"d":"€18"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":3.325,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":20.825,"d":"€21"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345819RR02","LEIPZIGER STRAßE","3,50","3,50","Not Implemented yet",{"$nulls":3},"150","PVC"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BCC","A / B","45,00","7",null,"Krümmung der Leitung nach links nach unten"]
["0,40","BCC","A / Y","30,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,60","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,80","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["3,20","BAP",null,null,"3 - 9",null,"Hohlraum sichtbar  "]
["3,20","BAC","C",null,"12 - 12",null,"Rohrbruch / Einsturz Einsturz "]
["3,50","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.5,2,{"$f":"H42*I42","v":{"v":7,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.5,3,{"$f":"H43*I43","v":{"v":10.5,"d":"€11"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":17.5,"d":"€18"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":3.325,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":20.825,"d":"€21"}}]

{"sheet":"09345819RR04","index":377,"n_rows":48,"n_cols":10,"rows_kept":48}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345819RR04","LEIPZIGER STRAßE","3,20","3,40","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["0,20","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,20","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["1,40","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,50","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["2,40","BAJ","A","40,00","12 - 12","JA","Verschobene Verbindung in längsrichtung ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,20","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J13)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H15/100)*J14","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H16/100)*J14","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H17/100)*J14","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H18*I18","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H19*I19","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J14:J19)","v":{"v":79.5,"d":"€80"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H21/100)*J20","v":{"v":15.105,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J20:J21)","v":{"v":94.605,"d":"€95"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345819RR04","LEIPZIGER STRAßE","3,20","3,40","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["0,20","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,20","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["1,40","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,50","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["2,40","BAJ","A","40,00","12 - 12","JA","Verschobene Verbindung in längsrichtung ",null,"Fräsen",{"v":50,"d":"€50"}]
["3,20","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J31:J39)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.2,2,{"$f":"H44*I44","v":{"v":6.4,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.2,3,{"$f":"H45*I45","v":{"v":9.600000000000001,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":79.5,"d":"€80"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":15.105,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":94.605,"d":"€95"}}]

{"sheet":"09345819RR05","index":378,"n_rows":50,"n_cols":10,"rows_kept":50}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345819RR05","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","E / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["0,20","BAC","C",null,"3 - 9",null,"Rohrbruch / Einsturz Einsturz ","A"]
["0,20","BAP",null,null,"3 - 9",null,"Hohlraum sichtbar  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,30","BAF","E / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["0,30","BAC","C",null,"3 - 9",null,"Rohrbruch / Einsturz Einsturz ","B"]
["0,30","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,30","BBE","B","25,00","4 - 8",null,"Andere Hindernisse Bruchstücke einer Abwasserleitung oder eines Abwasserkanals liegen in der \r\nRohrsohle "]
["2,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J14)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H16/100)*J15","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H17/100)*J15","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H18/100)*J15","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H19*I19","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H20*I20","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J15:J20)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H22/100)*J21","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J21:J22)","v":{"v":16.065,"d":"€16"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345819RR05","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","E / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["0,20","BAC","C",null,"3 - 9",null,"Rohrbruch / Einsturz Einsturz ","A"]
["0,20","BAP",null,null,"3 - 9",null,"Hohlraum sichtbar  "]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,30","BAF","E / E",null,"3 - 9",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["0,30","BAC","C",null,"3 - 9",null,"Rohrbruch / Einsturz Einsturz ","B"]
["0,30","BCC","Y / B","45,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["1,30","BBE","B","25,00","4 - 8",null,"Andere Hindernisse Bruchstücke einer Abwasserleitung oder eines Abwasserkanals liegen in der \r\nRohrsohle "]
["2,70","BDC","Y / A",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar Inspektionsziel vor Erreichen des Endknotens erreicht"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J32:J41)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H43/100)*J42","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H44/100)*J42","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H45/100)*J42","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H46*I46","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H47*I47","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J42:J47)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H49/100)*J48","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J48:J49)","v":{"v":16.065,"d":"€16"}}]

{"sheet":"09345819RR06","index":379,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345819RR06","LEIPZIGER STRAßE","2,50","3,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,90","BAI","Z","10,00","4 - 8","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["1,90","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,90","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,90","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,40","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,50","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H16*I16","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H17*I17","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":76,"d":"€76"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":14.44,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":90.44,"d":"€90"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345819RR06","LEIPZIGER STRAßE","2,50","3,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,90","BAI","Z","10,00","4 - 8","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["1,90","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,90","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,90","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,40","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,50","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.5,2,{"$f":"H40*I40","v":{"v":5,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.5,3,{"$f":"H41*I41","v":{"v":7.5,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":12.5,"d":"€13"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":2.375,"d":"€2"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":14.875,"d":"€15"}}]

{"sheet":"09345820NN04","index":380,"n_rows":52,"n_cols":10,"rows_kept":52}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345820NN04","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["0,10","BAO",null,null,"4 - 8",null,"Boden sichtbar  ","A"]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,70","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["0,70","BAO",null,null,"4 - 8",null,"Boden sichtbar  ","B"]
["2,80","BAJ","B","70,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,80","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  "]
["2,90","BAC","C",null,"12 - 12",null,"Rohrbruch / Einsturz Einsturz "]
["2,90","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J15)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H17/100)*J16","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H18/100)*J16","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H19/100)*J16","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H20*I20","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H21*I21","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J16:J21)","v":{"v":78,"d":"€78"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H23/100)*J22","v":{"v":14.82,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J22:J23)","v":{"v":92.82,"d":"€93"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345820NN04","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["0,10","BAO",null,null,"4 - 8",null,"Boden sichtbar  ","A"]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,70","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["0,70","BAO",null,null,"4 - 8",null,"Boden sichtbar  ","B"]
["2,80","BAJ","B","70,00","6","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["2,80","BAP",null,null,"12 - 12",null,"Hohlraum sichtbar  "]
["2,90","BAC","C",null,"12 - 12",null,"Rohrbruch / Einsturz Einsturz "]
["2,90","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J33:J43)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H45/100)*J44","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H46/100)*J44","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H47/100)*J44","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H48*I48","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H49*I49","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J44:J49)","v":{"v":78,"d":"€78"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H51/100)*J50","v":{"v":14.82,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J50:J51)","v":{"v":92.82,"d":"€93"}}]

{"sheet":"09345820NN05","index":381,"n_rows":44,"n_cols":10,"rows_kept":44}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345820NN05","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAF","I / E",null,"2 - 10",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["0,10","BAP",null,null,"2 - 10",null,"Hohlraum sichtbar  ","A"]
["0,20","BAF","I / E",null,"2 - 10",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["0,20","BAP",null,null,"2 - 10",null,"Hohlraum sichtbar  ","B"]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J11)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H13/100)*J12","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H14/100)*J12","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H15/100)*J12","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H16*I16","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H17*I17","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J12:J17)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H19/100)*J18","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J18:J19)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345820NN05","LEIPZIGER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAF","I / E",null,"2 - 10",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["0,10","BAP",null,null,"2 - 10",null,"Hohlraum sichtbar  ","A"]
["0,20","BAF","I / E",null,"2 - 10",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["0,20","BAP",null,null,"2 - 10",null,"Hohlraum sichtbar  ","B"]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J29:J35)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H37/100)*J36","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H38/100)*J36","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H39/100)*J36","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H40*I40","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H41*I41","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J36:J41)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H43/100)*J42","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J42:J43)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09345820RR01","index":382,"n_rows":54,"n_cols":10,"rows_kept":54}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345820RR01","LEIPZIGER STRAßE","3,90","3,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAJ","C","30,00","6","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,10","BAJ","B","30,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,80","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["0,80","BAO",null,null,"3 - 9",null,"Boden sichtbar  ","A"]
["1,00","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,20","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["1,20","BAO",null,null,"3 - 9",null,"Boden sichtbar  ","B"]
["3,50","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["3,70","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,80","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J16)","v":{"v":100,"d":"€100"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H18/100)*J17","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H19/100)*J17","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H20/100)*J17","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.9,2,{"$f":"H21*I21","v":{"v":7.8,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.9,3,{"$f":"H22*I22","v":{"v":11.7,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J17:J22)","v":{"v":146.5,"d":"€147"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H24/100)*J23","v":{"v":27.835,"d":"€28"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J23:J24)","v":{"v":174.335,"d":"€174"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345820RR01","LEIPZIGER STRAßE","3,90","3,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAJ","C","30,00","6","JA","Verschobene Verbindung im Winkel ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,10","BAJ","B","30,00","12","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,80","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","A"]
["0,80","BAO",null,null,"3 - 9",null,"Boden sichtbar  ","A"]
["1,00","BCC","A / Y","90,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,20","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar","B"]
["1,20","BAO",null,null,"3 - 9",null,"Boden sichtbar  ","B"]
["3,50","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["3,70","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,80","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J34:J45)","v":{"v":100,"d":"€100"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H47/100)*J46","v":{"v":10,"d":"€10"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H48/100)*J46","v":{"v":5,"d":"€5"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H49/100)*J46","v":{"v":12,"d":"€12"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.9,2,{"$f":"H50*I50","v":{"v":7.8,"d":"€8"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.9,3,{"$f":"H51*I51","v":{"v":11.7,"d":"€12"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J46:J51)","v":{"v":146.5,"d":"€147"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H53/100)*J52","v":{"v":27.835,"d":"€28"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J52:J53)","v":{"v":174.335,"d":"€174"}}]

{"sheet":"09345820RR02","index":383,"n_rows":46,"n_cols":10,"rows_kept":46}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345820RR02","LEIPZIGER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["0,10","BAO",null,null,"4 - 8",null,"Boden sichtbar  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,80","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,90","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J12)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H14/100)*J13","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H15/100)*J13","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H16/100)*J13","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H17*I17","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H18*I18","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J13:J18)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H20/100)*J19","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J19:J20)","v":{"v":18.445,"d":"€18"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345820RR02","LEIPZIGER STRAßE","3,10","3,10","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,10","BAF","I / E",null,"4 - 8",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["0,10","BAO",null,null,"4 - 8",null,"Boden sichtbar  "]
["0,30","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["2,80","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["2,90","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,10","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J30:J37)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H39/100)*J38","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H40/100)*J38","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H41/100)*J38","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.1,2,{"$f":"H42*I42","v":{"v":6.2,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.1,3,{"$f":"H43*I43","v":{"v":9.3,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J38:J43)","v":{"v":15.5,"d":"€16"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H45/100)*J44","v":{"v":2.945,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J44:J45)","v":{"v":18.445,"d":"€18"}}]

{"sheet":"09345820RR03","index":384,"n_rows":50,"n_cols":10,"rows_kept":50}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345820RR03","LEIPZIGER STRAßE","3,30","3,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAJ","B","40,00","3","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,80","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["1,00","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,90","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,90","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["3,10","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,30","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J14)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H16/100)*J15","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H17/100)*J15","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H18/100)*J15","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.3,2,{"$f":"H19*I19","v":{"v":6.6,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.3,3,{"$f":"H20*I20","v":{"v":9.899999999999999,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J15:J20)","v":{"v":80,"d":"€80"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H22/100)*J21","v":{"v":15.2,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J21:J22)","v":{"v":95.2,"d":"€95"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345820RR03","LEIPZIGER STRAßE","3,30","3,30","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAJ","B","40,00","3","JA","Verschobene Verbindung radial ",null,"Fräsen",{"v":50,"d":"€50"}]
["0,20","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["0,80","BAF","I / E",null,"3 - 9",null,"Oberflächenschaden fehlende Wand Ursache nicht eindeutig festellbar"]
["1,00","BCC","A / Y","45,00","9",null,"Krümmung der Leitung nach links nicht erkennbar"]
["1,90","AEC","A","100,00",null,null,"Grundlagen änderung  "]
["1,90","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["3,10","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,20","BCC","Y / A","45,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,30","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J32:J41)","v":{"v":50,"d":"€50"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H43/100)*J42","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H44/100)*J42","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H45/100)*J42","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3.3,2,{"$f":"H46*I46","v":{"v":6.6,"d":"€7"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3.3,3,{"$f":"H47*I47","v":{"v":9.899999999999999,"d":"€10"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J42:J47)","v":{"v":80,"d":"€80"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H49/100)*J48","v":{"v":15.2,"d":"€15"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J48:J49)","v":{"v":95.2,"d":"€95"}}]

{"sheet":"09345821RR01","index":385,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345821RR01","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,70","BAC","A","200,00","12 - 12",null,"Rohrbruch / Einsturz Bruch "]
["2,80","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H13*I13","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H14*I14","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":17.255,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345821RR01","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,70","BAC","A","200,00","12 - 12",null,"Rohrbruch / Einsturz Bruch "]
["2,80","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H34*I34","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H35*I35","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":17.255,"d":"€17"}}]

{"sheet":"09345821RR02","index":386,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345821RR02","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,50","BAB","B / B","5,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["2,70","BAC","A","300,00","12 - 12",null,"Rohrbruch / Einsturz Bruch "]
["2,80","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,90","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H14*I14","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H15*I15","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":17.255,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345821RR02","LEIPZIGER STRAßE","2,90","2,90","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,50","BAB","B / B","5,00","12 - 12",null,"Rissbildung Riss am Rohrumfang"]
["2,70","BAC","A","300,00","12 - 12",null,"Rohrbruch / Einsturz Bruch "]
["2,80","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,90","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.9,2,{"$f":"H36*I36","v":{"v":5.8,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.9,3,{"$f":"H37*I37","v":{"v":8.7,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":14.5,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":2.755,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":17.255,"d":"€17"}}]

{"sheet":"09345821RR03","index":387,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345821RR03","LEIPZIGER STRAßE","3,00","3,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,80","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,00","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3,2,{"$f":"H12*I12","v":{"v":6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3,3,{"$f":"H13*I13","v":{"v":9,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.85,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":17.85,"d":"€18"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345821RR03","LEIPZIGER STRAßE","3,00","3,00","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,80","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["3,00","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",3,2,{"$f":"H32*I32","v":{"v":6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",3,3,{"$f":"H33*I33","v":{"v":9,"d":"€9"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":15,"d":"€15"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.85,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":17.85,"d":"€18"}}]

{"sheet":"09345821RR04","index":388,"n_rows":38,"n_cols":10,"rows_kept":38}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345821RR04","LEIPZIGER STRAßE","2,80","2,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,60","BAB","B / A","8,00","6",null,"Rissbildung Riss in Längsrichtung"]
["2,70","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,80","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J8)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H10/100)*J9","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H11/100)*J9","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H12/100)*J9","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.8,2,{"$f":"H13*I13","v":{"v":5.6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.8,3,{"$f":"H14*I14","v":{"v":8.399999999999999,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J9:J14)","v":{"v":13.999999999999998,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H16/100)*J15","v":{"v":2.6599999999999997,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J15:J16)","v":{"v":16.659999999999997,"d":"€17"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345821RR04","LEIPZIGER STRAßE","2,80","2,80","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,60","BAB","B / A","8,00","6",null,"Rissbildung Riss in Längsrichtung"]
["2,70","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,80","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J26:J29)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H31/100)*J30","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H32/100)*J30","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H33/100)*J30","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.8,2,{"$f":"H34*I34","v":{"v":5.6,"d":"€6"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.8,3,{"$f":"H35*I35","v":{"v":8.399999999999999,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J30:J35)","v":{"v":13.999999999999998,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H37/100)*J36","v":{"v":2.6599999999999997,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J36:J37)","v":{"v":16.659999999999997,"d":"€17"}}]

{"sheet":"09345821RR05","index":389,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345821RR05","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,60","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,70","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H12*I12","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H13*I13","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":16.065,"d":"€16"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345821RR05","LEIPZIGER STRAßE","2,70","2,70","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,60","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,70","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H32*I32","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H33*I33","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":16.065,"d":"€16"}}]

{"sheet":"09345821RR06","index":390,"n_rows":36,"n_cols":10,"rows_kept":36}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345821RR06","LEIPZIGER STRAßE","2,70","3,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,60","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,70","BCE","XP",{"$nulls":3},"Endknoten  "]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J7)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H9/100)*J8","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H10/100)*J8","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H11/100)*J8","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H12*I12","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H13*I13","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J8:J13)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H15/100)*J14","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J14:J15)","v":{"v":16.065,"d":"€16"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09345821RR06","LEIPZIGER STRAßE","2,70","3,20","Not Implemented yet",{"$nulls":3},"150","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,60","BCC","Y / A","90,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["2,70","BCE","XP",{"$nulls":3},"Endknoten  ",null,null,{"v":0,"d":"€0"}]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J25:J27)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H29/100)*J28","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H30/100)*J28","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H31/100)*J28","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",2.7,2,{"$f":"H32*I32","v":{"v":5.4,"d":"€5"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",2.7,3,{"$f":"H33*I33","v":{"v":8.100000000000001,"d":"€8"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J28:J33)","v":{"v":13.500000000000002,"d":"€14"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H35/100)*J34","v":{"v":2.5650000000000004,"d":"€3"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J34:J35)","v":{"v":16.065,"d":"€16"}}]

{"sheet":"09346098","index":391,"n_rows":48,"n_cols":10,"rows_kept":48}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09346098","BERLINER STRAßE","14,50","14,50","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,00","BAF","E / E",null,"3 - 6",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["5,60","BAI","Z","5,00","11 - 1","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["6,60","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["7,40","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["9,70","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["13,00","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["14,50","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["14,50","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J13)","v":{"v":50,"d":"€50"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H15/100)*J14","v":{"v":5,"d":"€5"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H16/100)*J14","v":{"v":2.5,"d":"€3"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H17/100)*J14","v":{"v":6,"d":"€6"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",14.5,2,{"$f":"H18*I18","v":{"v":29,"d":"€29"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",14.5,3,{"$f":"H19*I19","v":{"v":43.5,"d":"€44"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J14:J19)","v":{"v":136,"d":"€136"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H21/100)*J20","v":{"v":25.84,"d":"€26"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J20:J21)","v":{"v":161.84,"d":"€162"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09346098","BERLINER STRAßE","14,50","14,50","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["2,00","BAF","E / E",null,"3 - 6",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar"]
["5,60","BAI","Z","5,00","11 - 1","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["6,60","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["7,40","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["9,70","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["13,00","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["14,50","BAF","E / E",null,"4 - 8",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["14,50","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J31:J39)","v":{"v":490,"d":"€490"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H41/100)*J40","v":{"v":49,"d":"€49"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H42/100)*J40","v":{"v":24.5,"d":"€25"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H43/100)*J40","v":{"v":58.8,"d":"€59"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",14.5,2,{"$f":"H44*I44","v":{"v":29,"d":"€29"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",14.5,3,{"$f":"H45*I45","v":{"v":43.5,"d":"€44"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J40:J45)","v":{"v":694.8,"d":"€695"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H47/100)*J46","v":{"v":132.012,"d":"€132"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J46:J47)","v":{"v":826.8119999999999,"d":"€827"}}]

{"sheet":"09346099","index":392,"n_rows":34,"n_cols":10,"rows_kept":34}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09346099","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J6)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H8/100)*J7","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H9/100)*J7","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H10/100)*J7","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H11*I11","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H12*I12","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J7:J12)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H14/100)*J13","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J13:J14)","v":{"v":1.19,"d":"€1"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09346099","BERLINER STRAßE","0,20","0,20","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,20","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J24:J25)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H27/100)*J26","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H28/100)*J26","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H29/100)*J26","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",0.2,2,{"$f":"H30*I30","v":{"v":0.4,"d":"€0"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",0.2,3,{"$f":"H31*I31","v":{"v":0.6000000000000001,"d":"€1"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J26:J31)","v":{"v":1,"d":"€1"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H33/100)*J32","v":{"v":0.19,"d":"€0"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J32:J33)","v":{"v":1.19,"d":"€1"}}]

{"sheet":"09346100","index":393,"n_rows":40,"n_cols":10,"rows_kept":40}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09346100","BERLINER STRAßE","14,70","14,70","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["13,60","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["14,70","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["14,70","BDC","Y / Z",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar andere"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J9)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H11/100)*J10","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H12/100)*J10","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H13/100)*J10","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",14.7,2,{"$f":"H14*I14","v":{"v":29.4,"d":"€29"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",14.7,3,{"$f":"H15*I15","v":{"v":44.099999999999994,"d":"€44"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J10:J15)","v":{"v":73.5,"d":"€74"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H17/100)*J16","v":{"v":13.965,"d":"€14"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J16:J17)","v":{"v":87.465,"d":"€87"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09346100","BERLINER STRAßE","14,70","14,70","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["13,60","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["14,70","BCA","C / A","150,00","2",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["14,70","BDC","Y / Z",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar andere"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J27:J31)","v":{"v":490,"d":"€490"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H33/100)*J32","v":{"v":49,"d":"€49"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H34/100)*J32","v":{"v":24.5,"d":"€25"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H35/100)*J32","v":{"v":58.8,"d":"€59"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",14.7,2,{"$f":"H36*I36","v":{"v":29.4,"d":"€29"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",14.7,3,{"$f":"H37*I37","v":{"v":44.099999999999994,"d":"€44"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J32:J37)","v":{"v":695.8,"d":"€696"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H39/100)*J38","v":{"v":132.202,"d":"€132"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J38:J39)","v":{"v":828.002,"d":"€828"}}]

{"sheet":"09346101","index":394,"n_rows":56,"n_cols":10,"rows_kept":56}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09346101","BERLINER STRAßE","17,20","17,20","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["3,80","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart ",null,"Fräsen",{"v":50,"d":"€50"}]
["4,70","BBF","A",null,"4 - 8","JA","Infiltration Schwitzen "]
["4,70","BBB","A","1,00","4 - 8","JA","Anhaftende Stoffe Inkrustation ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,70","BBF","A",null,"2 - 10","JA","Infiltration Schwitzen "]
["5,70","BBB","A","2,00","2 - 10","JA","Anhaftende Stoffe Inkrustation ",null,"Fräsen",{"v":50,"d":"€50"}]
["7,50","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["7,80","BBF","A",null,"2 - 10","JA","Infiltration Schwitzen "]
["7,80","BBB","A","2,00","2 - 10","JA","Anhaftende Stoffe Inkrustation ",null,"Fräsen",{"v":50,"d":"€50"}]
["10,50","BBE","B","15,00","4 - 8",null,"Andere Hindernisse Bruchstücke einer Abwasserleitung oder eines Abwasserkanals liegen in der \r\nRohrsohle "]
["10,50","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen"]
["17,20","BDC","Y / Z",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar andere"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J17)","v":{"v":200,"d":"€200"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H19/100)*J18","v":{"v":20,"d":"€20"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H20/100)*J18","v":{"v":10,"d":"€10"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H21/100)*J18","v":{"v":24,"d":"€24"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",17.2,2,{"$f":"H22*I22","v":{"v":34.4,"d":"€34"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",17.2,3,{"$f":"H23*I23","v":{"v":51.599999999999994,"d":"€52"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J18:J23)","v":{"v":340,"d":"€340"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H25/100)*J24","v":{"v":64.6,"d":"€65"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J24:J25)","v":{"v":404.6,"d":"€405"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09346101","BERLINER STRAßE","17,20","17,20","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["0,00","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","A"]
["3,80","BAI","Z","5,00","12 - 12","JA","Einragendes Dichtungsmaterial andere Dichtungsart "]
["4,70","BBF","A",null,"4 - 8","JA","Infiltration Schwitzen "]
["4,70","BBB","A","1,00","4 - 8","JA","Anhaftende Stoffe Inkrustation ",null,"Fräsen",{"v":50,"d":"€50"}]
["5,70","BBF","A",null,"2 - 10","JA","Infiltration Schwitzen "]
["5,70","BBB","A","2,00","2 - 10","JA","Anhaftende Stoffe Inkrustation ",null,"Fräsen",{"v":50,"d":"€50"}]
["7,50","BAF","E / E",null,"12 - 12",null,"Oberflächenschaden Zuschlagstoffe fehlen Ursache nicht eindeutig festellbar","B"]
["7,80","BBF","A",null,"2 - 10","JA","Infiltration Schwitzen "]
["7,80","BBB","A","2,00","2 - 10","JA","Anhaftende Stoffe Inkrustation ",null,"Fräsen",{"v":50,"d":"€50"}]
["10,50","BBE","B","15,00","4 - 8",null,"Andere Hindernisse Bruchstücke einer Abwasserleitung oder eines Abwasserkanals liegen in der \r\nRohrsohle "]
["10,50","BCA","C / A","150,00","9",null,"Anschluss Sattelanschluss – gemeißelt offen",null,"Einmessen,Öffnen,Hut",{"v":490,"d":"€490"}]
["17,20","BDC","Y / Z",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar andere"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J35:J47)","v":{"v":640,"d":"€640"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H49/100)*J48","v":{"v":64,"d":"€64"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H50/100)*J48","v":{"v":32,"d":"€32"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H51/100)*J48","v":{"v":76.8,"d":"€77"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",17.2,2,{"$f":"H52*I52","v":{"v":34.4,"d":"€34"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",17.2,3,{"$f":"H53*I53","v":{"v":51.599999999999994,"d":"€52"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J48:J53)","v":{"v":898.8,"d":"€899"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H55/100)*J54","v":{"v":170.772,"d":"€171"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J54:J55)","v":{"v":1069.572,"d":"€1,070"}}]

{"sheet":"09346102","index":395,"n_rows":54,"n_cols":10,"rows_kept":54}
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09346102","LEIPZIGER STRAßE","5,70","5,70","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["1,00","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["1,00","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,20","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,40","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["2,00","BDD","A","30,00",null,null,"Wasserspiegel klar (Sohle sichtbar) ","A"]
["2,40","AEC","A","200,00",null,null,"Grundlagen änderung  "]
["2,40","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["5,70","BDD","A",{"$nulls":3},"Wasserspiegel klar (Sohle sichtbar) ","B"]
["5,70","BBE","C","50,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["5,70","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J5:J16)","v":{"v":0,"d":"€0"}}]
["Reparatur",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H18/100)*J17","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H19/100)*J17","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H20/100)*J17","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.7,2,{"$f":"H21*I21","v":{"v":11.4,"d":"€11"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.7,3,{"$f":"H22*I22","v":{"v":17.1,"d":"€17"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J17:J22)","v":{"v":28.5,"d":"€29"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H24/100)*J23","v":{"v":5.415,"d":"€5"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J23:J24)","v":{"v":33.915,"d":"€34"}}]
[]
[]
[]
[]
["Haltung","Straße","Inspizierte Länge","Länge","Tiefe",null,"Schadensbeschreibung",null,"Durchmesser","Material"]
["09346102","LEIPZIGER STRAßE","5,70","5,70","Not Implemented yet",{"$nulls":3},"200","B"]
[]
["Station","Kürzel","Charakterisi.","Quantifizierung","Lage im Kreis",null,"Schadensbeschreibung / Info","Strecke","Sanierungsvorschlag","Kostenans."]
["0,00","BCD","XP",{"$nulls":3},"Anfangsknoten  "]
["1,00","AEC","A","150,00",null,null,"Grundlagen änderung  "]
["1,00","AED","PVC",{"$nulls":3},"Grundlagen änderung  "]
["1,00","BDB",{"$nulls":4},"Allgemeine Anmerkung  "]
["1,20","BCC","Y / A","30,00","12",null,"Krümmung der Leitung nicht erkennbar nach oben"]
["1,40","BCC","Y / B","30,00","6",null,"Krümmung der Leitung nicht erkennbar nach unten"]
["2,00","BDD","A","30,00",null,null,"Wasserspiegel klar (Sohle sichtbar) ","A"]
["2,40","AEC","A","200,00",null,null,"Grundlagen änderung  "]
["2,40","AED","B",{"$nulls":3},"Grundlagen änderung  "]
["5,70","BDD","A",{"$nulls":3},"Wasserspiegel klar (Sohle sichtbar) ","B"]
["5,70","BBE","C","50,00","2 - 10",null,"Andere Hindernisse anderer Gegenstand liegt in der Rohrsohle "]
["5,70","BDC","Y / Y",{"$nulls":3},"Inspektion endet vor dem Endknoten nicht erkennbar nicht erkennbar"]
[{"$nulls":6},"netto-Zwischensumme",null,null,{"$f":"SUM(J34:J45)","v":{"v":0,"d":"€0"}}]
["Renovation",{"$nulls":5},"Baustelleneinrichtung anteilig Haltung",10,null,{"$f":"(H47/100)*J46","v":{"v":0,"d":"€0"}}]
[{"$nulls":6},"Verkehrssicherung anteilig Haltung",5,null,{"$f":"(H48/100)*J46","v":{"v":0,"d":"€0"}}]
["Sanierungspriorität",null,"Info",{"$nulls":3},"Aufrechterhaltung der Vorflut Haltung",12,null,{"$f":"(H49/100)*J46","v":{"v":0,"d":"€0"}}]
["kurzfristing","ja oder nein","6-12 Monate",{"$nulls":3},"Kanalreinigung vor Sanierung",5.7,2,{"$f":"H50*I50","v":{"v":11.4,"d":"€11"}}]
["mittelfristig","ja oder nein","1 bis 5 Jahre",{"$nulls":3},"Kamerainspektion Abnahme",5.7,3,{"$f":"H51*I51","v":{"v":17.1,"d":"€17"}}]
["langfristig","ja oder nein","5 bis 10 Jahre",{"$nulls":3},"Summe netto Haltung",null,null,{"$f":"SUM(J46:J51)","v":{"v":28.5,"d":"€29"}}]
[{"$nulls":6},"Mehrwertsteuer",19,null,{"$f":"(H53/100)*J52","v":{"v":5.415,"d":"€5"}}]
["Sanierung im Verbund","ja oder nein",{"$nulls":4},"Summe brutto Haltung",null,null,{"$f":"SUM(J52:J53)","v":{"v":33.915,"d":"€34"}}]